(module MAPBGA-121_8x8mm_0.65mm_Copper_alignment_marks (layer F.Cu) (tedit 548E9CCC)
  (solder_mask_margin 0.05)
  (solder_paste_margin 0.02)
  (attr smd)
  (fp_text reference U1 (at 0 -4.75) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text value Freescale_MK22FN256VDC12 (at 0 5) (layer Cmts.User)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text user A1 (at -5 -3.75) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_line (start -4.25 -4.25) (end 4.25 -4.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.25 -4.25) (end 4.25 4.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.25 4.25) (end -4.25 4.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.25 4.25) (end -4.25 -4.25) (layer F.CrtYd) (width 0.05))
  (pad A1 smd rect (at -3.25 -3.25) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad A2 smd rect (at -2.6 -3.25) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad A3 smd rect (at -1.95 -3.25) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad A4 smd rect (at -1.3 -3.25) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad A5 smd rect (at -0.65 -3.25) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad A6 smd rect (at 0 -3.25) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad A7 smd rect (at 0.65 -3.25) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad A8 smd rect (at 1.3 -3.25) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad A9 smd rect (at 1.95 -3.25) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad A10 smd rect (at 2.6 -3.25) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad A11 smd rect (at 3.25 -3.25) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad B1 smd rect (at -3.25 -2.6) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad B2 smd rect (at -2.6 -2.6) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad B3 smd rect (at -1.95 -2.6) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad B4 smd rect (at -1.3 -2.6) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad B5 smd rect (at -0.65 -2.6) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad B6 smd rect (at 0 -2.6) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad B7 smd rect (at 0.65 -2.6) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad B8 smd rect (at 1.3 -2.6) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad B9 smd rect (at 1.95 -2.6) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad B10 smd rect (at 2.6 -2.6) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad B11 smd rect (at 3.25 -2.6) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad C1 smd rect (at -3.25 -1.95) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad C2 smd rect (at -2.6 -1.95) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad C3 smd rect (at -1.95 -1.95) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad C4 smd rect (at -1.3 -1.95) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad C5 smd rect (at -0.65 -1.95) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad C6 smd rect (at 0 -1.95) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad C7 smd rect (at 0.65 -1.95) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad C8 smd rect (at 1.3 -1.95) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad C9 smd rect (at 1.95 -1.95) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad C10 smd rect (at 2.6 -1.95) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad C11 smd rect (at 3.25 -1.95) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad D1 smd rect (at -3.25 -1.3) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad D2 smd rect (at -2.6 -1.3) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad D3 smd rect (at -1.95 -1.3) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad D4 smd rect (at -1.3 -1.3) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad D5 smd rect (at -0.65 -1.3) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad D6 smd rect (at 0 -1.3) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad D7 smd rect (at 0.65 -1.3) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad D8 smd rect (at 1.3 -1.3) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad D9 smd rect (at 1.95 -1.3) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad D10 smd rect (at 2.6 -1.3) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad D11 smd rect (at 3.25 -1.3) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad E1 smd rect (at -3.25 -0.65) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad E2 smd rect (at -2.6 -0.65) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad E3 smd rect (at -1.95 -0.65) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad E4 smd rect (at -1.3 -0.65) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad E5 smd rect (at -0.65 -0.65) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad E6 smd rect (at 0 -0.65) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad E7 smd rect (at 0.65 -0.65) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad E8 smd rect (at 1.3 -0.65) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad E9 smd rect (at 1.95 -0.65) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad E10 smd rect (at 2.6 -0.65) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad E11 smd rect (at 3.25 -0.65) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad F1 smd rect (at -3.25 0) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad F2 smd rect (at -2.6 0) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad F3 smd rect (at -1.95 0) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad F4 smd rect (at -1.3 0) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad F5 smd rect (at -0.65 0) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad F6 smd rect (at 0 0) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad F7 smd rect (at 0.65 0) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad F8 smd rect (at 1.3 0) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad F9 smd rect (at 1.95 0) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad F10 smd rect (at 2.6 0) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad F11 smd rect (at 3.25 0) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad G1 smd rect (at -3.25 0.65) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad G2 smd rect (at -2.6 0.65) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad G3 smd rect (at -1.95 0.65) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad G4 smd rect (at -1.3 0.65) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad G5 smd rect (at -0.65 0.65) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad G6 smd rect (at 0 0.65) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad G7 smd rect (at 0.65 0.65) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad G8 smd rect (at 1.3 0.65) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad G9 smd rect (at 1.95 0.65) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad G10 smd rect (at 2.6 0.65) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad G11 smd rect (at 3.25 0.65) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad H1 smd rect (at -3.25 1.3) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad H2 smd rect (at -2.6 1.3) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad H3 smd rect (at -1.95 1.3) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad H4 smd rect (at -1.3 1.3) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad H5 smd rect (at -0.65 1.3) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad H6 smd rect (at 0 1.3) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad H7 smd rect (at 0.65 1.3) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad H8 smd rect (at 1.3 1.3) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad H9 smd rect (at 1.95 1.3) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad H10 smd rect (at 2.6 1.3) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad H11 smd rect (at 3.25 1.3) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad J1 smd rect (at -3.25 1.95) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad J2 smd rect (at -2.6 1.95) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad J3 smd rect (at -1.95 1.95) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad J4 smd rect (at -1.3 1.95) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad J5 smd rect (at -0.65 1.95) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad J6 smd rect (at 0 1.95) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad J7 smd rect (at 0.65 1.95) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad J8 smd rect (at 1.3 1.95) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad J9 smd rect (at 1.95 1.95) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad J10 smd rect (at 2.6 1.95) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad J11 smd rect (at 3.25 1.95) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad K1 smd rect (at -3.25 2.6) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad K2 smd rect (at -2.6 2.6) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad K3 smd rect (at -1.95 2.6) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad K4 smd rect (at -1.3 2.6) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad K5 smd rect (at -0.65 2.6) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad K6 smd rect (at 0 2.6) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad K7 smd rect (at 0.65 2.6) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad K8 smd rect (at 1.3 2.6) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad K9 smd rect (at 1.95 2.6) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad K10 smd rect (at 2.6 2.6) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad K11 smd rect (at 3.25 2.6) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad L1 smd rect (at -3.25 3.25) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad L2 smd rect (at -2.6 3.25) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad L3 smd rect (at -1.95 3.25) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad L4 smd rect (at -1.3 3.25) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad L5 smd rect (at -0.65 3.25) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad L6 smd rect (at 0 3.25) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad L7 smd rect (at 0.65 3.25) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad L8 smd rect (at 1.3 3.25) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad L9 smd rect (at 1.95 3.25) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad L10 smd rect (at 2.6 3.25) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad L11 smd rect (at 3.25 3.25) (size 0.2689 0.2689) (layers F.Cu F.Paste F.Mask))
  (pad 0 connect rect (at -4.175 -3.95) (size 0.15 0.6) (layers F.Cu F.Mask)
    (solder_mask_margin 0.1))
  (pad 0 connect rect (at -3.95 -4.175 90) (size 0.15 0.6) (layers F.Cu F.Mask)
    (solder_mask_margin 0.1))
  (pad 0 connect rect (at 4.175 -3.95) (size 0.15 0.6) (layers F.Cu F.Mask)
    (solder_mask_margin 0.1))
  (pad 0 connect rect (at 4.175 3.95) (size 0.15 0.6) (layers F.Cu F.Mask)
    (solder_mask_margin 0.1))
  (pad 0 connect rect (at -4.175 3.95) (size 0.15 0.6) (layers F.Cu F.Mask)
    (solder_mask_margin 0.1))
  (pad 0 connect rect (at 3.95 -4.175 90) (size 0.15 0.6) (layers F.Cu F.Mask)
    (solder_mask_margin 0.1))
  (pad 0 connect rect (at 3.95 4.175 90) (size 0.15 0.6) (layers F.Cu F.Mask)
    (solder_mask_margin 0.1))
  (pad 0 connect rect (at -3.95 4.175 90) (size 0.15 0.6) (layers F.Cu F.Mask)
    (solder_mask_margin 0.1))
)
