(footprint "Ebyte E220-900MM22S" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "LCSC" "")
  (property "MFG" "Ebyte")
  (property "MPN" "E220-900MM22S")
  (property "Sheetfile" "BendAlert2.kicad_sch")
  (property "Sheetname" "")
  (attr smd)
  (fp_text reference "A1" (at 0 -6.05 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 7e01d3a2-7afc-4ed3-a308-2be2225a481d)
  )
  (fp_text value "E220-900MM22S" (at 0 -3.65 unlocked) (layer "F.Fab")
      (effects (font (size 0.26 0.25) (thickness 0.0625)))
    (tstamp 4e133587-644f-419c-a123-1c8f7011bd6b)
  )
  (fp_text user "${REFERENCE}" (at 0 -3.2 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp 1144837d-565c-4ca7-bfd4-05ad6beb4ac9)
  )
  (fp_arc (start -5.225 -5.125) (mid -5.203033 -5.178033) (end -5.15 -5.2)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 117ec9f1-d107-469a-b3b3-19f4f064b8b4))
  (fp_arc (start -5.146967 5.221967) (mid -5.2 5.2) (end -5.221967 5.146967)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 6b7b2488-217a-45aa-8f7d-a11de85eb171))
  (fp_arc (start 5.15 -5.225) (mid 5.203033 -5.203033) (end 5.225 -5.15)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 22db861b-ed68-454b-8153-49a58a145b3d))
  (fp_arc (start 5.25 5.15) (mid 5.228033 5.203033) (end 5.175 5.225)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp ac63d2de-fd98-4f91-adb0-3ae417fcd373))
  (fp_poly
    (pts
      (xy -5.6 -2.55)
      (xy -5.85 -2.35)
      (xy -5.85 -2.75)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp d786ebba-50cb-4756-a798-391f02eca004))
  (fp_poly
    (pts
      (xy -5.146967 3.646967)
      (xy -5.146967 5.146967)
      (xy -3.646967 5.146967)
      (xy -3.646967 5.296967)
      (xy -5.146967 5.296967)
      (xy -5.296967 5.146967)
      (xy -5.296967 3.646967)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp e1de2b9c-d1ba-4551-83c7-6c1c4777445b))
  (fp_poly
    (pts
      (xy -3.65 -5.125)
      (xy -5.15 -5.125)
      (xy -5.15 -3.625)
      (xy -5.3 -3.625)
      (xy -5.3 -5.125)
      (xy -5.15 -5.275)
      (xy -3.65 -5.275)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 269d0c06-4fcf-4d42-97e1-9ebabec5c236))
  (fp_poly
    (pts
      (xy 3.675 5.15)
      (xy 5.175 5.15)
      (xy 5.175 3.65)
      (xy 5.325 3.65)
      (xy 5.325 5.15)
      (xy 5.175 5.3)
      (xy 3.675 5.3)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 3d6a6be7-7b85-4ffb-8a6d-7da46f6952a0))
  (fp_poly
    (pts
      (xy 5.15 -3.65)
      (xy 5.15 -5.15)
      (xy 3.65 -5.15)
      (xy 3.65 -5.3)
      (xy 5.15 -5.3)
      (xy 5.3 -5.15)
      (xy 5.3 -3.65)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 5f4515f3-5907-4c62-acd0-c42e5e3abe74))
  (fp_line (start -5.600001 2.550001) (end -5.600001 -2.550001)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b93e42d7-c28b-4fb9-9cfa-9df55a4535c6))
  (fp_line (start -5.500001 -5.000001) (end -5.498381 -2.89897)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 78127665-0714-4bee-8c6d-e22cb18da486))
  (fp_line (start -5.500001 5.000001) (end -5.498381 2.89897)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b69a874b-7dcd-4e3f-9a68-09bcbac7fdaa))
  (fp_line (start -5.000001 -5.500001) (end -2.89897 -5.498381)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4cbeda1a-e0f7-407f-8135-3ac4924ea975))
  (fp_line (start -5.000001 5.500001) (end -2.89897 5.498381)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c4f64b16-4920-442f-b83c-a33f5dda272b))
  (fp_line (start -2.550001 -5.600001) (end 2.55 -5.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8fcf55b6-4149-458c-a913-16525a53927e))
  (fp_line (start 2.55 5.6) (end -2.550001 5.600001)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a9d96732-910d-43db-9631-9065a32d773c))
  (fp_line (start 5 -5.5) (end 2.898969 -5.49838)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f72f4139-5816-4ad6-b4b1-7e5bdbe1d228))
  (fp_line (start 5 5.5) (end 2.898969 5.49838)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 54c4f2cc-40b1-436b-9912-4026591af7d3))
  (fp_line (start 5.5 -5) (end 5.49838 -2.898969)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d1f855a4-bfaa-4a18-a9a8-a8b4285eef47))
  (fp_line (start 5.5 5) (end 5.49838 2.898969)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3301ffb6-5083-4f7b-984e-84de73c5744b))
  (fp_line (start 5.6 -2.55) (end 5.6 2.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e9749573-8fda-4a09-b15a-4b0764e48ad2))
  (fp_arc (start -5.600001 -2.550001) (mid -5.574079 -2.731733) (end -5.498381 -2.89897)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4793a964-3c48-428e-8e0e-fce5f0b24794))
  (fp_arc (start -5.500001 -5.000001) (mid -5.353554 -5.353554) (end -5.000001 -5.500001)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 51aa7c1a-1c79-44fb-8f35-eb1a6c4cdcb5))
  (fp_arc (start -5.498381 2.89897) (mid -5.574079 2.731733) (end -5.600001 2.550001)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 55daa8af-2724-4468-921e-ad7200ba9d80))
  (fp_arc (start -5.000001 5.500001) (mid -5.353554 5.353554) (end -5.500001 5.000001)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp cff81e73-2408-4a08-917f-66a1ad63af0a))
  (fp_arc (start -2.89897 -5.498381) (mid -2.731733 -5.574079) (end -2.550001 -5.600001)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9d59d7eb-12c3-4f07-953b-1f8064bf61b8))
  (fp_arc (start -2.550001 5.600001) (mid -2.731733 5.574079) (end -2.89897 5.498381)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1b0a27d9-db4c-4360-a018-5ded92622dcd))
  (fp_arc (start 2.55 -5.6) (mid 2.731732 -5.574078) (end 2.898969 -5.49838)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f9c1d1c6-7848-423f-b9a5-a89e91beebe5))
  (fp_arc (start 2.898969 5.49838) (mid 2.731732 5.574078) (end 2.55 5.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f054749a-086e-4013-bd00-13b5758e9231))
  (fp_arc (start 5 -5.5) (mid 5.353553 -5.353553) (end 5.5 -5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp afce377c-161a-43a6-8e6a-15e2c241b0b5))
  (fp_arc (start 5.49838 -2.898969) (mid 5.574078 -2.731732) (end 5.6 -2.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1fd79817-7c55-4459-819c-9736a8d751d2))
  (fp_arc (start 5.5 5) (mid 5.353553 5.353553) (end 5 5.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 958adfe1-83cc-4b90-9ec6-f7ef89de8c26))
  (fp_arc (start 5.6 2.55) (mid 5.574078 2.731732) (end 5.49838 2.898969)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4b3f3a0f-c4c5-49c3-82db-9b0d9bb72f16))
  (fp_rect (start -5 -5) (end 5 5)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 2f8e5fd9-b534-4e5b-8710-4aeb3127c9ef))
  (pad "1" smd roundrect (at -4.8 -2.54) (size 1.3 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp 50418d03-3585-439e-ac73-9f98f911c345))
  (pad "2" smd roundrect (at -4.8 -1.27) (size 1.3 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp 277ca24d-2554-401a-a2f4-bad9eca117aa))
  (pad "3" smd roundrect (at -4.8 0) (size 1.3 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp 04457087-3dde-4051-8e54-a14e027abc8a))
  (pad "4" smd roundrect (at -4.8 1.27) (size 1.3 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp 910da8da-c5fe-4b8c-a5b3-beb34b5801ef))
  (pad "5" smd roundrect (at -4.8 2.54) (size 1.3 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp aef08452-23b4-4f23-ab36-a411b73a7e69))
  (pad "6" smd roundrect (at -2.54 4.8 90) (size 1.3 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp 631196a2-5af9-46a9-8430-d52e9edf7b1f))
  (pad "7" smd roundrect (at -1.27 4.8 90) (size 1.3 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp bb6a3f02-2004-4ed2-bf35-f7cebb1d71de))
  (pad "8" smd roundrect (at 0 4.8 90) (size 1.3 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp 259e2356-b2bd-4b1f-9185-35c9c60525ce))
  (pad "9" smd roundrect (at 1.27 4.8 90) (size 1.3 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp 5b586c49-fc50-42b5-8ab9-08c0ae8c3613))
  (pad "10" smd roundrect (at 2.54 4.8 90) (size 1.3 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp ada3bb7b-89cc-49ef-b1eb-47ed9ac2f678))
  (pad "11" smd roundrect (at 4.8 2.54 180) (size 1.3 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp d5236483-4969-48ec-a609-d1ebb84f142c))
  (pad "12" smd roundrect (at 4.8 1.27 180) (size 1.3 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp 71dea271-a47d-43d7-a0e6-db357185e58a))
  (pad "13" smd roundrect (at 4.8 0 180) (size 1.3 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp 76417e9c-1fe6-455b-98a2-5720d4fbdeba))
  (pad "14" smd roundrect (at 4.8 -1.27 180) (size 1.3 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp 541d2d29-e4ca-45f2-9a2e-d0cc2fd8c799))
  (pad "15" smd roundrect (at 4.8 -2.54 180) (size 1.3 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp b29330a6-f3d8-47e7-b2de-04b4325d4a2a))
  (pad "16" smd roundrect (at 2.54 -4.8 270) (size 1.3 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp 50431585-945b-424d-aede-c0736b652c33))
  (pad "17" smd roundrect (at 1.27 -4.8 270) (size 1.3 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp fb45f11b-d3b6-475b-86f4-e673efd1270a))
  (pad "18" smd roundrect (at 0 -4.8 270) (size 1.3 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp 62b29ce2-270c-43c6-bae4-fe9092d88256))
  (pad "19" smd roundrect (at -1.27 -4.8 270) (size 1.3 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp 9713bab9-f10e-4fc9-abbc-c3c881ffa9f0))
  (pad "20" smd roundrect (at -2.54 -4.8 270) (size 1.3 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp af182edf-1292-4171-8a4d-2c3677363f16))
  (zone (net 0) (net_name "") (layer "F.Cu") (tstamp fa9a779a-2f2a-4afd-9d2d-4206a6766729) (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias allowed) (pads allowed) (copperpour allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy -5 -5)
        (xy -3 -5)
        (xy -3 -4.25)
        (xy 3 -4.25)
        (xy 3 -5)
        (xy 5 -5)
        (xy 5 -3)
        (xy 4.25 -3)
        (xy 4.25 3)
        (xy 5 3)
        (xy 5 5)
        (xy 3 5)
        (xy 3 4.25)
        (xy -3 4.25)
        (xy -3 5)
        (xy -5 5)
        (xy -5 3)
        (xy -4.25 3)
        (xy -4.25 -3)
        (xy -5 -3)
      )
    )
  )
  (model ":KICAD7_3DMODEL_DIR:RF_Module.3dshapes/Ebyte E220-900MM22S.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
