(footprint "PinHeader_2x04_P1.27mm_Vertical_Mod" (version 20220417) (generator pcbnew)
  (layer "F.Cu")
  (descr "Through hole straight pin header, 2x04, 1.27mm pitch, double rows")
  (tags "Through hole pin header THT 2x04 1.27mm double row")
  (property "Dielectric" "")
  (property "Footprint_Density" "")
  (property "Footprint_Library" "")
  (property "JLCPCB Part" "")
  (property "LCSC" "")
  (property "MFG" "")
  (property "MPN" "")
  (property "MPN_ALT1" "")
  (property "Mouser" "")
  (property "Note" "")
  (property "Package" "")
  (property "Sheetfile" "ESC_Dual_10A.kicad_sch")
  (property "Sheetname" "")
  (property "Spice_Model" "")
  (property "Spice_Netlist_Enabled" "")
  (property "Spice_Primitive" "")
  (property "Tolerance" "")
  (property "USD_per_1" "")
  (property "USD_per_1000" "")
  (property "Voltage" "")
  (property "ki_description" "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)")
  (property "ki_keywords" "connector")
  (attr through_hole)
  (fp_text reference "J5" (at 0.635 -1.695) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 71015010-c3cc-401f-9481-1848674330b6)
  )
  (fp_text value "Conn_01x08" (at 0.635 5.505) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 55ee0697-e51d-456a-a0b9-d3bc19de07a4)
  )
  (fp_text user "${REFERENCE}" (at 0.635 1.905 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e7bbb2c5-9ac9-480b-af1f-a1f445445c50)
  )
  (fp_rect (start -1.0668 -0.635) (end 2.3368 4.445)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp 0d0d3820-4468-4a61-a852-dde128cf741a))
  (fp_line (start -1.35 4.45) (end -1.35 -0.65)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp cee10981-568b-4da9-a8b0-b30601c50aec))
  (fp_line (start -1.1 -0.9) (end 2.35 -0.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0f7cdc88-c778-4280-ab84-78c8ba4ac4ef))
  (fp_line (start 2.35 4.7) (end -1.1 4.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 96b3bf37-41e5-42ce-861d-956a19d8ec3f))
  (fp_line (start 2.6 -0.65) (end 2.6 4.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f4fa31c4-19e5-4daa-8943-bf6169d4983a))
  (fp_arc (start -1.35 -0.65) (mid -1.276777 -0.826777) (end -1.1 -0.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7e258890-0d9d-4aa5-abe9-42ba8dbd8cf9))
  (fp_arc (start -1.1 4.7) (mid -1.276777 4.626777) (end -1.35 4.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f22ea637-975e-4326-a247-7baff5047d02))
  (fp_arc (start 2.35 -0.9) (mid 2.526777 -0.826777) (end 2.6 -0.65)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0926032e-9c66-43ed-97a5-c945bd2bb868))
  (fp_arc (start 2.6 4.45) (mid 2.526777 4.626777) (end 2.35 4.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7520668c-39c0-44b3-b3bc-601c39c424dc))
  (fp_line (start -1.07 -0.635) (end 2.34 -0.635)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 14faa458-c532-4b2d-ab47-d647d76bf918))
  (fp_line (start -1.07 4.445) (end -1.07 -0.635)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3675097b-75f4-4fba-ab34-747382537cc2))
  (fp_line (start 2.34 -0.635) (end 2.34 4.445)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp db96be1d-91a7-43e1-86ed-cb700c7b023e))
  (fp_line (start 2.34 4.445) (end -1.07 4.445)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6b671ae1-9789-48a4-9577-2c68e525d40a))
  (pad "1" thru_hole rect (at 0 0) (size 1 0.8) (drill 0.6) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp 7dc65770-8128-42cd-921a-042e52abd682))
  (pad "2" thru_hole roundrect (at 1.27 0) (size 1 0.8) (drill 0.6) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (roundrect_rratio 0.25) (tstamp ef05a441-a2c0-476f-8d96-4f3c45c9fb80))
  (pad "3" thru_hole roundrect (at 0 1.27) (size 1 0.8) (drill 0.6) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp 1ec5954e-32c8-422d-9149-9d9dcb661046))
  (pad "4" thru_hole roundrect (at 1.27 1.27) (size 1 0.8) (drill 0.6) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp 74868f48-e253-45c4-a8ec-1b882a1f7adc))
  (pad "5" thru_hole roundrect (at 0 2.54) (size 1 0.8) (drill 0.6) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp 329b9973-64ea-4d3a-bc9e-f831d616c892))
  (pad "6" thru_hole roundrect (at 1.27 2.54) (size 1 0.8) (drill 0.6) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp 9f9199aa-418a-4053-a4c0-2d29c274e222))
  (pad "7" thru_hole roundrect (at 0 3.81) (size 1 0.8) (drill 0.6) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp d34d8785-33ac-4090-acaf-0bd2189f7d3d))
  (pad "8" thru_hole roundrect (at 1.27 3.81) (size 1 0.8) (drill 0.6) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp ce2118eb-29e1-4c4f-8f18-d128344549fb))
  (model "${KICAD7_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x04_P1.27mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
