(module "WLP-4_0.73x0.73mm_Layout2x2_P0.35mm_Ball0.22mm_Pad0.2mm_NSMD" (layer F.Cu) (tedit 5E35B845)
  (descr "WLP-4, 2x2 raster, 0.73x0.73mm package, pitch 0.35mm; https://datasheets.maximintegrated.com/en/ds/MAX40200.pdf")
  (tags "BGA 4 0.35")
  (solder_mask_margin 0.02)
  (solder_paste_margin 0.000001)
  (attr smd)
  (fp_text reference "U2" (at 0.6 2.4) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "MAX40200ANS" (at 0 1.364) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user "%R" (at 0 0) (layer F.Fab)
    (effects (font (size 0.17 0.17) (thickness 0.0255)))
  )
  (fp_line (start -0.474 0.474) (end -0.474 -0.292) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.474 0.474) (end -0.474 0.474) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.474 -0.474) (end 0.474 0.474) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.292 -0.474) (end 0.474 -0.474) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.37 -1.37) (end -1.37 -1.37) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.37 1.37) (end 1.37 -1.37) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.37 1.37) (end 1.37 1.37) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.37 -1.37) (end -1.37 1.37) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.364 -0.364) (end 0.364 0.364) (layer F.Fab) (width 0.1))
  (fp_line (start -0.182 -0.364) (end 0.364 -0.364) (layer F.Fab) (width 0.1))
  (fp_line (start -0.364 -0.182) (end -0.182 -0.364) (layer F.Fab) (width 0.1))
  (fp_line (start -0.364 0.364) (end -0.364 -0.182) (layer F.Fab) (width 0.1))
  (fp_line (start 0.364 0.364) (end -0.364 0.364) (layer F.Fab) (width 0.1))
  (pad "A1" smd circle (at -0.175 -0.175) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "A2" smd circle (at 0.175 -0.175) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "B1" smd circle (at -0.175 0.175) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "B2" smd circle (at 0.175 0.175) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask"))
  (model "${KICAD7_3DMODEL_DIR}/Package_BGA.3dshapes/WLP-4_0.73x0.73mm_Layout2x2_P0.35mm_Ball0.22mm_Pad0.2mm_NSMD.wrl"
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "${KICAD7_3DMODEL_DIR}/Package_BGA.3dshapes/DSBGA-4_0.73x0.73mm_P0.35.step"
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
