(module JST_ZH_B8B-ZR (layer F.Cu) (tedit 5818F99A)
  (solder_mask_margin -0.05)
  (fp_text reference J2 (at 0 -1.125) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text value PROGRAM (at 0 -2.375) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_line (start 7.25 -2.25) (end 7.25 2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 7.25 2.25) (end -7.25 2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -7.25 2.25) (end -7.25 -2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -7.25 -2.25) (end 7.25 -2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -6.75 -1.75) (end -6.75 1.75) (layer F.SilkS) (width 0.127))
  (fp_line (start -6.75 1.75) (end 6.75 1.75) (layer F.SilkS) (width 0.127))
  (fp_line (start 6.75 1.75) (end 6.75 -1.75) (layer F.SilkS) (width 0.127))
  (fp_line (start -6.75 -1.75) (end 6.75 -1.75) (layer F.SilkS) (width 0.127))
  (pad 1 thru_hole circle (at -5.25 0.45) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -3.75 0.45) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -2.25 0.45) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at -0.75 0.45) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 0.75 0.45) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 2.25 0.45) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 3.75 0.45) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 5.25 0.45) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
  (pad 1 connect roundrect (at -5.25 0.25) (size 1 1.6) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 2 connect roundrect (at -3.75 0.25) (size 1 1.6) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 3 connect roundrect (at -2.25 0.25) (size 1 1.6) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 4 connect roundrect (at -0.75 0.25) (size 1 1.6) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 5 connect roundrect (at 0.75 0.25) (size 1 1.6) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 6 connect roundrect (at 2.25 0.25) (size 1 1.6) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 7 connect roundrect (at 3.75 0.25) (size 1 1.6) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 8 connect roundrect (at 5.25 0.25) (size 1 1.6) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (model 3D/SH/JST_ZH_B8B-ZR.wrl
    (at (xyz 0 -0.06900000000000001 0))
    (scale (xyz 0.393701 0.393701 0.393701))
    (rotate (xyz 270 0 0))
  )
  (model Connector_JST.3dshapes/JST_B8B-ZR.step
    (at (xyz 0 -0.06889763779527559 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
