(footprint "3216_B_Shunt"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(tags "1206 3216")
	(property "Reference" "B1B_R16"
		(at 2.1 0 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "accc1611-ca45-4175-940d-4f52f0d27cbb")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
			(justify left)
		)
	)
	(property "Value" "300u"
		(at 1.8 0.6 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "c8b956fa-0951-4e22-92cf-1509564ae19e")
		(effects
			(font
				(size 0.2 0.2)
				(thickness 0.05)
			)
			(justify left)
		)
	)
	(property "Footprint" "Resistor_SMD:3216_B_Shunt"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "5425acfe-6619-45e4-b562-1785ade554bb")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "1f8f09de-67ca-452d-b196-a33f79e56d81")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "300 µOhm 1% 5W"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "18f2d19f-669c-4d34-bdc9-dc2eefc04334")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "Vishay"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "376ebb07-3bd6-4269-bb0a-57472f8cd3f2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "WSLF1206L3000FE6"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "25c1a18f-3a23-4ab6-aca0-e27bf6712c63")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" "C29615611"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4cdc3cbf-d735-4bcc-a2ff-06dd675db1a9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Preferred" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "66041552-34a5-4b11-94b9-c512a83a76dd")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "fa53f3de-0c51-470a-8f05-7932bed01717")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Dielectric" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7aa29026-9705-49d9-be17-fb0da16c7895")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint_Density" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a27da395-b60e-40f0-833c-0a3bab134ac8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint_Library" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ad13f104-401d-465b-8ae8-541250757e3d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "JLCPCB Part" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4f668ed5-ea4e-4fb5-980d-c827e788fa71")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Mouser" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "91a498e5-a04c-4d91-b93b-276572cf1da1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(solder_mask_margin 0.05)
	(solder_paste_margin -0.05)
	(attr smd)
	(net_tie_pad_groups "1,2" "3,4")
	(fp_poly
		(pts
			(xy 0.525 -0.975001) (xy -0.525 -0.975001) (xy -0.525 -0.825001) (xy 0.525 -0.825001)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "ba3c0682-397e-4d66-8f69-5e5aa662b8f3")
	)
	(fp_poly
		(pts
			(xy 0.525 0.825001) (xy -0.525 0.825001) (xy -0.525 0.975001) (xy 0.525 0.975001)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "54d654bf-a9ee-4edb-8605-ebc1863ee2e1")
	)
	(fp_line
		(start -2.125 0.675)
		(end -2.125 -0.675)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "81419e3c-2bb4-48a3-83ea-b68a514eb98e")
	)
	(fp_line
		(start -1.7 -1.1)
		(end 1.7 -1.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ce86c18d-4462-457a-802b-53d338a33669")
	)
	(fp_line
		(start 1.7 1.1)
		(end -1.7 1.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "f263b32d-be42-4d11-a8b5-0d1f13cf43ae")
	)
	(fp_line
		(start 2.125 -0.675)
		(end 2.125 0.675)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "5f44954c-fe25-4633-ab55-f00b0dddf879")
	)
	(fp_arc
		(start -2.125 -0.675)
		(mid -2.00052 -0.97552)
		(end -1.7 -1.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "67f82db5-5c27-4d2b-a516-cc4dc2704ba5")
	)
	(fp_arc
		(start -1.7 1.1)
		(mid -2.00052 0.97552)
		(end -2.125 0.675)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "55bdb38f-97ca-4506-86c0-c75ea1403182")
	)
	(fp_arc
		(start 1.7 -1.1)
		(mid 2.00052 -0.97552)
		(end 2.125 -0.675)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "eea6509f-e342-4bde-9d4b-88424dd8a7ea")
	)
	(fp_arc
		(start 2.125 0.675)
		(mid 2.00052 0.97552)
		(end 1.7 1.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "8df04bb5-0b69-4511-bb88-dd63cd1038c6")
	)
	(fp_poly
		(pts
			(xy 1.6 0.8) (xy -1.6 0.8) (xy -1.6 -0.8) (xy 1.6 -0.8)
		)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "640975dd-fb38-4930-823f-73d54225c9f0")
	)
	(pad "" smd roundrect
		(at -1.325 0)
		(size 1.3 1.9)
		(layers "F.Paste")
		(roundrect_rratio 0.1923076923)
		(uuid "6b648600-9fe6-4937-8737-3dff10783f33")
	)
	(pad "" smd roundrect
		(at 1.325 0)
		(size 1.3 1.9)
		(layers "F.Paste")
		(roundrect_rratio 0.1923076923)
		(uuid "258f7035-1829-49e1-bb64-1f38a9edcd7f")
	)
	(pad "1" smd roundrect
		(at -1.325 0)
		(size 1.3 1.9)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.04545454546)
		(chamfer top_right bottom_right)
		(uuid "9ac4803e-d70e-47b3-bf2c-e60cbf83e319")
	)
	(pad "2" smd oval
		(at -0.175 0)
		(size 0.7 0.2)
		(drill
			(offset -0.25 0)
		)
		(layers "F.Cu")
		(uuid "e2483f51-8c44-44f0-aefd-da825159a1e5")
	)
	(pad "3" smd oval
		(at 0.175 0 180)
		(size 0.7 0.2)
		(drill
			(offset -0.25 0)
		)
		(layers "F.Cu")
		(uuid "fd8cf3c0-5938-4534-83dc-aa99cd5feb2a")
	)
	(pad "4" smd roundrect
		(at 1.325 0 180)
		(size 1.3 1.9)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.04545454546)
		(chamfer top_right bottom_right)
		(uuid "a3ccb4f1-5b68-4047-a478-ec9a005a7f5b")
	)
	(model "${KICAD7_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
		(hide yes)
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${KICAD7_3DMODEL_DIR}/Resistor_SMD.3dshapes/WSLF1206L3000FE6.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
