(module LED_WS2812_PLCC6_5.0x5.0mm_P1.6mm (layer F.Cu) (tedit 5C1C9402)
  (descr https://cdn-shop.adafruit.com/datasheets/WS2812.pdf)
  (tags "LED RGB NeoPixel")
  (attr smd)
  (fp_text reference REF** (at 0 -3.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value LED_WS2812_PLCC6_5.0x5.0mm_P1.6mm (at 0 3.25) (layer F.Fab)
    (effects (font (size 0.25 0.25) (thickness 0.0625)))
  )
  (fp_text user %R (at 0 1.75) (layer F.Fab)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_line (start 3.45 -2.75) (end -3.45 -2.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.45 2.75) (end 3.45 -2.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.45 2.75) (end 3.45 2.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.45 -2.75) (end -3.45 2.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.5 -1.5) (end -1.5 -2.5) (layer F.Fab) (width 0.1))
  (fp_line (start -2.5 -2.5) (end 2.5 -2.5) (layer F.Fab) (width 0.1))
  (fp_line (start 2.5 -2.5) (end 2.5 2.5) (layer F.Fab) (width 0.1))
  (fp_line (start 2.5 2.5) (end -2.5 2.5) (layer F.Fab) (width 0.1))
  (fp_line (start -2.5 2.5) (end -2.5 -2.5) (layer F.Fab) (width 0.1))
  (fp_line (start -2.75 2.75) (end 2.75 2.75) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.75 -2.25) (end -2.75 -2.75) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.75 -2.75) (end 2.75 -2.75) (layer F.SilkS) (width 0.12))
  (fp_circle (center 0 0) (end 0 -2) (layer F.Fab) (width 0.1))
  (pad 4 smd roundrect (at 2.45 1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (pad 5 smd roundrect (at 2.45 0) (size 1.5 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (pad 6 smd roundrect (at 2.45 -1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (pad 3 smd roundrect (at -2.45 1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (pad 2 smd roundrect (at -2.45 0) (size 1.5 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (pad 1 smd roundrect (at -2.45 -1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (model ${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/SK9822.step
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
