(footprint "1005_A" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (tags "0402 1005 Resistor")
  (property "LCSC" "C914087")
  (property "MFG" "BHFUSE")
  (property "MPN" "BSMD0402L-050")
  (property "Sheetfile" "QuadCameraCarrier.kicad_sch")
  (property "Sheetname" "")
  (solder_mask_margin 0.03)
  (solder_paste_margin -0.02)
  (attr smd)
  (fp_text reference "F8" (at 0.875 0 unlocked) (layer "F.SilkS")
      (effects (font (size 0.4 0.4) (thickness 0.1)) (justify left))
    (tstamp 08e77dfb-5cf3-44cf-848b-e6363b1fff5a)
  )
  (fp_text value "6V 1A" (at 1 0.4 unlocked) (layer "F.Fab")
      (effects (font (size 0.2 0.2) (thickness 0.05)) (justify left))
    (tstamp 5c8e32d3-591e-4803-8b48-f428179072ee)
  )
  (fp_poly
    (pts
      (xy 0.2 -0.3)
      (xy -0.2 -0.3)
      (xy -0.2 -0.45)
      (xy 0.2 -0.45)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 4eb2de93-8255-470a-a1a1-e0ead2035524))
  (fp_poly
    (pts
      (xy 0.2 0.45)
      (xy -0.2 0.45)
      (xy -0.2 0.3)
      (xy 0.2 0.3)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 32ca6dfa-f699-48c2-84ce-6c8fb897cb5d))
  (fp_line (start -1 -0.1) (end -1 0.1)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2ad96223-92bc-416a-8063-b803da6098c5))
  (fp_line (start 0.65 -0.45) (end -0.65 -0.45)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bdcf5277-86dc-4f74-9ed3-b97c888379cf))
  (fp_line (start 0.65 0.45) (end -0.65 0.45)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d6f6c08f-7014-48b2-9dcc-18bdff428374))
  (fp_line (start 1 -0.1) (end 1 0.1)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0044ec96-f0c6-4d7e-8c82-530f78172f81))
  (fp_arc (start -1 -0.1) (mid -0.897487 -0.347487) (end -0.65 -0.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 58f6c2ee-8fe5-4399-9b55-32bcebea8a68))
  (fp_arc (start -0.65 0.45) (mid -0.897487 0.347487) (end -1 0.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3f79c47e-fc09-4eed-88d0-a4ecfedbaf29))
  (fp_arc (start 0.65 -0.45) (mid 0.897487 -0.347487) (end 1 -0.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6993aead-8f94-4385-adfe-c00cd9880a39))
  (fp_arc (start 1 0.1) (mid 0.897487 0.347487) (end 0.65 0.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f5b7750b-281a-49dc-b31c-eedfaac91f88))
  (fp_line (start -0.5 -0.25) (end 0.5 -0.25)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 8625b7c8-0226-4346-85a3-f6ef1e2fff6f))
  (fp_line (start -0.5 0.25) (end -0.5 -0.25)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 2038be94-65bc-43c8-b4e3-ee96e8b44500))
  (fp_line (start 0.5 -0.25) (end 0.5 0.25)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 8929eea7-3123-4710-aa0f-61be77fe63da))
  (fp_line (start 0.5 0.25) (end -0.5 0.25)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 53391cb1-b93f-4db1-90f7-f964ac755220))
  (pad "" smd circle (at -0.55 0) (size 0.5 0.5) (layers "F.Paste") (tstamp 4988c092-6fcb-48c5-b99e-4992e5c97990))
  (pad "" smd circle (at 0.55 0) (size 0.5 0.5) (layers "F.Paste") (tstamp 6431f603-bb61-442b-99d3-02bd893ada39))
  (pad "1" smd roundrect (at -0.55 0) (size 0.6 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.08) (chamfer top_right bottom_right) (tstamp 23f87512-34a5-474e-bbc2-77604142a74f))
  (pad "2" smd roundrect (at 0.55 0) (size 0.6 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.08) (chamfer top_left bottom_left) (tstamp 862a12a6-16b0-42a1-bca8-3dcf84b7c7a3))
  (model "${KICAD7_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
