(module JST_GH_BM04B-GHS (layer F.Cu) (tedit 575080F8)
  (descr "JST GH series connector, BM04B-GHS-TBT, top entry type")
  (tags "connector jst GH SMT top vertical entry 1.25mm pitch")
  (attr smd)
  (fp_text reference P2 (at -3.5 -2) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value UART (at 0 -3.25) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_line (start -2.5 2.975) (end 2.5 2.975) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.5 2.975) (end 2.5 2.475) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.5 2.475) (end -2.5 2.475) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.5 2.475) (end -2.5 2.975) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.2 -0.225) (end -4.2 -1.325) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.2 -1.325) (end -2.55 -1.325) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.55 -1.325) (end -2.55 -0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.55 -0.825) (end -3.7 -0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.7 -0.825) (end -3.7 -0.225) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.7 -0.225) (end -4.2 -0.225) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.2 -0.225) (end 4.2 -1.325) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.2 -1.325) (end 2.55 -1.325) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.55 -1.325) (end 2.55 -0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.55 -0.825) (end 3.7 -0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.7 -0.825) (end 3.7 -0.225) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.7 -0.225) (end 4.2 -0.225) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.125 0.325) (end -2.125 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.125 0.825) (end -1.625 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.625 0.825) (end -1.625 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.625 0.325) (end -2.125 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.875 0.325) (end -0.875 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.875 0.825) (end -0.375 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.375 0.825) (end -0.375 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.375 0.325) (end -0.875 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.375 0.325) (end 0.375 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.375 0.825) (end 0.875 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.875 0.825) (end 0.875 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.875 0.325) (end 0.375 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.625 0.325) (end 1.625 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.625 0.825) (end 2.125 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.125 0.825) (end 2.125 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.125 0.325) (end 1.625 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.6 -3.05) (end -4.6 3.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.6 3.6) (end 4.6 3.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.6 3.6) (end 4.6 -3.05) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.6 -3.05) (end -4.6 -3.05) (layer F.CrtYd) (width 0.05))
  (pad 1 smd rect (at -1.875 -1.675) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.625 -1.675) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0.625 -1.675) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 1.875 -1.675) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 3.6 1.675) (size 1 2.8) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -3.6 1.675) (size 1 2.8) (layers F.Cu F.Paste F.Mask))
  (model Connectors_JST.3dshapes/JST_GH_BM04B-GHS-TBT_04x1.25mm_Straight.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
