(module "USB_C_Plug_JAE_DX07P024AJ1" (layer F.Cu) (tedit 5E2EDB67)
  (descr "Universal Serial Bus (USB) Shielded I/O Plug, Type C, Right Angle, Surface Mount, https://www.jae.com/en/searchfilter/?topics_keyword=DX07P024AJ1&mainItemSelect=1")
  (tags "USB Type-C Plug Edge Mount")
  (attr smd)
  (fp_text reference "REF**" (at -2.6925 -3.54) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "USB_C_Plug_JAE_DX07P024AJ1" (at -0.1725 4.27) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -4.5525 3.27) (end -4.5525 -2.38) (layer B.CrtYd) (width 0.05))
  (fp_line (start 4.1475 3.27) (end -4.5525 3.27) (layer B.CrtYd) (width 0.05))
  (fp_line (start 4.1475 -2.38) (end 4.1475 3.27) (layer B.CrtYd) (width 0.05))
  (fp_line (start -4.5525 -2.38) (end 4.1475 -2.38) (layer B.CrtYd) (width 0.05))
  (fp_line (start -4.5525 3.27) (end -4.5525 -2.38) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.1475 3.27) (end -4.5525 3.27) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.1475 -2.38) (end 4.1475 3.27) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.5525 -2.38) (end 4.1475 -2.38) (layer F.CrtYd) (width 0.05))
  (fp_text user "%R" (at 0 0.5525) (layer F.Fab)
    (effects (font (size 0.75 0.75) (thickness 0.1)))
  )
  (fp_text user "PCB Edge" (at 0 3.0225) (layer Dwgs.User)
    (effects (font (size 0.5 0.5) (thickness 0.1)))
  )
  (fp_line (start 3.575 2.3725) (end 3.9 1.9225) (layer Dwgs.User) (width 0.1))
  (fp_line (start -2.925 2.8225) (end -2.925 2.5725) (layer Dwgs.User) (width 0.1))
  (fp_line (start 2.925 2.8225) (end 2.925 2.5725) (layer Dwgs.User) (width 0.1))
  (fp_line (start 1.1 2.8225) (end 1.1 2.6225) (layer Dwgs.User) (width 0.1))
  (fp_line (start -0.3 2.6225) (end -0.3 2.8225) (layer Dwgs.User) (width 0.1))
  (fp_arc (start 3.125 2.5725) (end 2.925 2.5725) (angle 90) (layer Dwgs.User) (width 0.1))
  (fp_arc (start -3.125 2.5725) (end -3.125 2.3725) (angle 90) (layer Dwgs.User) (width 0.1))
  (fp_arc (start -2.725 2.8225) (end -2.725 3.0225) (angle 90) (layer Dwgs.User) (width 0.1))
  (fp_arc (start 2.725 2.8225) (end 2.925 2.8225) (angle 90) (layer Dwgs.User) (width 0.1))
  (fp_arc (start 1.3 2.8225) (end 1.3 3.0225) (angle 90) (layer Dwgs.User) (width 0.1))
  (fp_arc (start 0.9 2.6225) (end 0.9 2.4225) (angle 90) (layer Dwgs.User) (width 0.1))
  (fp_arc (start -0.1 2.6225) (end -0.3 2.6225) (angle 90) (layer Dwgs.User) (width 0.1))
  (fp_arc (start -0.5 2.8225) (end -0.3 2.8225) (angle 90) (layer Dwgs.User) (width 0.1))
  (fp_line (start 3.9 1.9225) (end 3.9 -1.9175) (layer Dwgs.User) (width 0.1))
  (fp_line (start -3.9 1.9225) (end -3.9 -0.2275) (layer Dwgs.User) (width 0.1))
  (fp_line (start 1.3 3.0225) (end 2.725 3.0225) (layer Dwgs.User) (width 0.1))
  (fp_line (start -0.5 3.0225) (end -2.725 3.0225) (layer Dwgs.User) (width 0.1))
  (fp_line (start -0.1 2.4225) (end 0.9 2.4225) (layer Dwgs.User) (width 0.1))
  (fp_line (start 3.125 2.3725) (end 3.575 2.3725) (layer Dwgs.User) (width 0.1))
  (fp_line (start -3.125 2.3725) (end -3.53 2.3725) (layer Dwgs.User) (width 0.1))
  (fp_line (start -3.53 2.3725) (end -3.9 1.9225) (layer Dwgs.User) (width 0.1))
  (fp_line (start -4.3 -0.2275) (end -3.9 -0.2275) (layer Dwgs.User) (width 0.1))
  (fp_line (start -4.3 -1.93) (end -4.3 -0.2275) (layer Dwgs.User) (width 0.1))
  (pad "A2" smd rect (at 2.25 1.1475) (size 0.26 1.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "A3" smd rect (at 1.75 1.1475) (size 0.26 1.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "A4" smd rect (at 1.25 1.1475) (size 0.26 1.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "A5" smd rect (at 0.75 1.1475) (size 0.26 1.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "A6" smd rect (at 0.25 1.1475 180) (size 0.26 1.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "A7" smd rect (at -0.25 1.1475 180) (size 0.26 1.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "A8" smd rect (at -0.75 1.1475) (size 0.26 1.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "A9" smd rect (at -1.25 1.1475) (size 0.26 1.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "A10" smd rect (at -1.75 1.1475) (size 0.26 1.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "A11" smd rect (at -2.25 1.1475) (size 0.26 1.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "A12" smd rect (at -2.825 1.1475) (size 0.41 1.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "A1" smd rect (at 2.825 1.1475) (size 0.41 1.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "S1" smd rect (at 3.405 0.8975) (size 0.36 2.05) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "S1" smd rect (at -3.405 0.8975) (size 0.36 2.05) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "B5" smd rect (at -0.75 1.1475) (size 0.26 1.55) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "B6" smd rect (at -0.25 1.1475 180) (size 0.26 1.55) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "B1" smd rect (at -2.825 1.1475) (size 0.41 1.55) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "B12" smd rect (at 2.825 1.1475) (size 0.41 1.55) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "B11" smd rect (at 2.25 1.1475) (size 0.26 1.55) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "B10" smd rect (at 1.75 1.1475) (size 0.26 1.55) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "B4" smd rect (at -1.25 1.1475) (size 0.26 1.55) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "B9" smd rect (at 1.25 1.1475) (size 0.26 1.55) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "B2" smd rect (at -2.25 1.1475) (size 0.26 1.55) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "B7" smd rect (at 0.25 1.1475) (size 0.26 1.55) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "B3" smd rect (at -1.75 1.1475) (size 0.26 1.55) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "B8" smd rect (at 0.75 1.1475) (size 0.26 1.55) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "S1" smd rect (at -3.625 -1.1725) (size 0.8 1.5) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "S1" smd rect (at 3.27 -1.1725 180) (size 0.7 1.5) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "" smd rect (at 3.405 1.0475) (size 0.36 1.75) (layers "F.Cu" "F.Mask"))
  (pad "" smd rect (at -3.405 1.0475) (size 0.36 1.75) (layers "F.Cu" "F.Mask"))
  (model "${KICAD7_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Plug_JAE_DX07P024AJ1.wrl"
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "${KICAD7_3DMODEL_DIR}/Connector_USB.3dshapes/JAE_DX07P024AJ5.STEP"
    (offset (xyz 0 -12.2 -0.4))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
