(module TI_MicroStar_Junior_BGA_2.5x2.5mm (layer F.Cu) (tedit 54270AE1)
  (solder_mask_margin -0.065)
  (solder_paste_margin -0.05)
  (attr smd)
  (fp_text reference U5 (at 0 -2) (layer Cmts.User)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text value TI_TPA2005D1_BGA (at 0 1.25) (layer F.SilkS) hide
    (effects (font (size 0.2 0.2) (thickness 0.05)))
  )
  (fp_text user A1 (at 1 1.75) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.15)))
  )
  (fp_line (start 1.5 -1.5) (end 1.5 1.5) (layer F.SilkS) (width 0.127))
  (fp_line (start 1.5 1.5) (end -1.5 1.5) (layer F.SilkS) (width 0.127))
  (fp_line (start -1.5 1.5) (end -1.5 -1.5) (layer F.SilkS) (width 0.127))
  (fp_line (start -1.5 -1.5) (end 1.5 -1.5) (layer F.SilkS) (width 0.127))
  (pad A1 smd circle (at 0.75 0.75) (size 0.38 0.38) (layers F.Cu F.Paste F.Mask))
  (pad A2 smd circle (at 0.25 0.75) (size 0.38 0.38) (layers F.Cu F.Paste F.Mask))
  (pad A3 smd circle (at -0.25 0.75) (size 0.38 0.38) (layers F.Cu F.Paste F.Mask))
  (pad A4 smd circle (at -0.75 0.75) (size 0.38 0.38) (layers F.Cu F.Paste F.Mask))
  (pad B1 smd circle (at 0.75 0.25) (size 0.38 0.38) (layers F.Cu F.Paste F.Mask))
  (pad B3 smd circle (at -0.25 0.25) (size 0.38 0.38) (layers F.Cu F.Paste F.Mask))
  (pad B4 smd circle (at -0.75 0.25) (size 0.38 0.38) (layers F.Cu F.Paste F.Mask))
  (pad C1 smd circle (at 0.75 -0.25) (size 0.38 0.38) (layers F.Cu F.Paste F.Mask))
  (pad C2 smd circle (at 0.25 -0.25) (size 0.38 0.38) (layers F.Cu F.Paste F.Mask))
  (pad C3 smd circle (at -0.25 -0.25) (size 0.38 0.38) (layers F.Cu F.Paste F.Mask))
  (pad C4 smd circle (at -0.75 -0.25) (size 0.38 0.38) (layers F.Cu F.Paste F.Mask))
  (pad D1 smd circle (at 0.75 -0.75) (size 0.38 0.38) (layers F.Cu F.Paste F.Mask))
  (pad D2 smd circle (at 0.25 -0.75) (size 0.38 0.38) (layers F.Cu F.Paste F.Mask))
  (pad D3 smd circle (at -0.25 -0.75) (size 0.38 0.38) (layers F.Cu F.Paste F.Mask))
  (pad D4 smd circle (at -0.75 -0.75) (size 0.38 0.38) (layers F.Cu F.Paste F.Mask))
)
