(footprint "Arc_Ri0.9_0.15-0.15_x12_270deg" (version 20221019) (generator pcbnew)
  (layer "F.Cu")
  (zone_connect 0)
  (attr board_only exclude_from_pos_files exclude_from_bom)
  (fp_text reference "REF**" (at 0 -8.075 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2c79dc91-7d87-4312-a8b9-19715fd00ffa)
  )
  (fp_text value "Arc_Ri0.9_0.15-0.15_x12_270deg" (at 0 -6.575 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 5beec144-4cc1-474b-a704-c5bb50798690)
  )
  (fp_text user "${REFERENCE}" (at 0 -5.075 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 329fd6c7-7418-4566-b934-69bde1aafa29)
  )
  (pad "1" smd custom (at -0.975 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 1.66442911166 -0.689429111656) (end 0.975 0.975) (width 0.15))
    ))
  (pad "1" smd custom (at 0 0.975) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -0.975 -0.975) (mid 0.689429111656 -1.66442911166) (end 0 0) (width 0.15))
    ))
  (pad "2" smd custom (at -1.275 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 2.17656114601 -0.901561146012) (end 1.275 1.275) (width 0.15))
    ))
  (pad "2" smd custom (at 0 1.275) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -1.275 -1.275) (mid 0.901561146012 -2.17656114601) (end 0 0) (width 0.15))
    ))
  (pad "3" smd custom (at -1.575 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 2.68869318037 -1.11369318037) (end 1.575 1.575) (width 0.15))
    ))
  (pad "3" smd custom (at 0 1.575) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -1.575 -1.575) (mid 1.11369318037 -2.68869318037) (end 0 0) (width 0.15))
    ))
  (pad "4" smd custom (at -1.875 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 3.20082521472 -1.32582521472) (end 1.875 1.875) (width 0.15))
    ))
  (pad "4" smd custom (at 0 1.875) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -1.875 -1.875) (mid 1.32582521472 -3.20082521472) (end 0 0) (width 0.15))
    ))
  (pad "5" smd custom (at -2.175 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 3.71295724908 -1.53795724908) (end 2.175 2.175) (width 0.15))
    ))
  (pad "5" smd custom (at 0 2.175) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -2.175 -2.175) (mid 1.53795724908 -3.71295724908) (end 0 0) (width 0.15))
    ))
  (pad "6" smd custom (at -2.475 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 4.22508928344 -1.75008928344) (end 2.475 2.475) (width 0.15))
    ))
  (pad "6" smd custom (at 0 2.475) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -2.475 -2.475) (mid 1.75008928344 -4.22508928344) (end 0 0) (width 0.15))
    ))
  (pad "7" smd custom (at -2.775 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 4.73722131779 -1.96222131779) (end 2.775 2.775) (width 0.15))
    ))
  (pad "7" smd custom (at 0 2.775) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -2.775 -2.775) (mid 1.96222131779 -4.73722131779) (end 0 0) (width 0.15))
    ))
  (pad "8" smd custom (at -3.075 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 5.24935335215 -2.17435335215) (end 3.075 3.075) (width 0.15))
    ))
  (pad "8" smd custom (at 0 3.075) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -3.075 -3.075) (mid 2.17435335215 -5.24935335215) (end 0 0) (width 0.15))
    ))
  (pad "9" smd custom (at -3.375 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 5.7614853865 -2.3864853865) (end 3.375 3.375) (width 0.15))
    ))
  (pad "9" smd custom (at 0 3.375) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -3.375 -3.375) (mid 2.3864853865 -5.7614853865) (end 0 0) (width 0.15))
    ))
  (pad "10" smd custom (at -3.675 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 6.27361742086 -2.59861742086) (end 3.675 3.675) (width 0.15))
    ))
  (pad "10" smd custom (at 0 3.675) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -3.675 -3.675) (mid 2.59861742086 -6.27361742086) (end 0 0) (width 0.15))
    ))
  (pad "11" smd custom (at -3.975 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 6.78574945521 -2.81074945521) (end 3.975 3.975) (width 0.15))
    ))
  (pad "11" smd custom (at 0 3.975) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -3.975 -3.975) (mid 2.81074945521 -6.78574945521) (end 0 0) (width 0.15))
    ))
  (pad "12" smd custom (at -4.275 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 7.29788148957 -3.02288148957) (end 4.275 4.275) (width 0.15))
    ))
  (pad "12" smd custom (at 0 4.275) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -4.275 -4.275) (mid 3.02288148957 -7.29788148957) (end 0 0) (width 0.15))
    ))
)

