(footprint "BM20B(0.8)-40DP-0.4V(51)" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -1.8 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 8e640f48-2c4f-48b6-a92e-3c74f95e2e52)
  )
  (fp_text value "BM20B(0.8)-40DP-0.4V(51)" (at 0 1.95 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp 505e0b3e-d9bc-4c12-8d9f-e5587bc3dc67)
  )
  (fp_text user "${REFERENCE}" (at 0 1.55 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp 72e14f42-78eb-4042-a16d-7be6bf349f06)
  )
  (fp_rect (start -4.7 -1.45) (end -4.05 -1.3)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 41949d99-5dcc-4794-a1aa-10ec146eac1b))
  (fp_rect (start -4.7 1.3) (end -4.05 1.45)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 17eaabdc-bf41-4f6a-8cfd-5522b8da1b69))
  (fp_rect (start 4.05 -1.45) (end 4.7 -1.3)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 41b85b7f-d606-4252-8695-25f54797d129))
  (fp_rect (start 4.05 1.3) (end 4.7 1.45)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 6da09808-e924-4509-9960-47bb7c6c6354))
  (fp_arc (start -5.475 -1.3) (mid -5.453033 -1.353033) (end -5.4 -1.375)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 52cd3752-fa61-4c1b-a1c1-61f224b73dc8))
  (fp_arc (start -5.4 1.375) (mid -5.453033 1.353033) (end -5.475 1.3)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 3b7edd14-3af0-4b8e-a6f5-222934c339d1))
  (fp_arc (start 5.4 -1.375) (mid 5.453033 -1.353033) (end 5.475 -1.3)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp f5536fde-37fa-4bee-aa4a-98bd98de2d52))
  (fp_arc (start 5.475 1.3) (mid 5.453033 1.353033) (end 5.4 1.375)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp fb894cf8-f33c-4ace-9b77-e6109c158d58))
  (fp_poly
    (pts
      (xy -3.8 1.45)
      (xy -3.95 1.7)
      (xy -3.65 1.7)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 13299604-1ee0-46f2-8f52-e58354bc4a32))
  (fp_poly
    (pts
      (xy -5.3 -1.3)
      (xy -5.3 -1.45)
      (xy -5.4 -1.45)
      (xy -5.55 -1.3)
      (xy -5.55 1.3)
      (xy -5.4 1.45)
      (xy -5.3 1.45)
      (xy -5.3 1.3)
      (xy -5.4 1.3)
      (xy -5.4 -1.3)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 47f0cba1-996c-447c-ae1c-52c1ff193339))
  (fp_poly
    (pts
      (xy 5.3 1.3)
      (xy 5.3 1.45)
      (xy 5.4 1.45)
      (xy 5.55 1.3)
      (xy 5.55 -1.3)
      (xy 5.4 -1.45)
      (xy 5.3 -1.45)
      (xy 5.3 -1.3)
      (xy 5.4 -1.3)
      (xy 5.4 1.3)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp b1a43285-89b6-4c54-ae6e-c34c199b9822))
  (fp_rect (start -4 -0.685) (end 4 -0.175)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 5b06a553-9558-4daa-b99f-4b31366fe8a7))
  (fp_rect (start -4 0.175) (end 4 0.685)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 0bafe1f4-a8f1-41f7-ba4c-9f71b2c82657))
  (fp_line (start -5.4 -1.3) (end -5.4 1.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a8ce0694-402c-49a5-b126-2de8c2e77e6f))
  (fp_line (start -5.25 -1.45) (end 5.25 -1.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ab4ae608-aacc-4682-bcba-0b3dfca09dff))
  (fp_line (start 5.25 1.45) (end -5.25 1.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 77f320dd-3d25-4953-a8ac-05246f4d1ba6))
  (fp_line (start 5.4 1.3) (end 5.4 -1.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e8d396fd-fcc8-4e40-a90d-d92a88efd367))
  (fp_arc (start -5.4 -1.3) (mid -5.356066 -1.406066) (end -5.25 -1.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp de4c4e6d-d14c-4559-b237-106810d4a8db))
  (fp_arc (start -5.25 1.45) (mid -5.356066 1.406066) (end -5.4 1.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ac06f289-908a-47f0-980c-85dc1ae7a5fb))
  (fp_arc (start 5.25 -1.45) (mid 5.356066 -1.406066) (end 5.4 -1.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e942fed6-b198-4801-b975-cb78e9eea54a))
  (fp_arc (start 5.4 1.3) (mid 5.356066 1.406066) (end 5.25 1.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1a04a093-bafb-43ca-ba07-21671043b60e))
  (fp_rect (start -5.24 -1.15) (end 5.24 1.15)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 633cc340-8a30-4fb5-a2fb-aedebe56129a))
  (pad "1" smd roundrect (at -3.8 1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp 9e9802fb-bc57-432c-ba43-9f5b2e6b3a22))
  (pad "2" smd roundrect (at -3.4 1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp d9bde345-ba11-42d9-a620-5b489886e447))
  (pad "3" smd roundrect (at -3 1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp 57170d3d-a906-4767-a329-bfa3fc1818ab))
  (pad "4" smd roundrect (at -2.6 1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp e1fea70e-121c-4679-84cf-638364e4861e))
  (pad "5" smd roundrect (at -2.2 1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp fbb2ef82-4ff7-4057-9889-0130f0292643))
  (pad "6" smd roundrect (at -1.8 1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp 1ca97a94-a9e5-470f-9b19-b2372c27127a))
  (pad "7" smd roundrect (at -1.4 1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp cd80a518-222d-4244-9491-5e8a1e79751d))
  (pad "8" smd roundrect (at -1 1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp 6157984c-84eb-4a49-8ebe-9707f2e933d6))
  (pad "9" smd roundrect (at -0.6 1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp 78a6fba2-61cb-404f-80b4-e9349eb2e0fe))
  (pad "10" smd roundrect (at -0.2 1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp 8cb78465-0c1f-4985-8a4d-3b6c3f338f03))
  (pad "11" smd roundrect (at 0.2 1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp 5fbd26ad-ea78-4f87-a9f5-b7f5cd8664d2))
  (pad "12" smd roundrect (at 0.6 1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp c3dee83f-4e98-4233-a41d-b1f3dea793a1))
  (pad "13" smd roundrect (at 1 1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp da0dc8b9-8ee3-4dd7-86e5-1fd57b5eda05))
  (pad "14" smd roundrect (at 1.4 1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp fedc106e-6b34-4e79-99d9-3edec9cd18d4))
  (pad "15" smd roundrect (at 1.8 1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp ebe9dbab-a7f5-4c45-a71f-76efab2b1a23))
  (pad "16" smd roundrect (at 2.2 1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp 65b6d27a-50e5-4f72-acb4-674d49a5e043))
  (pad "17" smd roundrect (at 2.6 1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp 4835e125-7fa1-4dc0-9c21-08712fc979b4))
  (pad "18" smd roundrect (at 3 1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp f44615c3-d389-445c-8505-59ca3aba421a))
  (pad "19" smd roundrect (at 3.4 1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp 76841d6d-5169-41ce-a6d8-5ceddd539e80))
  (pad "20" smd roundrect (at 3.8 1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp 9fa6403f-5d91-4531-b81b-e6ca415ecc0f))
  (pad "21" smd roundrect (at 3.8 -1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp 286026a1-5b2a-4f6a-b45e-b285686251db))
  (pad "22" smd roundrect (at 3.4 -1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp 09577bf5-720a-4895-ad14-681a53a09fa1))
  (pad "23" smd roundrect (at 3 -1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp 1a8885e5-2646-4e22-ac52-cedb2808a4b7))
  (pad "24" smd roundrect (at 2.6 -1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp c897e230-449f-4178-9208-0ae5f1a4c24b))
  (pad "25" smd roundrect (at 2.2 -1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp 944a2aeb-342d-4a32-ad88-de80f91024a2))
  (pad "26" smd roundrect (at 1.8 -1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp ccee81b6-80a2-4281-839b-8c673947eff2))
  (pad "27" smd roundrect (at 1.4 -1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp 5ae8f29b-f922-402b-b7ff-e06109b77b51))
  (pad "28" smd roundrect (at 1 -1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp b3ed33ff-c1e6-4afb-955b-e38303d055ae))
  (pad "29" smd roundrect (at 0.6 -1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp e1af4de0-401b-42d8-8e6f-6df93383ae2a))
  (pad "30" smd roundrect (at 0.2 -1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp 72df0a2c-d636-42fb-99c0-86cb1e9f7c16))
  (pad "31" smd roundrect (at -0.2 -1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp dd2ee6b6-3a2b-4661-94f2-34dab764596d))
  (pad "32" smd roundrect (at -0.6 -1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp 3d6cc8cc-aaa3-4250-94f6-190e2cb9c52c))
  (pad "33" smd roundrect (at -1 -1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp 36dded33-e54c-4b7f-ba0b-7cede7c592ff))
  (pad "34" smd roundrect (at -1.4 -1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp 9607e781-6dad-4d0d-b81a-d292d36ddcca))
  (pad "35" smd roundrect (at -1.8 -1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp 641e4f15-7d95-40ed-95bd-cbfc5ca2f579))
  (pad "36" smd roundrect (at -2.2 -1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp e3ba1616-1de4-4365-9f92-ed428ef93b0d))
  (pad "37" smd roundrect (at -2.6 -1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp 594d4012-1df0-444e-b3d3-672e34137c9e))
  (pad "38" smd roundrect (at -3 -1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp 770eb0b1-a7c3-450a-a9a4-0e1754c6c019))
  (pad "39" smd roundrect (at -3.4 -1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp 49db63fc-411c-4627-b067-98950a60ab82))
  (pad "40" smd roundrect (at -3.8 -1.09) (size 0.23 0.42) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.145)
    (thermal_bridge_angle 45) (tstamp 263076e3-aaf2-46cb-ad4b-6c02e4a841ec))
  (pad "MP" smd roundrect (at -5.01 -0.925) (size 0.3 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1111)
    (thermal_bridge_angle 45) (tstamp 87068403-8daa-4e1a-8112-e72373964250))
  (pad "MP" smd roundrect (at -5.01 0.925) (size 0.3 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1111)
    (thermal_bridge_angle 45) (tstamp bf37e466-c081-430e-97f4-e225ad003b78))
  (pad "MP" smd roundrect (at 5.01 -0.925) (size 0.3 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1111)
    (thermal_bridge_angle 45) (tstamp 695cbbfc-3616-4ded-9aba-7689a4780120))
  (pad "MP" smd roundrect (at 5.01 0.925) (size 0.3 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1111)
    (thermal_bridge_angle 45) (tstamp 0fd9b4ab-1d3c-464e-9ac7-1728f884e57e))
)
