(module USB_A_3.0_Board_edge_connector_Mount_around (layer F.Cu) (tedit 54576F1C)
  (attr smd)
  (fp_text reference USB1 (at 0 -7) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text value USB3.0_A_Connector (at 0 -0.75) (layer Cmts.User)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_line (start -6 0) (end 6 0) (layer Dwgs.User) (width 0.127))
  (pad 1 smd rect (at 3 -5.05) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 1 -5.05) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1 -5.05) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -3 -5.05) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -4 -5.05) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -2 -5.05) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 0 -5.05) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 2 -5.05) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 4 -5.05) (size 0.7 2.3) (layers F.Cu F.Paste F.Mask))
  (pad "" np_thru_hole circle (at 2.25 -2.85) (size 1.25 1.25) (drill 1.2) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -2.25 -2.85) (size 1.25 1.25) (drill 1.2) (layers *.Cu *.Mask))
  (pad 10 smd rect (at -5.25 -2.85) (size 1 5) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 5.25 -2.85) (size 1 5) (layers F.Cu F.Paste F.Mask))
)
