(footprint "TDFN-8-1EP_3x2mm_P0.5mm_EP1.80x1.65mm" (version 20220818) (generator pcbnew)
  (layer "F.Cu")
  (descr "8-lead plastic dual flat, 2x3x0.75mm size, 0.5mm pitch (http://ww1.microchip.com/downloads/en/DeviceDoc/8L_TDFN_2x3_MN_C04-0129E-MN.pdf)")
  (tags "TDFN DFN 0.5mm")
  (property "Sheetfile" "File: AK80 Controller v1.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "CAN FD Transceiver with Silent Mode, up to 8 Mbps, TDFN-8")
  (property "ki_keywords" "CAN FD Transceiver")
  (attr smd)
  (fp_text reference "U2" (at 0 -1.88 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ffe08f8f-f841-4285-9a1d-3f18ab954b88)
  )
  (fp_text value "MCP2558FD-xMNY" (at 0 1.88 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2033b429-1cf3-4a52-a70a-084805d75a95)
  )
  (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab")
      (effects (font (size 0.6 0.6) (thickness 0.09)))
    (tstamp 41eff214-a987-4803-b26b-9a3a92ae9279)
  )
  (fp_line (start -1.45 1.12) (end 1.45 1.12)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2141a1ce-54ba-48d6-8fe8-da566c7a860a))
  (fp_line (start -0.45 -1.12) (end 1.45 -1.12)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2cd188b9-d727-4219-98fb-6ac53e176363))
  (fp_line (start -2.13 -1.25) (end -2.13 1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 475dade1-63b4-444d-a40f-e7afe352c84e))
  (fp_line (start -2.13 1.25) (end 2.13 1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 781eb565-f738-459b-a239-43871e3c2dae))
  (fp_line (start 2.13 -1.25) (end -2.13 -1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8109d98c-c4f6-4153-bf33-b09a678ed792))
  (fp_line (start 2.13 1.25) (end 2.13 -1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7187ee83-9611-486a-b752-c0c409716b6c))
  (fp_line (start -1.5 -0.5) (end -1.5 1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ecb7e51a-50e5-44f5-b900-66452a4da7f5))
  (fp_line (start -1.5 1) (end 1.5 1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2e5de82e-8cc8-4527-9ded-f156c8eec043))
  (fp_line (start -1 -1) (end -1.5 -0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ac98a32b-8be7-482e-a16a-e8c3b295b89e))
  (fp_line (start 1.5 -1) (end -1 -1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0d8876e1-f429-4284-a606-2f40d2150f1d))
  (fp_line (start 1.5 1) (end 1.5 -1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 76cd381c-1d36-408c-b837-5115bc2a0492))
  (pad "" smd rect (at 0 -0.5) (size 0.7 0.65) (layers "F.Paste") (tstamp cf5127fc-664f-448d-9784-7801a77f3d61))
  (pad "" smd rect (at 0 0) (size 1.8 0.7) (layers "F.Paste") (tstamp aee123ef-57fd-4877-afb3-09c7b343a1dc))
  (pad "" smd rect (at 0 0.5) (size 0.7 0.65) (layers "F.Paste") (tstamp c373a5c0-05e8-4544-b52a-85c0ebc16f4a))
  (pad "1" smd roundrect (at -1.5 -0.75) (size 0.78 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a4b6a274-052d-4601-9a30-f306ca798e15))
  (pad "2" smd roundrect (at -1.5 -0.25) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp bfd6ba6c-5405-4179-8f2b-1c44a7062fd5))
  (pad "3" smd roundrect (at -1.5 0.25) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ece8273c-69c4-4dbc-92f0-fc645b36500f))
  (pad "4" smd roundrect (at -1.5 0.75) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 876f201b-390c-4bb2-af22-34e07200c8fd))
  (pad "5" smd roundrect (at 1.5 0.75) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 3617bce8-eb35-498d-ae2c-5e5931dc7b76))
  (pad "6" smd roundrect (at 1.5 0.25) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d8f81f73-0b96-45fb-a475-a8b7d0d321e6))
  (pad "7" smd roundrect (at 1.5 -0.25) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5d09e2fd-4d6f-42c8-a70a-b271b0d7724f))
  (pad "8" smd roundrect (at 1.5 -0.75) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 33304c07-cd35-42a6-8c9b-5f771b400ba5))
  (pad "9" smd rect (at 0 0) (size 1.8 1.65) (layers "F.Cu" "F.Mask") (tstamp 93d13589-3d88-4066-bfe9-5c18289dbdcd))
  (model "${KICAD7_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/TDFN-8-1EP_3x2mm_P0.5mm_EP1.80x1.65mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
