(module Program_5P_1.25mm (layer F.Cu) (tedit 547E3C20)
  (solder_mask_margin 0.001)
  (attr virtual)
  (fp_text reference P2 (at -2.25 0 90) (layer Cmts.User)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text value PROG (at -1.1 0 90) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text user SIO (at 1.5 2.5) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text user CLK (at 1.5 1.25) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text user RST (at 1.5 0) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text user VCC (at 1.5 -1.25) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text user GND (at 1.75 -2.5) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (pad 1 thru_hole rect (at 0 -2.5) (size 0.75 0.75) (drill 0.425) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 0 2.5) (size 0.75 0.75) (drill 0.425) (layers *.Cu *.Mask))
  (pad 2 connect oval (at 0 -1.25) (size 0.75 0.5) (layers F.Cu F.Mask))
  (pad 3 connect oval (at 0 0) (size 0.75 0.5) (layers F.Cu F.Mask))
  (pad 4 connect oval (at 0 1.25) (size 0.75 0.5) (layers F.Cu F.Mask))
)
