(module TO-277A_AAK (layer F.Cu) (tedit 59452A56)
  (descr "Thermal enhanced ultra thin SMD package; 3 leads; body: 5.8 x 4.3 x 0.78 mm")
  (tags "TO-277A SOT-1289")
  (attr smd)
  (fp_text reference D1 (at -3 -1.75 -90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value FSV20100V (at 0 5.3 -180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0.86) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 2.25 -2.49) (end 1.9 -2.49) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.9 -2.49) (end -2.25 -2.49) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.25 -2.49) (end -2.25 -0.74) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.25 -0.74) (end 2.25 -2.49) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.15 4.11) (end 2.15 -2.39) (layer F.Fab) (width 0.05))
  (fp_line (start 2.15 -2.39) (end -2.15 -2.39) (layer F.Fab) (width 0.05))
  (fp_line (start -2.15 -2.39) (end -2.15 4.11) (layer F.Fab) (width 0.05))
  (fp_line (start -2.15 4.11) (end 2.15 4.11) (layer F.Fab) (width 0.05))
  (fp_line (start 2.61 4.55) (end -2.61 4.55) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.61 4.55) (end 2.61 -2.79) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.61 -2.79) (end -2.61 4.55) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.61 -2.79) (end 2.61 -2.79) (layer F.CrtYd) (width 0.05))
  (fp_circle (center -1.75 -1.94) (end -1.85 -1.99) (layer F.Fab) (width 0.1))
  (pad A smd roundrect (at -1.04 -1.9 180) (size 1.4 1.27) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.1))
  (pad K smd roundrect (at 0 1.9 180) (size 4.72 4.8) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.05))
  (pad A smd roundrect (at 1.04 -1.9 180) (size 1.4 1.27) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.1))
  (model ${KICAD7_3DMODEL_DIR}/TO_SOT_Packages_SMD.3dshapes/TO-277A.step
    (at (xyz 0 -0.03 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 -180))
  )
)
