(footprint "DF12NC(3.0)-80DP-0.5V(51) [Mirrored]" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at -11.975 0 90 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ebfc541b-a038-4ab1-ac73-21e27378b9bb)
  )
  (fp_text value "DF12NC(3.0)-80DP-0.5V(51) [Mirrored]" (at 0 -0.6 unlocked) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
    (tstamp f912db8c-ce39-427f-a9e9-ff33d4fe2b85)
  )
  (fp_text user "${REFERENCE}" (at 0 0.725 unlocked) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
    (tstamp e0122e43-598e-4554-8966-801a3bd521a6)
  )
  (fp_arc (start -11.275 -2) (mid -11.253033 -2.053033) (end -11.2 -2.075)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp b0f8881f-94d7-465c-b174-02c7c45d6252))
  (fp_arc (start -11.2 2.075) (mid -11.253033 2.053033) (end -11.275 2)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 57b43951-9914-4c9f-8e4f-4df77b53f8d4))
  (fp_arc (start 11.2 -2.075) (mid 11.253033 -2.053033) (end 11.275 -2)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 2ba6dfb5-27e8-4e42-b80a-993e510d5450))
  (fp_arc (start 11.275 2) (mid 11.253033 2.053033) (end 11.2 2.075)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 2b370a95-0993-43ae-a30b-28f57088a1cc))
  (fp_poly
    (pts
      (xy -9.6 3)
      (xy -9.9 3)
      (xy -9.75 2.75)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 3e5fc5b5-942b-4f23-b5c3-1c0ea927e19c))
  (fp_poly
    (pts
      (xy -10.1 -2)
      (xy -11.2 -2)
      (xy -11.2 2)
      (xy -10.1 2)
      (xy -10.1 2.15)
      (xy -11.2 2.15)
      (xy -11.35 2)
      (xy -11.35 -2)
      (xy -11.2 -2.15)
      (xy -10.1 -2.15)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 43d88476-d409-407b-8c5f-00d87159d33e))
  (fp_poly
    (pts
      (xy 10.1 2)
      (xy 11.2 2)
      (xy 11.2 -2)
      (xy 10.1 -2)
      (xy 10.1 -2.15)
      (xy 11.2 -2.15)
      (xy 11.35 -2)
      (xy 11.35 2)
      (xy 11.2 2.15)
      (xy 10.1 2.15)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp e280eee2-4f68-431f-a012-fbdaf6055bf1))
  (fp_line (start -11.35 -1.9) (end -11.35 1.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp bd6c23a9-b22a-4acc-a067-99d6f7341984))
  (fp_line (start -11.1 -2.15) (end -10.05 -2.15)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2ce949d0-3b20-484e-a8dd-830dd7d39910))
  (fp_line (start -11.1 2.15) (end -10.05 2.15)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp bc3540cd-0d00-4e12-b259-93843ab7a92c))
  (fp_line (start -10.05 -2.15) (end -10.05 -2.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5d900036-e480-4f5b-98d5-31df1d65fb48))
  (fp_line (start -10.05 2.15) (end -10.05 2.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4811ce16-1c10-49d6-a642-3bc9b86ea019))
  (fp_line (start -9.85 -2.75) (end 9.85 -2.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c19a8be5-3f99-4a46-ad25-9cd6ec763277))
  (fp_line (start 9.85 2.75) (end -9.85 2.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1b9eed98-8c55-4211-968e-3148ae208cae))
  (fp_line (start 10.05 -2.15) (end 10.05 -2.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f83db3ba-052a-4366-8059-2d5fb132c36c))
  (fp_line (start 10.05 2.15) (end 10.05 2.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 088c2a07-7e9e-42ec-aa11-b8b0d7a202a7))
  (fp_line (start 11.1 -2.15) (end 10.05 -2.15)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9d1baa65-3c89-4ac1-ad37-db81780648e8))
  (fp_line (start 11.1 2.15) (end 10.05 2.15)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 519cd55f-63ec-4a61-85d5-befa044fb5e2))
  (fp_line (start 11.35 -1.9) (end 11.35 1.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fc4946b7-b6e3-4120-b98d-fd859039dd36))
  (fp_arc (start -11.35 -1.9) (mid -11.276777 -2.076777) (end -11.1 -2.15)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 31032549-90a9-42fa-a3e3-8cf776c60ec7))
  (fp_arc (start -11.1 2.15) (mid -11.276777 2.076777) (end -11.35 1.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp bc1b5c8d-2608-4435-a1a2-8dd3d78b9cd3))
  (fp_arc (start -10.05 -2.55) (mid -9.991421 -2.691421) (end -9.85 -2.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2015ba7c-57bb-42a5-b74d-b6093b7f24e7))
  (fp_arc (start -9.85 2.75) (mid -9.991421 2.691421) (end -10.05 2.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 06b8624c-ae44-4dff-95ba-c470b026c5c9))
  (fp_arc (start 9.85 -2.75) (mid 9.991421 -2.691421) (end 10.05 -2.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4ca32d08-ceb4-46eb-ab3c-099e85a77f84))
  (fp_arc (start 10.05 2.55) (mid 9.991421 2.691421) (end 9.85 2.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ee352b44-9564-474f-9e53-3d4b7154fc39))
  (fp_arc (start 11.1 -2.15) (mid 11.276777 -2.076777) (end 11.35 -1.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8f9b8eb9-1248-4f30-be06-862e8195f1b3))
  (fp_arc (start 11.35 1.9) (mid 11.276777 2.076777) (end 11.1 2.15)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a511ba17-5bda-4b90-b4b4-522b31e0190a))
  (fp_rect (start -11.1 -1.9) (end 11.1 1.9)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 769547ae-3d43-4594-b978-c1ae549ecd3f))
  (pad "" smd oval (at -9.75 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 3fc0bf53-ba53-490e-96fe-7190ec744c21))
  (pad "" smd oval (at -9.75 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp d123e72a-57f1-4cf4-89f1-e99387662048))
  (pad "" smd oval (at -9.25 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 91fb862a-9d55-4250-bb36-7e5b1871a342))
  (pad "" smd oval (at -9.25 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp f821d15b-08f9-4487-ba50-8c617f61b819))
  (pad "" smd oval (at -8.75 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp b489c007-7fbf-4f1d-a9a4-044d6fdca044))
  (pad "" smd oval (at -8.75 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 0bc9f834-feb5-46ff-8d43-ba32197f5978))
  (pad "" smd oval (at -8.25 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 5432adf3-36f0-4f11-876b-65a945a8df74))
  (pad "" smd oval (at -8.25 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 926ff283-26bc-4051-90fd-b752f752aa1a))
  (pad "" smd oval (at -7.75 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp baeaffcb-a7e9-4429-b67b-b306f49a8f5c))
  (pad "" smd oval (at -7.75 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp b785c93c-008b-4307-974a-e94173f32768))
  (pad "" smd oval (at -7.25 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 577c42ff-c7a7-4f3e-a6f9-9d5adbe92e75))
  (pad "" smd oval (at -7.25 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 3184166c-ce2d-4a02-a079-5b6ffc0e61cd))
  (pad "" smd oval (at -6.75 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp b69b6db5-b01b-46c8-ac6a-2fa6f0660f5a))
  (pad "" smd oval (at -6.75 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 8b696bef-5e36-455c-be24-bbd04a86b31c))
  (pad "" smd oval (at -6.25 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp e492b43d-0003-4dfb-b374-ec71b16364da))
  (pad "" smd oval (at -6.25 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 9ee6778e-f1a7-4b1f-b9da-cf3a5da94c82))
  (pad "" smd oval (at -5.75 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp fe03a93a-2b01-4461-8bc9-d9a542365989))
  (pad "" smd oval (at -5.75 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 691fb3f2-8a50-42d3-87d8-d46bf890bba9))
  (pad "" smd oval (at -5.25 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 5f4a9278-77ef-45d8-8c55-dc06ea216a98))
  (pad "" smd oval (at -5.25 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 2ea6db3f-7585-47b5-9412-5ad418fe0661))
  (pad "" smd oval (at -4.75 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp e3d0dcad-585f-412b-9275-4c55c20bf84d))
  (pad "" smd oval (at -4.75 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp e1174bfb-2939-4862-a462-f1234178950b))
  (pad "" smd oval (at -4.25 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 5b9c8b98-74ef-43dd-a16e-9dc96b5d5bb0))
  (pad "" smd oval (at -4.25 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 1a32d3f3-175f-462b-a636-3fac4ba14cb4))
  (pad "" smd oval (at -3.75 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp e2527a45-a5dc-4e66-bc0b-aa4c9ddde52e))
  (pad "" smd oval (at -3.75 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 63ee566a-b57d-493f-96ad-8129a2c54c31))
  (pad "" smd oval (at -3.25 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp a7305ee2-33b5-432f-bcb4-c376e2fa6996))
  (pad "" smd oval (at -3.25 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp b9b01579-268e-46a2-a5d0-63cc020f0903))
  (pad "" smd oval (at -2.75 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp a6ddcb71-7d5c-4b76-9a77-f366e0675c85))
  (pad "" smd oval (at -2.75 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 2165586c-7705-4f10-8d78-3297e785d320))
  (pad "" smd oval (at -2.25 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 0f6ecf64-0a2d-4782-b904-31cb49525560))
  (pad "" smd oval (at -2.25 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp d15e312f-4e3d-4209-b771-ce418d6e4028))
  (pad "" smd oval (at -1.75 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp caba2a7b-ed08-4d86-9041-68cd2c1c0abf))
  (pad "" smd oval (at -1.75 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp e520a530-0afb-44b1-9ada-325eff585598))
  (pad "" smd oval (at -1.25 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp f3c7613b-1d55-48f1-96ab-d228a322320d))
  (pad "" smd oval (at -1.25 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp f5ea726e-262f-4647-baf4-baf80ccc85fb))
  (pad "" smd oval (at -0.75 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 25195986-b5ea-4f4e-af77-1c8f44f14d50))
  (pad "" smd oval (at -0.75 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp f81bf020-997b-4b15-a600-80a6f268d306))
  (pad "" smd oval (at -0.25 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 14433d57-bfb5-46fe-880f-cfde5983d08a))
  (pad "" smd oval (at -0.25 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 7afdfe69-e676-4604-9b3d-e08c128873b0))
  (pad "" smd oval (at 0.25 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 3053ed3b-e921-4049-a447-0c1203954e49))
  (pad "" smd oval (at 0.25 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 82f2f2b0-c40a-40ce-8fc8-dbc1dbe597cf))
  (pad "" smd oval (at 0.75 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp d9f9ed8c-03fb-474e-b43e-d06c40065973))
  (pad "" smd oval (at 0.75 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 1df6e7fe-6bda-45e5-acc8-328a95b644f4))
  (pad "" smd oval (at 1.25 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp e019471a-4217-4d3a-80c5-c6e9345b13ac))
  (pad "" smd oval (at 1.25 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 441dc132-c01f-44b7-9c0d-2110fc908197))
  (pad "" smd oval (at 1.75 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 0cd6b830-918b-40ed-a93f-01d18fb70a5b))
  (pad "" smd oval (at 1.75 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 9d42890d-5fba-47b7-9fd4-e2be7fdbf8a0))
  (pad "" smd oval (at 2.25 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 1a7e8eb4-8326-4169-a979-c301ad12c221))
  (pad "" smd oval (at 2.25 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 7ae5f664-1c3f-455a-bcd1-b674cc4ce8a8))
  (pad "" smd oval (at 2.75 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 10144631-f5c7-4d18-a472-4149644ea392))
  (pad "" smd oval (at 2.75 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp b3b7a660-7eaf-4c5a-bb5f-2c743ac1fb60))
  (pad "" smd oval (at 3.25 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 3f8c8a18-0067-4580-8a1f-a0125031083c))
  (pad "" smd oval (at 3.25 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 4db1b7cf-7153-4410-a564-5e9ee64cf3c9))
  (pad "" smd oval (at 3.75 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 03ca623f-2570-4959-b862-0dba776dd1dc))
  (pad "" smd oval (at 3.75 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp cae118de-626b-4157-9ebf-69ec79174aa4))
  (pad "" smd oval (at 4.25 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp caf6c830-b7a9-45bd-b646-81272acf8bc7))
  (pad "" smd oval (at 4.25 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp e6b64cea-c4be-451c-93a0-555991d58314))
  (pad "" smd oval (at 4.75 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 93e7e230-24bc-4d30-b6b4-be74a2fc99c1))
  (pad "" smd oval (at 4.75 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 4414683d-028a-40ad-8d8b-f017cc34315c))
  (pad "" smd oval (at 5.25 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp b8669ad4-2aa6-468e-8f8f-33d0376c4a8f))
  (pad "" smd oval (at 5.25 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 598eb127-0a3e-495d-923c-48aabc475693))
  (pad "" smd oval (at 5.75 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 936534ce-e73e-425b-8cf7-e0015eaef29d))
  (pad "" smd oval (at 5.75 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp b5db78b0-1af9-4e9d-8cd9-0d13608d715a))
  (pad "" smd oval (at 6.25 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp e7aeb04d-4fb5-4fd6-858d-cdf3bebfa2e7))
  (pad "" smd oval (at 6.25 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 6d8ef67f-fd83-4b77-b202-1339fa748b01))
  (pad "" smd oval (at 6.75 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 2d5a463d-a0c2-4542-b671-6f840c49d9f1))
  (pad "" smd oval (at 6.75 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp db7b0c64-fb0c-4474-9390-ecd573055f18))
  (pad "" smd oval (at 7.25 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 6ba7f6ef-cbb7-4708-a398-77c038796e69))
  (pad "" smd oval (at 7.25 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 853a7569-987e-4772-bdde-eee223b08c85))
  (pad "" smd oval (at 7.75 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 8a8d14db-0af7-429a-8e08-cf07598f630a))
  (pad "" smd oval (at 7.75 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 8ea53856-1f4c-43f4-9cd6-720ebe2d223d))
  (pad "" smd oval (at 8.25 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp c3bec99f-e989-4784-bf78-0850c0433fb3))
  (pad "" smd oval (at 8.25 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 426a6325-998c-4c18-802f-19a174c3c961))
  (pad "" smd oval (at 8.75 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 5d1c301c-69a7-45a1-b273-12b0e6d6d171))
  (pad "" smd oval (at 8.75 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp a4c7f1f1-fde3-4e47-a20a-abf75b83e665))
  (pad "" smd oval (at 9.25 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 1d1c9a70-8eea-4a78-b8db-6d4f29e56221))
  (pad "" smd oval (at 9.25 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp c67a1c37-3a66-44fb-89bd-1d45bd68420f))
  (pad "" smd oval (at 9.75 -2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 287e6e4f-047b-4d06-a9a2-6c2c6f54bbca))
  (pad "" smd oval (at 9.75 2) (size 0.28 0.8) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 01b90dfd-104f-4cd9-96ed-98c6951874b7))
  (pad "1" smd roundrect (at -9.75 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp fe4873cd-b5aa-4d74-b489-616f55bffba7))
  (pad "2" smd roundrect (at -9.75 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 8b54d475-daa3-4db9-b250-f9780c63a76b))
  (pad "3" smd roundrect (at -9.25 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp a10372e2-f8ce-4e5f-b279-b4fe63f25028))
  (pad "4" smd roundrect (at -9.25 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 5c4d99a7-3438-4ce5-804f-45f2adb72ec9))
  (pad "5" smd roundrect (at -8.75 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp c0bb6e9f-a51f-4f78-a750-7f73eaa8608d))
  (pad "6" smd roundrect (at -8.75 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 6c683fa7-aab8-471f-932e-68d0d7de13ba))
  (pad "7" smd roundrect (at -8.25 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp e0d374a4-418a-4195-9e99-6f7df57a21fd))
  (pad "8" smd roundrect (at -8.25 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp a6e9d606-1cf1-4ae2-a608-450429998690))
  (pad "9" smd roundrect (at -7.75 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 806f57de-ec06-46c3-9e18-9ab0040fce32))
  (pad "10" smd roundrect (at -7.75 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 5e8aaee1-8215-47d2-b7a6-42ce210b40e9))
  (pad "11" smd roundrect (at -7.25 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 069cea94-bcf9-49e3-a094-3a35d050e26f))
  (pad "12" smd roundrect (at -7.25 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 051c555a-8d1a-4338-b34c-a57b05d821e7))
  (pad "13" smd roundrect (at -6.75 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp c484427b-f525-4bb7-b9ef-2b8a0dca3672))
  (pad "14" smd roundrect (at -6.75 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 254452ce-e595-4f74-9598-34d08bcdae7b))
  (pad "15" smd roundrect (at -6.25 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 9d68de50-8335-4120-891a-ddb7676a452b))
  (pad "16" smd roundrect (at -6.25 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 2acb7096-882c-42ac-86be-f11e21587fe8))
  (pad "17" smd roundrect (at -5.75 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp fda3ef1b-680e-459e-8fdb-cae96ec81e5f))
  (pad "18" smd roundrect (at -5.75 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 6bc61ae3-265c-4e7f-9ca0-aaa6f843f5f1))
  (pad "19" smd roundrect (at -5.25 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 12a98761-a236-4fb6-83b3-c32f7c875017))
  (pad "20" smd roundrect (at -5.25 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 9aa01d4e-5bdb-4223-8759-1c6bed92a2a0))
  (pad "21" smd roundrect (at -4.75 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 0121be2a-d95f-4bf8-ae5a-f7fe39f2288a))
  (pad "22" smd roundrect (at -4.75 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 9c4a8605-ca2d-4a83-b0bd-c07b622e0bed))
  (pad "23" smd roundrect (at -4.25 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 51fec22d-06a0-4902-ba1c-89ffbe1780fe))
  (pad "24" smd roundrect (at -4.25 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp b8111ca6-3cbc-4194-ab24-611adcd0e309))
  (pad "25" smd roundrect (at -3.75 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp ca093f25-a6c9-47e2-bfd4-cccd9cdf6c1f))
  (pad "26" smd roundrect (at -3.75 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 299153b6-92f2-480e-afe2-f0cd8bdae5b0))
  (pad "27" smd roundrect (at -3.25 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 65b9a284-2ae0-41ba-a1ea-77fadcb116eb))
  (pad "28" smd roundrect (at -3.25 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 467b1c22-7470-4b70-8098-499dcc628629))
  (pad "29" smd roundrect (at -2.75 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 896ee80f-ff28-4c1d-b737-55f92d378e93))
  (pad "30" smd roundrect (at -2.75 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 6a6e616c-522c-4296-88d6-a480b81f9189))
  (pad "31" smd roundrect (at -2.25 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 78ce2f92-a390-4dae-af75-b6359087a78d))
  (pad "32" smd roundrect (at -2.25 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 7d562e41-c951-4197-85ce-b6452ef57f4f))
  (pad "33" smd roundrect (at -1.75 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 545786f6-3973-4af2-86a1-a446cd5b8ef1))
  (pad "34" smd roundrect (at -1.75 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 3f47f70d-bfd6-4186-bdf2-dd2ffd722ce4))
  (pad "35" smd roundrect (at -1.25 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp c3ce2fe5-1a96-4cbc-b15c-ca0bd7c59578))
  (pad "36" smd roundrect (at -1.25 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp dd741aee-b046-4d98-baaf-1ea0df98cc75))
  (pad "37" smd roundrect (at -0.75 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 4b284012-dbba-4903-bdb7-f3d450c610e7))
  (pad "38" smd roundrect (at -0.75 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp cfccbaa1-6ace-4ae3-bbe1-bbc4292c8586))
  (pad "39" smd roundrect (at -0.25 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 8c01cdd6-a856-416a-a5e5-5330cf5385b1))
  (pad "40" smd roundrect (at -0.25 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp b6787e09-1c27-4a3c-9b3d-13b9a293e0a4))
  (pad "41" smd roundrect (at 0.25 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 97ae875e-77bc-4a86-9ad6-a0ad63970cb7))
  (pad "42" smd roundrect (at 0.25 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 69ba1218-9e3e-40c2-b296-6248ffc8dd1c))
  (pad "43" smd roundrect (at 0.75 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 724abbe0-e25d-4019-a38f-e155ce6ec436))
  (pad "44" smd roundrect (at 0.75 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 92556cad-7863-4040-aa49-3b6ae529c22a))
  (pad "45" smd roundrect (at 1.25 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp f9ef23e1-8fdd-4a61-8294-0662199b8ad2))
  (pad "46" smd roundrect (at 1.25 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp bfaa40dc-849e-4b97-bfd8-f0e8e15687ec))
  (pad "47" smd roundrect (at 1.75 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 724e4cb0-04d6-4512-9630-cd35405a2a7d))
  (pad "48" smd roundrect (at 1.75 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp c1d97d96-cfff-4215-940f-da19629e7d1d))
  (pad "49" smd roundrect (at 2.25 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp e66772f1-200f-4cd3-bda7-c5a6fe9131cb))
  (pad "50" smd roundrect (at 2.25 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 0afa889a-933a-4815-b2c3-474f1269ae2c))
  (pad "51" smd roundrect (at 2.75 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 5b8f741a-f414-442e-bcf5-5722f1f434f4))
  (pad "52" smd roundrect (at 2.75 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 548927f4-258e-419b-841c-f0901d474275))
  (pad "53" smd roundrect (at 3.25 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 287af27d-d303-4589-b515-77653c2fee08))
  (pad "54" smd roundrect (at 3.25 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 7b724c47-6dd1-4233-bdb6-606687ba2c27))
  (pad "55" smd roundrect (at 3.75 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 1c16c700-f59c-4b81-bae0-178775e96eb6))
  (pad "56" smd roundrect (at 3.75 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 43eee42a-e5e3-405b-8426-8a71d893f3e4))
  (pad "57" smd roundrect (at 4.25 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 72f51b15-b79b-4c9d-af48-40a50af822c0))
  (pad "58" smd roundrect (at 4.25 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 14695095-a479-4287-b07a-ae3cb3f869eb))
  (pad "59" smd roundrect (at 4.75 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp eaa66a37-3ba9-430d-b517-93f3d45588b3))
  (pad "60" smd roundrect (at 4.75 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 82d377dd-7dda-4f1d-bd03-dfb2f22367c6))
  (pad "61" smd roundrect (at 5.25 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 4ff3c196-91b7-4503-909c-0ee0e768389e))
  (pad "62" smd roundrect (at 5.25 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp f0cba461-8879-432e-bf8d-6665839c4222))
  (pad "63" smd roundrect (at 5.75 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp c42955ba-efda-4bc2-8b99-27e6cf73853a))
  (pad "64" smd roundrect (at 5.75 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 9ff13dd3-a828-4a18-aa3a-7a12d0b42b3b))
  (pad "65" smd roundrect (at 6.25 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp abb55428-0617-4814-a823-b014ba008d81))
  (pad "66" smd roundrect (at 6.25 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 7972c08f-6461-4332-930c-2cff50135b83))
  (pad "67" smd roundrect (at 6.75 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp f41f1a9a-f5b2-4f7d-93bc-ff1fd5c5e9ef))
  (pad "68" smd roundrect (at 6.75 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 9f987404-17a4-40b9-bd31-a0b44398f7e5))
  (pad "69" smd roundrect (at 7.25 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp e6428397-bffb-40f3-9f50-79ff74acf945))
  (pad "70" smd roundrect (at 7.25 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp a2200a48-c9ee-4577-bfa7-ae86869fe115))
  (pad "71" smd roundrect (at 7.75 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 4cf555f7-d03e-4a2a-a2cd-d097cbbe3984))
  (pad "72" smd roundrect (at 7.75 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp d0a42b2d-d839-44f3-92d9-920ef4543d75))
  (pad "73" smd roundrect (at 8.25 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp ccfabf77-046a-4300-81ae-b80f7a3d981e))
  (pad "74" smd roundrect (at 8.25 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp c1fef6db-3990-4d64-95be-e9af24b6faff))
  (pad "75" smd roundrect (at 8.75 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 88a769f4-1a54-41ca-bfad-9d798ed4fe0f))
  (pad "76" smd roundrect (at 8.75 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 58598a02-1b52-4211-a3f3-753db825670b))
  (pad "77" smd roundrect (at 9.25 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 1cbd2f49-bba9-41d5-bf56-4deb053ec30a))
  (pad "78" smd roundrect (at 9.25 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 56a0d5a7-059f-4fd6-8d87-19cc9ec2939f))
  (pad "79" smd roundrect (at 9.75 2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp e8a5b9fc-1bc7-4c77-af41-9638fa629a5e))
  (pad "80" smd roundrect (at 9.75 -2) (size 0.28 1.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 41031c97-8cc1-4e8f-9efb-fe5c3311f740))
  (model ":KICAD6_3DMODEL_DIR:Connector_Hirose.3dshapes/DF12NC(3.0)-80DP.stp"
    (offset (xyz -11.1 -1.9 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
