(footprint "microSD_Molex_0475710001" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Sheetfile" "QuadCameraCarrier.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Micro SD Card Socket")
  (property "ki_keywords" "connector SD microsd")
  (solder_mask_margin 0.02)
  (solder_paste_margin -0.02)
  (attr smd)
  (fp_text reference "J25" (at 0 -0.55) (layer "F.SilkS") hide
      (effects (font (size 0.6 0.6) (thickness 0.125)))
    (tstamp e88906c8-d9b5-4dee-a7f7-18541c340343)
  )
  (fp_text value "Micro_SD_Card_Det" (at 0 0.25) (layer "F.Fab")
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    (tstamp 4a5e7f43-327d-4df8-be06-cf03e38726db)
  )
  (fp_line (start -5.35 0.85) (end -5.35 1.55)
    (stroke (width 0.125) (type solid)) (layer "F.SilkS") (tstamp 89d73704-7baf-4321-bb58-69fb5f217b7c))
  (fp_line (start -5.35 3.15) (end -5.35 4.15)
    (stroke (width 0.125) (type solid)) (layer "F.SilkS") (tstamp a234b788-0e56-4ea3-81fc-87ea732345ef))
  (fp_line (start -4.55 0.85) (end -5.35 0.85)
    (stroke (width 0.125) (type solid)) (layer "F.SilkS") (tstamp fe9e4b19-cf09-4b10-8ddc-e70be129eafb))
  (fp_line (start -4.15 5.45) (end 4.6 5.45)
    (stroke (width 0.125) (type solid)) (layer "F.SilkS") (tstamp 716e8aa7-f1a9-44b1-b9b6-9c538ae6669a))
  (fp_line (start 5.95 0.85) (end 4.35 0.85)
    (stroke (width 0.125) (type solid)) (layer "F.SilkS") (tstamp d4c27fa9-ceec-409f-83d0-a42c83d53c11))
  (fp_line (start 5.95 2.05) (end 5.95 0.85)
    (stroke (width 0.125) (type solid)) (layer "F.SilkS") (tstamp bdb6ea50-7b2e-4315-8739-360526c41668))
  (fp_line (start 6 4.55) (end 6 4.4)
    (stroke (width 0.125) (type solid)) (layer "F.SilkS") (tstamp f8898c56-3e67-4921-976b-a58849c7dc47))
  (fp_line (start -5.65 5.45) (end -5.65 1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3b72bef7-2111-44e0-931b-f9db94ea6bce))
  (fp_line (start -5.6 0.85) (end -5.6 1.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1f3fde04-94f2-44e0-ac4e-8f97e0053dc7))
  (fp_line (start -5.35 0.6) (end 5.95 0.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 89030c3d-c9d3-41c9-aff3-3746f2f5aa72))
  (fp_line (start 6.1 5.7) (end -5.4 5.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c087c1ba-964d-4b7d-9e1e-a8bba9e00176))
  (fp_line (start 6.2 0.85) (end 6.200335 2.071018)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 177999c2-35e0-4f3b-8c06-2dfeb05444fa))
  (fp_line (start 6.35 5.45) (end 6.35 2.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 133e1786-4c5d-4d62-9736-302814d79813))
  (fp_arc (start -5.65 1.85) (mid -5.637171 1.770943) (end -5.6 1.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp feac8439-6491-4014-948a-7afdf2a8297f))
  (fp_arc (start -5.6 0.85) (mid -5.526777 0.673223) (end -5.35 0.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 989d7b38-75a0-4d2c-a8dd-ac2cef211fc8))
  (fp_arc (start -5.4 5.7) (mid -5.576777 5.626777) (end -5.65 5.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8d149762-3855-4608-b674-6bc188cb9e4f))
  (fp_arc (start 5.95 0.6) (mid 6.126777 0.673223) (end 6.2 0.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0bdf0a4c-2a76-4922-bed6-06cdc79a8e17))
  (fp_arc (start 6.200335 2.071018) (mid 6.309265 2.163223) (end 6.35 2.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 965d570d-0918-48e6-843a-980cdaf8760c))
  (fp_arc (start 6.35 5.45) (mid 6.276777 5.626777) (end 6.1 5.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b7f3ec10-97c3-4992-b50f-1187519657c6))
  (fp_line (start -4.8 0) (end 6.2 0)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp f363368e-27fa-4e68-9133-f9bf6ade7b36))
  (fp_line (start -4.8 5.45) (end 6.2 5.45)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 0ed23c29-bda1-4e83-95a2-c29d1e47a367))
  (fp_line (start -4.8 15.15) (end -4.8 0)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 7854a1f5-bedd-431e-9d58-649ed9a9867c))
  (fp_line (start -4.8 15.15) (end 6.2 15.15)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp cdcda99f-06eb-46ce-bc61-08a9dafa3e47))
  (fp_line (start 6.2 0) (end 6.2 15.15)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 1e5f6dd1-1622-4244-9bdb-b20948255bab))
  (pad "1" smd roundrect (at 3.85 1.31) (size 0.7 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1) (tstamp 764c2761-1a3c-496b-b906-c6eeb3f79f1e))
  (pad "2" smd roundrect (at 2.75 1.31) (size 0.7 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1) (tstamp a9a540a5-310f-4407-9e01-3af7208dd3d2))
  (pad "3" smd roundrect (at 1.65 1.31) (size 0.7 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1) (tstamp 82bb97a9-89db-492b-954f-48d78be5b7d1))
  (pad "4" smd roundrect (at 0.55 1.31) (size 0.7 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1) (tstamp 10a05b55-385f-4fa4-b9fc-bb5c4cdaa8a7))
  (pad "5" smd roundrect (at -0.55 1.31) (size 0.7 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1) (tstamp fc0a71ee-c135-46f7-b09e-42ad525d2918))
  (pad "6" smd roundrect (at -1.65 1.31) (size 0.7 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1) (tstamp 9e7a08ee-1b3b-40e7-b6da-65e9b4c9bbef))
  (pad "7" smd roundrect (at -2.75 1.31) (size 0.7 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1) (tstamp a59c18c5-33f5-492d-aa42-1e2fff68946d))
  (pad "8" smd roundrect (at -3.85 1.31) (size 0.7 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1) (tstamp cdaf16fc-81a3-43c1-9d0b-d286c51d48e5))
  (pad "G1" smd roundrect (at -4.925 2.36) (size 1.15 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1) (tstamp 2d5e8a94-aad8-4a4d-a389-7c94d030f9d5))
  (pad "G2" smd roundrect (at -4.925 4.95) (size 1.15 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1) (tstamp ad9babc9-bd7f-49d4-a5d8-dc687456ef63))
  (pad "G3" smd roundrect (at 5.475 2.8) (size 1.45 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1) (tstamp 059c5338-d36a-4c89-82ed-8fccead2e8dc))
  (pad "G4" smd roundrect (at 5.7 3.95) (size 1 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1) (tstamp 14c647cf-f702-4e6f-a6ff-e50ab23e1bc2))
  (pad "G5" smd roundrect (at 5.5 5.1) (size 1.4 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1) (tstamp 386a70a2-2d23-4315-b019-3eaecfb915f9))
  (model "${KICAD7_3DMODEL_DIR}/Connector_Card.3dshapes/Molex_475710001.stp"
    (offset (xyz 0 -3.149999953 1.089999984))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 180))
  )
  (model "${KICAD7_3DMODEL_DIR}/Connector_Card.3dshapes/Molex_475710001_card.step"
    (offset (xyz 0 -3.149999953 1.089999984))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 180))
  )
)
