(footprint "R_Array_Convex_16P8" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "SMT resistor net, Bourns CAT16 series, 8 way")
  (tags "SMT resistor net Bourns CAT16 series 8 way")
  (property "LCSC" "C422182")
  (property "MFG" "UNI-ROYAL")
  (property "MPN" "16P8WGF330JT4E")
  (property "Sheetfile" "QuadCameraCarrier.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "8 resistor network, parallel topology")
  (property "ki_keywords" "R network parallel topology isolated")
  (attr smd)
  (fp_text reference "RN1" (at 0 -2.9 180) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 780c1e0e-7f40-4c16-98be-ae9a21bf5462)
  )
  (fp_text value "33" (at 0 1.75 180) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05) bold))
    (tstamp ae96efe9-00b0-42ee-9694-3422b5381b33)
  )
  (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05) bold))
    (tstamp 71e1c491-83f2-4f8c-98bf-8883235115de)
  )
  (fp_rect (start -1.05 -2.3) (end 1.05 -2.15)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 694e466d-05a6-414d-94c6-fbdedd1ed5bb))
  (fp_rect (start -1.05 2.15) (end 1.05 2.3)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp ec535efb-4417-4bc2-aa8d-dccea4c6608e))
  (fp_line (start -1.2 -2.05) (end -1.2 2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4ff445f3-5a8d-40c7-9b6f-5aabe7690bf2))
  (fp_line (start -0.95 -2.3) (end 0.95 -2.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 51ee3fc8-d762-47b9-a65c-3fc1fd236570))
  (fp_line (start 0.95 2.3) (end -0.95 2.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a825d733-c1d1-43ce-9123-6057fb28e53d))
  (fp_line (start 1.2 2.05) (end 1.2 -2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f0c5e38a-236e-498f-b1ce-85aee0ba294c))
  (fp_arc (start -1.2 -2.05) (mid -1.126777 -2.226777) (end -0.95 -2.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 812d6b1d-2ad9-423a-96fe-92c6d484b49a))
  (fp_arc (start -0.95 2.3) (mid -1.126777 2.226777) (end -1.2 2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ce845a71-e103-4c5a-a498-07f12888496b))
  (fp_arc (start 0.95 -2.3) (mid 1.126777 -2.226777) (end 1.2 -2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d69a3e93-7454-4e4a-be29-d175748852c7))
  (fp_arc (start 1.2 2.05) (mid 1.126777 2.226777) (end 0.95 2.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8bd7a7e5-797c-4fec-8e66-94dade6cca24))
  (fp_line (start -0.8 -2) (end 0.8 -2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b5e75cc1-fb5c-4c22-8fd5-9f50861cd3b3))
  (fp_line (start -0.8 2) (end -0.8 -2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 235d8ffa-4bea-48bb-8416-aaae7fb5251b))
  (fp_line (start 0.8 -2) (end 0.8 2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 588763b6-50b6-4548-9444-dc710274b619))
  (fp_line (start 0.8 2) (end -0.8 2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 377acd60-d344-41bd-a352-eeb9d62ca7b5))
  (pad "" smd oval (at -0.7 -1.8) (size 0.6 0.375) (layers "F.Paste") (tstamp 4c91c2ec-d8f2-4c51-8b36-0e880b1fc150))
  (pad "" smd oval (at -0.7 -1.25) (size 0.6 0.25) (layers "F.Paste") (tstamp 0b7048f1-0118-454d-aeca-90c1fea95f85))
  (pad "" smd oval (at -0.7 -0.75) (size 0.6 0.25) (layers "F.Paste") (tstamp 726a9761-a7bc-4f30-a901-d94ee4f2b569))
  (pad "" smd oval (at -0.7 -0.25) (size 0.6 0.25) (layers "F.Paste") (tstamp 92226fc2-5f11-402a-a861-e4964b42b070))
  (pad "" smd oval (at -0.7 0.25) (size 0.6 0.25) (layers "F.Paste") (tstamp c3a5c3ee-fb41-4e52-b285-b4d529df035b))
  (pad "" smd oval (at -0.7 0.75) (size 0.6 0.25) (layers "F.Paste") (tstamp 2b5a012c-c121-4f76-92cc-8458916e5d36))
  (pad "" smd oval (at -0.7 1.25) (size 0.6 0.25) (layers "F.Paste") (tstamp 797f87dd-88f1-47c7-b8ce-7ceb1398e543))
  (pad "" smd oval (at -0.7 1.8) (size 0.6 0.375) (layers "F.Paste") (tstamp b25e0be9-faf2-4493-9fec-750502607555))
  (pad "" smd oval (at 0.7 -1.8) (size 0.6 0.375) (layers "F.Paste") (tstamp 4270633e-e2ab-423e-9b87-e9f41d9572de))
  (pad "" smd oval (at 0.7 -1.25) (size 0.6 0.25) (layers "F.Paste") (tstamp a80762d9-81e5-4ed3-939e-24dca9f5fd47))
  (pad "" smd oval (at 0.7 -0.75) (size 0.6 0.25) (layers "F.Paste") (tstamp 14a1d7dc-a499-4310-8418-08d63e888103))
  (pad "" smd oval (at 0.7 -0.25) (size 0.6 0.25) (layers "F.Paste") (tstamp 75f5b160-d870-4760-983d-6f4f1ce9cca5))
  (pad "" smd oval (at 0.7 0.25) (size 0.6 0.25) (layers "F.Paste") (tstamp d8a926f3-59c1-49ec-a379-4c91a9b2c838))
  (pad "" smd oval (at 0.7 0.75) (size 0.6 0.25) (layers "F.Paste") (tstamp 2bf0081c-6c54-4667-94e9-e1056af85187))
  (pad "" smd oval (at 0.7 1.25) (size 0.6 0.25) (layers "F.Paste") (tstamp 53841402-75ba-4dd0-ad44-a6449c2328a7))
  (pad "" smd oval (at 0.7 1.8) (size 0.6 0.375) (layers "F.Paste") (tstamp 5f0d923e-c820-4d8d-8e88-236240da204e))
  (pad "1" smd roundrect (at -0.7 -1.8) (size 0.7 0.45) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2)
    (chamfer_ratio 0.08) (chamfer top_right bottom_right) (tstamp 7d43a961-f148-42d8-a1b3-f657d48358c3))
  (pad "2" smd roundrect (at -0.7 -1.25) (size 0.7 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp 12abe167-a9e8-49b5-b4ed-146fd5c5ae9f))
  (pad "3" smd roundrect (at -0.7 -0.75) (size 0.7 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp 85b76fac-efa7-489d-85ce-4348ef22acdc))
  (pad "4" smd roundrect (at -0.7 -0.25) (size 0.7 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp 13c42dde-6b78-45e6-bf4b-5c4220e1aa8f))
  (pad "5" smd roundrect (at -0.7 0.25) (size 0.7 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp 86b45037-fc2b-4103-9615-5c1f54012fac))
  (pad "6" smd roundrect (at -0.7 0.75) (size 0.7 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp 007f03b2-4e24-471f-9dae-f27f6a352936))
  (pad "7" smd roundrect (at -0.7 1.25) (size 0.7 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp c9f3abae-2901-4d29-96f7-61ed0e0f7baa))
  (pad "8" smd roundrect (at -0.7 1.8) (size 0.7 0.45) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2)
    (chamfer_ratio 0.08) (chamfer top_right bottom_right) (tstamp 8a432a21-d689-4aec-aeec-b38ef1682958))
  (pad "9" smd roundrect (at 0.7 1.8 180) (size 0.7 0.45) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2)
    (chamfer_ratio 0.08) (chamfer top_right bottom_right) (tstamp db9d4bb9-f485-4ba4-9216-b21f313095ef))
  (pad "10" smd roundrect (at 0.7 1.25 180) (size 0.7 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp c6998a08-fb2e-4c5e-8a08-d7059684bce0))
  (pad "11" smd roundrect (at 0.7 0.75 180) (size 0.7 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp df0b9bd9-835c-4725-a569-bd94ee9cdc51))
  (pad "12" smd roundrect (at 0.7 0.25 180) (size 0.7 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp 74f39b01-0f80-4a63-a09b-07f77c905718))
  (pad "13" smd roundrect (at 0.7 -0.25 180) (size 0.7 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp c2abfd9a-4e1b-4684-b8d5-b68b1b444928))
  (pad "14" smd roundrect (at 0.7 -0.75 180) (size 0.7 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp 893b1654-5560-4ae7-aab7-855971a0878e))
  (pad "15" smd roundrect (at 0.7 -1.25 180) (size 0.7 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp 0636d696-3a1d-4695-8466-ebcbb1ca8fe5))
  (pad "16" smd roundrect (at 0.7 -1.8 180) (size 0.7 0.45) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2)
    (chamfer_ratio 0.08) (chamfer top_right bottom_right) (tstamp 68083c98-8b8c-4c9a-a69f-ed3280541ea6))
  (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_8x0602.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
