(module Program_Pogo_8P (layer F.Cu) (tedit 56478199)
  (solder_mask_margin -0.02)
  (attr virtual)
  (fp_text reference REF** (at -4.2 0 90) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value Program_Pogo_8P (at 0 -1.2) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (pad 1 thru_hole rect (at -3.4 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask))
  (pad 2 thru_hole circle (at 2.4 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask))
  (pad 3 connect oval (at -2.5 0) (size 0.8 1.2) (layers F.Cu F.Mask))
  (pad 4 connect oval (at -1.5 0) (size 0.8 1.2) (layers F.Cu F.Mask))
  (pad 5 connect oval (at -0.5 0) (size 0.8 1.2) (layers F.Cu F.Mask))
  (pad 6 connect oval (at 0.5 0) (size 0.8 1.2) (layers F.Cu F.Mask))
  (pad 7 connect oval (at 1.5 0) (size 0.8 1.2) (layers F.Cu F.Mask))
  (pad 8 connect oval (at 3.3 0) (size 0.8 1.2) (layers F.Cu F.Mask))
)
