(footprint "1608_B" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (tags "0603 1608")
  (solder_mask_margin 0.025)
  (solder_paste_margin -0.001)
  (attr smd)
  (fp_text reference "R2" (at 1.3 0 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)) (justify left))
    (tstamp 26adbce3-a190-4dc8-82ee-bc33e41788d1)
  )
  (fp_text value "680" (at 1.3 0.6 unlocked) (layer "F.Fab")
      (effects (font (size 0.2 0.2) (thickness 0.05)) (justify left))
    (tstamp 6aa9a588-2565-4d28-9a14-11dc023d84e8)
  )
  (fp_poly
    (pts
      (xy 0.3 -0.425)
      (xy -0.3 -0.425)
      (xy -0.3 -0.575)
      (xy 0.3 -0.575)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 0e4aefd0-4dbd-44a7-926a-963f222c6651))
  (fp_poly
    (pts
      (xy 0.3 0.575)
      (xy -0.3 0.575)
      (xy -0.3 0.425)
      (xy 0.3 0.425)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 91440c85-7e39-4275-8c7c-187dc9e012be))
  (fp_line (start -1.2 0.275) (end -1.2 -0.275)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 32e63e65-e567-4324-8e85-629835674bd0))
  (fp_line (start -0.9 0.575) (end 0.9 0.575)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7b4194cc-09c6-4fdb-9428-bd2c6b3c38b1))
  (fp_line (start 0.9 -0.575) (end -0.9 -0.575)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c3ee9be0-4664-4d41-9b1f-39a0cd7aabed))
  (fp_line (start 1.2 -0.275) (end 1.2 0.275)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7d56a939-fc5e-4678-b583-e270b6f7c153))
  (fp_arc (start -1.2 -0.275) (mid -1.112132 -0.487132) (end -0.9 -0.575)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fd19fc82-3c01-4e28-ba6e-d5c54ddeba8d))
  (fp_arc (start -0.9 0.575) (mid -1.112132 0.487132) (end -1.2 0.275)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 66fbcc99-b8ae-4c20-8313-48a0c3c6e4e8))
  (fp_arc (start 0.9 -0.575) (mid 1.112132 -0.487132) (end 1.2 -0.275)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ebdda74e-ddf0-400b-b92e-4687e0cbc84a))
  (fp_arc (start 1.2 0.275) (mid 1.112132 0.487132) (end 0.9 0.575)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a5702c6b-73dd-46d2-9dfa-9e18c0fc48af))
  (fp_line (start -0.8 -0.4) (end 0.8 -0.4)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp f55fc466-c3f7-47bd-932e-db1659b7ca1b))
  (fp_line (start -0.8 0.4) (end -0.8 -0.4)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 7524467f-be28-4b96-9303-28d19a89424e))
  (fp_line (start 0.8 -0.4) (end 0.8 0.4)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 5dbab687-bb9a-4f0c-850e-c79f5d9ada7b))
  (fp_line (start 0.8 0.4) (end -0.8 0.4)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 0fd2ed2d-3ebf-4659-94e1-3fcd04942964))
  (pad "" smd oval (at -0.725 0) (size 0.55 0.75) (layers "F.Paste") (tstamp a10fded9-eac6-4104-aa5c-fc54d0dec548))
  (pad "" smd oval (at 0.725 0) (size 0.55 0.75) (layers "F.Paste") (tstamp f583b0b4-7ad8-4c2d-8a82-05977f198409))
  (pad "1" smd roundrect (at -0.725 0) (size 0.65 0.85) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp 27ed1176-7498-471e-beaa-8d1a15c737d7))
  (pad "2" smd roundrect (at 0.725 0) (size 0.65 0.85) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.05) (chamfer top_left bottom_left) (tstamp c61d29c5-99e3-4ae4-b577-cd9ce79e478b))
  (model "${KICAD7_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
