(footprint "JST_GH_BM04B-GHS-TBT_1x04-1MP_P1.25mm_Vertical" (version 20221018) (generator pcbnew)
  locked (layer "F.Cu")
  (descr "JST GH series connector, BM04B-GHS-TBT (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator")
  (tags "connector JST GH side entry")
  (property "LCSC" "C3011955")
  (property "MFG" "HCTL")
  (property "MPN" "HC-GH-4PLT")
  (property "Sheetfile" "QuadCameraCarrier.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
  (property "ki_keywords" "connector")
  (attr smd)
  (fp_text reference "J18" (at 0 -4) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2e0eac1c-da64-4ad8-9c70-5693f22f376e)
  )
  (fp_text value "CAN_OUT" (at 0 4) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b8866e74-4e87-4a8f-b489-5630194ad569)
  )
  (fp_text user "${REFERENCE}" (at 0 -1.5) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3cac0b66-c9cd-4089-8056-28c405079619)
  )
  (fp_line (start -4.235 0.26) (end -4.235 1.86)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp eae70f80-2645-4f66-b561-4a46cb06a1f5))
  (fp_line (start -4.235 1.86) (end -2.435 1.86)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7c7c2e94-f13d-47e5-b53e-28392245622a))
  (fp_line (start -2.965 -2.61) (end 2.965 -2.61)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3d94f8dd-86ef-4905-b78a-aa4e78ad0a14))
  (fp_line (start -2.435 1.86) (end -2.435 2.8)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5912cfdb-fe88-4df1-99c1-0e9b1a70838f))
  (fp_line (start 4.235 0.26) (end 4.235 1.86)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2ed73efe-13cc-46da-a93e-7b808008de88))
  (fp_line (start 4.235 1.86) (end 2.435 1.86)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b3076372-465f-495a-b92a-98168a440bfa))
  (fp_line (start -4.375 -2.55) (end -4.375 1.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c102255a-65b8-4413-a5f4-013bbb8cdcce))
  (fp_line (start -3.975 -2.95) (end 3.975 -2.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6dafc494-63f4-4359-b288-971ec6c339f8))
  (fp_line (start -2.325 2) (end -4.125 2)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1adf7439-4c40-41db-8049-c2f79c2ba9f7))
  (fp_line (start -2.325 2.65) (end -2.325 2)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2530d914-4027-44b9-b622-c35de961e598))
  (fp_line (start 2.025 2.95) (end -2.025 2.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 07391d68-456a-45e3-872d-4a5ff02d768c))
  (fp_line (start 2.325 2) (end 4.125 2)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 68a71936-d401-4c2a-a973-7216304efc54))
  (fp_line (start 2.325 2.65) (end 2.325 2)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2c02aa1b-e010-4b2a-a6c0-550008d8b4d8))
  (fp_line (start 4.375 -2.55) (end 4.375 1.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5c0372b0-5241-4384-847b-1f8dbe9dbff3))
  (fp_arc (start -4.375 -2.55) (mid -4.257843 -2.832843) (end -3.975 -2.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2ddc0945-5b2f-4e70-99bb-a35223c9c0ad))
  (fp_arc (start -4.125 2) (mid -4.301777 1.926777) (end -4.375 1.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a3bd6c26-aeaa-4e71-b4fe-bf0a8f21a295))
  (fp_arc (start -2.025 2.95) (mid -2.237132 2.862132) (end -2.325 2.65)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp af130d0e-5a39-48f3-b293-74929907f460))
  (fp_arc (start 2.325 2.65) (mid 2.237132 2.862132) (end 2.025 2.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 65a13aa4-619d-4de7-889b-33fe0618beda))
  (fp_arc (start 3.975 -2.95) (mid 4.257843 -2.832843) (end 4.375 -2.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4c901ad8-616a-40e9-8b2f-4faeda3ad41f))
  (fp_arc (start 4.375 1.75) (mid 4.301777 1.926777) (end 4.125 2)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3630d09e-7bb0-41cb-b106-0eeb7b1d2c75))
  (fp_line (start -4.125 -2.5) (end 4.125 -2.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 748318b1-d21a-40f4-88fd-084acd68ff69))
  (fp_line (start -4.125 1.75) (end -4.125 -2.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bbf48361-b15e-4303-9825-cc325c6814fe))
  (fp_line (start -4.125 1.75) (end 4.125 1.75)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ca31b1a8-c550-4687-8044-65585f4b513c))
  (fp_line (start -2.375 1.75) (end -1.875 1.042893)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bcc6b2d7-bf4b-44f9-b625-62e60dbf0606))
  (fp_line (start -2.125 -0.5) (end -2.125 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 89e7782d-45b5-4028-99e1-6329144241f6))
  (fp_line (start -2.125 0) (end -1.625 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6b0c79f4-2d8c-4d06-9dda-634ef1ae76ed))
  (fp_line (start -1.875 1.042893) (end -1.375 1.75)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6dc48b1a-79a9-451c-842f-99e8452c4c87))
  (fp_line (start -1.625 -0.5) (end -2.125 -0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5116a68d-00e6-45eb-abfa-c86f179fa398))
  (fp_line (start -1.625 0) (end -1.625 -0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c770539f-ae59-4bc9-a7ad-95a9bc0e4ee1))
  (fp_line (start -0.875 -0.5) (end -0.875 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp def30f95-8aed-4808-96df-d102c55132b4))
  (fp_line (start -0.875 0) (end -0.375 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7ce1f9d7-12c5-454a-b42b-88b0ee14a97c))
  (fp_line (start -0.375 -0.5) (end -0.875 -0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 585ffde2-ce0a-4541-8d22-7ef3e1cf3aad))
  (fp_line (start -0.375 0) (end -0.375 -0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cf687648-87b2-4e88-9a75-de0ceac74080))
  (fp_line (start 0.375 -0.5) (end 0.375 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 798aa5c5-5cf8-442c-b431-54e01884328e))
  (fp_line (start 0.375 0) (end 0.875 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d40e2329-5121-4910-8043-0e4ae60b85db))
  (fp_line (start 0.875 -0.5) (end 0.375 -0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3c5b9cfd-fa4f-48c6-8383-9099b267b32d))
  (fp_line (start 0.875 0) (end 0.875 -0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ae26f508-5d3d-4a14-864c-e1f41ea00672))
  (fp_line (start 1.625 -0.5) (end 1.625 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d0fb496f-3793-4b8d-bcd1-71d1c165d08d))
  (fp_line (start 1.625 0) (end 2.125 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 269237c8-5230-4deb-a541-c521387265eb))
  (fp_line (start 2.125 -0.5) (end 1.625 -0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 31ee19db-415c-44d5-a412-0053c5d8c586))
  (fp_line (start 2.125 0) (end 2.125 -0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1ffc44f4-f06e-475d-a1de-0600ffffff0b))
  (fp_line (start 4.125 1.75) (end 4.125 -2.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3f9ce929-1171-44ef-bcd7-527a005f010e))
  (pad "1" smd roundrect locked (at -1.875 1.95) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 82651238-691a-4f82-887d-590fc7c478a9))
  (pad "2" smd roundrect locked (at -0.625 1.95) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 38206bd1-f75c-46ea-9aa9-34a33d8e2d41))
  (pad "3" smd roundrect locked (at 0.625 1.95) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 21d0fe16-c38b-444b-b2ae-72762ebbe2d3))
  (pad "4" smd roundrect locked (at 1.875 1.95) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp fe5f86c3-0609-464f-9308-607b02733212))
  (pad "MP" smd roundrect locked (at -3.725 -1.4) (size 1 2.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 0f004517-1d6e-43f2-b487-bec97468e438))
  (pad "MP" smd roundrect locked (at 3.725 -1.4) (size 1 2.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp bf83fd0c-c361-402f-a6b6-c8ee3f2ff804))
  (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_GH_BM04B-GHS-TBT_1x04-1MP_P1.25mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
