(footprint "USB_C_Receptacle_XKB_U262-241N-4BV64" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Sheetfile" "RK3588_Camcorder_Carrier.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "USB Full-Featured Type-C Receptacle connector")
  (property "ki_keywords" "usb universal serial bus type-C full-featured")
  (attr through_hole)
  (fp_text reference "J12" (at -5.5 -0.5 90 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)) (justify left))
    (tstamp d7844463-e0e9-4d32-95ad-c7cf4211072c)
  )
  (fp_text value "USB-C OTG" (at 0 0.4 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp e83e71c5-6d58-4d6c-9491-583cafd749e8)
  )
  (fp_text user "${REF}" (at 0 0.9 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp df8f80fb-76e0-47f3-bfd8-ed149896f73d)
  )
  (fp_rect (start -4.45 -6.2) (end -4.3 -4)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 6c2deaed-4816-4504-8b95-75b75db869bf))
  (fp_rect (start -4.45 -1.4) (end -4.3 -0.15)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp b8fd32e7-5153-42f5-b701-6c6e05e80c83))
  (fp_rect (start -3.75 -7.75) (end -2.9 -7.9)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 1e28d0c5-600e-4d7d-8acf-a158498b2f8b))
  (fp_rect (start 3.15 -7.75) (end 3.75 -7.9)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 1baee4fc-44d0-4696-a523-316d9dd7f0dd))
  (fp_rect (start 4.3 -6.2) (end 4.45 -4)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 2e4cb637-10d7-446f-aa90-ae7523e588a0))
  (fp_rect (start 4.3 -1.4) (end 4.45 -0.15)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 8ff28ae4-02bb-467b-8a87-f13231467c99))
  (fp_line (start -6.2 0) (end -6.2 10)
    (stroke (width 0.12) (type default)) (layer "Dwgs.User") (tstamp 6366be7c-55b5-4380-9d16-76362bdd1ed5))
  (fp_line (start -6.2 0) (end 6.2 0)
    (stroke (width 0.12) (type default)) (layer "Dwgs.User") (tstamp 59be2ebc-c3a4-4e67-8d13-ecd0a89cdf41))
  (fp_line (start 6.2 0) (end 6.2 10)
    (stroke (width 0.12) (type default)) (layer "Dwgs.User") (tstamp 6e3b7bcc-9c8c-4bc8-9be3-6e707f19c5f8))
  (fp_rect (start -4.47 0) (end 4.47 -7.9)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 6ea0d47e-9256-4978-bb8f-e3040c712d45))
  (pad "" np_thru_hole circle (at -3.4 -5.9) (size 0.7 0.7) (drill 0.5) (layers "*.Mask") (tstamp 0131509b-69b8-4dfc-a732-f37b73a1ac19))
  (pad "" np_thru_hole circle (at 3.4 -5.9) (size 0.7 0.7) (drill 0.5) (layers "*.Mask") (tstamp 45edf525-6774-4926-ad98-76a5ea28b1a6))
  (pad "A1" smd roundrect (at -2.625 -7.925) (size 0.25 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 7f51e532-6c62-4792-8819-e9ea01f0f130))
  (pad "A2" smd roundrect (at -2.125 -7.925) (size 0.25 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 022d40d5-477e-4106-af00-73022d32648c))
  (pad "A3" smd roundrect (at -1.625 -7.925) (size 0.25 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp b34a804d-1680-4148-ab25-da8ce60ebf20))
  (pad "A4" smd roundrect (at -1.125 -7.925) (size 0.25 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp e76ad696-a46b-48f5-8586-9759f8e5851f))
  (pad "A5" smd roundrect (at -0.625 -7.925) (size 0.25 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp f9b45db7-db8d-4642-82a5-3b13f60f0026))
  (pad "A6" smd roundrect (at -0.125 -7.925) (size 0.25 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 02d79479-2838-4856-b30a-767a1c869046))
  (pad "A7" smd roundrect (at 0.375 -7.925) (size 0.25 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp a928735a-27b3-4d55-bd96-e70a0de547ab))
  (pad "A8" smd roundrect (at 0.875 -7.925) (size 0.25 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 400bcaac-7f23-477c-b70a-c9a75ea5b8e4))
  (pad "A9" smd roundrect (at 1.375 -7.925) (size 0.25 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 3dc65573-047d-4162-b3ac-45ff0110cc36))
  (pad "A10" smd roundrect (at 1.875 -7.925) (size 0.25 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp a76ade50-56be-4c44-a0d8-4ece04c8e4be))
  (pad "A11" smd roundrect (at 2.375 -7.925) (size 0.25 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 0a5ebf36-ef80-4ab9-bb67-245e6cb10413))
  (pad "A12" smd roundrect (at 2.875 -7.925) (size 0.25 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 65e352cd-ebc7-4e72-9591-850b43a735cd))
  (pad "B1" smd roundrect (at 2.625 -6.525) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp f085c606-c83e-4ec9-8e0d-3b4926c7e6ea))
  (pad "B2" smd roundrect (at 2.125 -6.525) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp cdd959bc-2c6e-4f5c-86de-9277bfbe8463))
  (pad "B3" smd roundrect (at 1.625 -6.525) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp d24e8df0-08e6-4734-9c95-a5c5efac8399))
  (pad "B4" smd roundrect (at 1.125 -6.525) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 2dbd233b-6368-42d0-a754-cf52d096c83c))
  (pad "B5" smd roundrect (at 0.625 -6.525) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 7d387939-9336-43c1-978c-c30d8698671f))
  (pad "B6" smd roundrect (at 0.125 -6.525) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 50cfae50-6975-4aa2-b341-776ccee4770f))
  (pad "B7" smd roundrect (at -0.375 -6.525) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 021ac623-aa1c-48fa-91ea-598342deaa29))
  (pad "B8" smd roundrect (at -0.875 -6.525) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp e28e6cf7-373a-4e96-a226-68f58f55e57d))
  (pad "B9" smd roundrect (at -1.375 -6.525) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 48d9c089-d8e3-45d0-b481-58ad8cbc4f0f))
  (pad "B10" smd roundrect (at -1.875 -6.525) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 74c338a2-9fe4-4c47-a9b7-024216298a8d))
  (pad "B11" smd roundrect (at -2.375 -6.525) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 458a65ad-90dc-4bfc-a100-e6d73d6a0f65))
  (pad "B12" smd roundrect (at -2.875 -6.525) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp aa29155a-b3fc-43d3-94cb-90a298012ee5))
  (pad "S1" thru_hole oval (at -4.32 -7.25) (size 0.8 1.8) (drill oval 0.6 1.6) (layers "*.Cu" "*.Mask") (tstamp ee65bb7a-a3d4-415d-aa62-9724d1eb8c1d))
  (pad "S1" thru_hole oval (at -4.32 -2.7) (size 1 2.3) (drill oval 0.6 1.9) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (tstamp b62e02db-14d6-4ada-b8e3-ef6521de73a1))
  (pad "S1" thru_hole oval (at -4.02 -6.75) (size 1.4 0.8) (drill oval 1.2 0.6) (layers "*.Cu" "*.Mask") (tstamp d1ca3e69-1006-4087-8d83-66d859db0eec))
  (pad "S1" thru_hole oval (at 4.02 -6.75) (size 1.4 0.8) (drill oval 1.2 0.6) (layers "*.Cu" "*.Mask") (tstamp 45e84ec9-7c11-43c6-802a-5c8b086ed2e2))
  (pad "S1" thru_hole oval (at 4.32 -7.25) (size 0.8 1.8) (drill oval 0.6 1.6) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (tstamp c27bd6af-4cf1-48d1-8172-9e39783428d0))
  (pad "S1" thru_hole oval (at 4.32 -2.7) (size 1 2.3) (drill oval 0.6 1.9) (layers "*.Cu" "*.Mask") (tstamp b9fba128-bf53-4542-b2b6-56e9a94e57dd))
  (model "${KICAD7_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_XKB_U262-241N-4BV64.step"
    (offset (xyz 0 0.49 1.65))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
