(footprint "R_Shunt_Vishay_WSK1216"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "R1"
		(at 2.75 0 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "12430fe6-bacf-44b8-ba63-1ba725de1910")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "0.5m"
		(at 0 1.249999 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "ce8b922d-c6b8-4eb6-b388-e35f7c87912d")
		(effects
			(font
				(size 0.2 0.2)
				(thickness 0.05)
			)
		)
	)
	(property "Footprint" "Resistor_SMD:R_Shunt_Vishay_WSK1216"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "266044a9-b6ea-4a31-a4bc-066aea68a0d2")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7cd83075-f31f-4a9d-a0f1-fab620d000d0")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "79396fe4-f815-4648-b7ee-92e53db2cbb1")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "LCSC" "C2688874"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "69be2145-c91a-4404-ad88-bacd40d257dc")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "Isabellenhuette"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "eb583e1e-3f56-4714-a686-24226b8f91f4")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "  BVN-Z-R0005-1.0"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "c9e603b6-f693-4c69-bf2a-0b9351a4daab")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Preferred" ""
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "97661f6a-c5da-448e-9d52-d0887aba6b74")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(zone_connect 2)
	(attr smd)
	(fp_line
		(start -2.225 -1.8)
		(end -2.225 1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "793adb25-2405-4ce0-92d7-870896b421fc")
	)
	(fp_line
		(start -2.075 1.95)
		(end 2.075 1.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "3d55eca5-c41d-4712-ae23-27a30baba02c")
	)
	(fp_line
		(start 2.075 -1.95)
		(end -2.075 -1.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "af434276-a05b-4b00-a24b-dd461dfe8f30")
	)
	(fp_line
		(start 2.225 1.8)
		(end 2.225 -1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f2e43c98-56cc-42c9-aca5-23ea972f6c3e")
	)
	(fp_arc
		(start -2.225 -1.8)
		(mid -2.181066 -1.906066)
		(end -2.075 -1.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "22126e97-404b-4d28-a97c-e5508007f543")
	)
	(fp_arc
		(start -2.075 1.95)
		(mid -2.181066 1.906066)
		(end -2.225 1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "49f28ece-5285-4391-88c1-09c9a4fca0b1")
	)
	(fp_arc
		(start 2.075 -1.95)
		(mid 2.181066 -1.906066)
		(end 2.225 -1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "31502bf6-6995-4038-9b93-f11958d96b22")
	)
	(fp_arc
		(start 2.225 1.8)
		(mid 2.181066 1.906066)
		(end 2.075 1.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "48181c5e-bbd2-4541-9ad3-cdec5da2ed41")
	)
	(fp_poly
		(pts
			(xy 2.049999 1.55) (xy -2.049999 1.55) (xy -2.049999 -1.55) (xy 2.049999 -1.55)
		)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "19ef32c0-98f2-4a78-a1e6-a0fb50103510")
	)
	(pad "1" smd roundrect
		(at 0.5 -1.052499)
		(size 3.15 1.495)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.06688963211)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "ee090c2b-474d-4ba2-b2eb-4abfd68e08a3")
	)
	(pad "2" smd roundrect
		(at -1.725 -1.0525)
		(size 0.7 1.495)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1428571429)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "4ea04ed1-677e-4655-8548-08d9af92f24e")
	)
	(pad "3" smd roundrect
		(at -1.725 1.0525)
		(size 0.7 1.495)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1428571429)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "515d9a7a-26d7-43d6-9d20-06dda43676c3")
	)
	(pad "4" smd roundrect
		(at 0.5 1.052499)
		(size 3.15 1.495)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.06688963211)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "f41976dd-dfce-43ae-a0b3-23a1911ef9f9")
	)
	(model "${KICAD7_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Shunt_Vishay_WSKW1216.step"
		(offset
			(xyz 3.81 0.055 1.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 90)
		)
	)
	(model "${KICAD7_3DMODEL_DIR}/Resistor_SMD.3dshapes/IsabellenHutte_BVN.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 90)
		)
	)
)