(footprint "JST_VH_B2P-VH_1x02_P3.96mm_Vertical" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "JST VH series connector, B2P-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator")
  (tags "connector JST VH vertical")
  (property "Sheetfile" "QuadCameraCarrier.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
  (property "ki_keywords" "connector")
  (attr through_hole)
  (fp_text reference "J17" (at 1.98 -4.9 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 737487c1-f566-46b8-8e44-6956d288340d)
  )
  (fp_text value "VIN" (at 1.98 6 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 66a78c6a-b9cd-4ce7-86fc-08f202c5278a)
  )
  (fp_text user "${REFERENCE}" (at 1.98 4.1 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ff9172bf-26da-4e77-b4eb-373a92b6a610)
  )
  (fp_line (start -2.86 -0.3) (end -2.26 0)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp da370285-f82e-445b-b2fa-d8c8ff460dbe))
  (fp_line (start -2.86 0.3) (end -2.86 -0.3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ce1f7ceb-3465-41f1-a8a6-85d4579d3c56))
  (fp_line (start -2.26 0) (end -2.86 0.3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3dfcd9f7-bcaa-41d3-92fc-94c716b610dc))
  (fp_line (start -2.06 -2.11) (end -0.86 -2.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 20742758-6cbd-4667-a0ca-44a8312f1957))
  (fp_line (start -2.06 4.91) (end -2.06 -2.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a96453bd-4ed7-44e8-8188-208bee41b1f8))
  (fp_line (start -0.86 -3.81) (end 4.82 -3.81)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3bececd3-46aa-40e7-8eab-14529070d30d))
  (fp_line (start -0.86 -2.11) (end -0.86 -3.81)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 152f504d-127b-46a6-8513-6c4b22a142c3))
  (fp_line (start 4.82 -3.81) (end 4.82 -2.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7d854954-af4b-445f-a56a-ec082657e34c))
  (fp_line (start 4.82 -2.11) (end 6.02 -2.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9c7e68cb-c7a6-428e-8c51-587add7fc8ac))
  (fp_line (start 6.02 -2.11) (end 6.02 4.91)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8728bc2a-ff78-4085-9d54-defca873fa03))
  (fp_line (start 6.02 4.91) (end -2.06 4.91)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4e97a843-5243-4f3a-8785-1df27ce84f68))
  (fp_line (start -2.45 -4.2) (end -2.45 5.3)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8d6f4ba8-f790-4979-bd44-5640c3e565f0))
  (fp_line (start -2.45 5.3) (end 6.41 5.3)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c9371c94-7b70-438d-920f-cf348f771ee6))
  (fp_line (start 6.41 -4.2) (end -2.45 -4.2)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 09889c8f-0093-43d7-bec1-6a21be6445a5))
  (fp_line (start 6.41 5.3) (end 6.41 -4.2)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2a965074-a05a-4c0b-9f7b-efd0ae96a6a5))
  (fp_line (start -1.95 -2) (end -1.95 4.8)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3fb75794-daaf-4a7e-943b-c09ea921802c))
  (fp_line (start -1.95 -1) (end -0.95 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d57bab0f-c9ca-4f3c-83bd-e0a8fe5fd74d))
  (fp_line (start -1.95 1) (end -0.95 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bf36aa53-e150-4cc5-9b79-b0b4c5c4c581))
  (fp_line (start -1.95 4.8) (end 5.91 4.8)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d6ae0c2a-eb1a-4661-b343-e2627f9c70ca))
  (fp_line (start -0.75 -3.7) (end 4.71 -3.7)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 70115294-2f04-4c0c-93bf-2ae6c2ad4cbf))
  (fp_line (start -0.75 -2) (end -0.75 -3.7)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c2b0bd56-6c49-4a49-b3b3-d7e6d631c2b1))
  (fp_line (start 4.71 -3.7) (end 4.71 -2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp da470f83-1874-458b-bfc6-0497877d3ccd))
  (fp_line (start 5.91 -2) (end -1.95 -2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 954573a4-2dec-451d-8399-e6a815e0f430))
  (fp_line (start 5.91 4.8) (end 5.91 -2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 88247fd3-d415-42a2-81f4-13f9e3e6d6ad))
  (pad "1" thru_hole roundrect (at 0 0) (size 2.7 2.7) (drill 1.7) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.092593) (tstamp 22ed6de7-5948-4ab8-be3c-f4f376581161))
  (pad "2" thru_hole circle (at 3.96 0) (size 2.7 2.7) (drill 1.7) (layers "*.Cu" "*.Mask") (tstamp fb5e9885-2320-489b-a90a-4ea58bb907b5))
  (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_VH_B2P-VH_1x02_P3.96mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model ":KICAD7_3DMODEL_DIR:Connector_JST.3dshapes/B2P-VH.STEP"
    (offset (xyz 1.98 -0.55 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
