(footprint "MR30PB_Dual_Mount" (version 20220417) (generator pcbnew)
  (layer "F.Cu")
  (property "Dielectric" "")
  (property "Footprint_Density" "")
  (property "Footprint_Library" "")
  (property "JLCPCB Part" "")
  (property "LCSC" "")
  (property "MFG" "")
  (property "MPN" "DO NOT POPULATE")
  (property "MPN_ALT1" "")
  (property "Mouser" "")
  (property "Note" "")
  (property "Package" "")
  (property "Sheetfile" "ESC_Dual_10A.kicad_sch")
  (property "Sheetname" "")
  (property "Spice_Model" "")
  (property "Spice_Netlist_Enabled" "")
  (property "Spice_Primitive" "")
  (property "Tolerance" "")
  (property "USD_per_1" "")
  (property "USD_per_1000" "")
  (property "Voltage" "")
  (property "exclude_from_bom" "")
  (property "ki_description" "Generic screw terminal, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
  (property "ki_keywords" "screw terminal")
  (attr through_hole exclude_from_bom)
  (fp_text reference "J4" (at 0 2.5 unlocked) (layer "Cmts.User")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 89bcf79b-7b07-47b0-9a21-bf2a4a977d22)
  )
  (fp_text value "M1" (at -1.7 1.3 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp c475c9bd-2f00-4fad-a866-07ebb9f323eb)
  )
  (fp_text user "${REFERENCE}" (at 1.8 1.35 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp fab2760f-77b6-431b-b162-affb7a3225a2)
  )
  (fp_line (start -1.9 1.9) (end -1.6 1.9)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 16eed54e-e6e7-497e-9d99-4a647369e7cd))
  (fp_line (start -1.8 -1.9) (end -1.7 -1.9)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 489947d7-60d0-4f09-ad22-5ec72b16e3a6))
  (fp_line (start 1.6 1.9) (end 1.9 1.9)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 2989483b-f32a-40b6-964a-5e8139d5c088))
  (fp_line (start 1.7 -1.9) (end 1.8 -1.9)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp b0b113e7-154b-419e-ab6c-f3a99bb095f1))
  (fp_arc (start -5.2 0.85) (mid -5.401016 0) (end -5.2 -0.85)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 65385134-fea7-4e93-8a3c-ac4c2a9e2290))
  (fp_arc (start 5.2 -0.85) (mid 5.400672 0) (end 5.2 0.85)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 6da5c0b9-338f-40c9-be12-cc0b58cf8ba9))
  (fp_line (start -3.5 -2.45) (end 3.5 -2.45)
    (stroke (width 0.05) (type default)) (layer "F.Fab") (tstamp 171b92af-2134-447d-9b9f-1eeaf2029796))
  (fp_line (start -3.5 -1.9) (end 3.5 -1.9)
    (stroke (width 0.05) (type default)) (layer "F.Fab") (tstamp a9bb5c4f-2caa-45cb-ad6c-cf03d1aacb34))
  (fp_line (start 3.5 1.9) (end -3.5 1.9)
    (stroke (width 0.05) (type default)) (layer "F.Fab") (tstamp b0ca975f-0016-474c-a37d-8fd00d8abda9))
  (fp_line (start 3.5 2.45) (end -3.5 2.45)
    (stroke (width 0.05) (type default)) (layer "F.Fab") (tstamp 8460b63f-0119-404e-9561-7a838aca1b44))
  (fp_rect (start -5.95 -2.45) (end 5.95 -12.85)
    (stroke (width 0.05) (type dash)) (fill none) (layer "F.Fab") (tstamp 0ee6b344-38ba-484c-9314-b0a6d4175844))
  (fp_arc (start -3.5 1.9) (mid -5.4 0) (end -3.5 -1.9)
    (stroke (width 0.05) (type default)) (layer "F.Fab") (tstamp d5bd64c4-21b6-492f-ac45-da5fd26d3d58))
  (fp_arc (start -3.5 2.45) (mid -5.95 0) (end -3.5 -2.45)
    (stroke (width 0.05) (type default)) (layer "F.Fab") (tstamp 1e21a9ea-bc18-4fd4-9d5f-44b6f32c399a))
  (fp_arc (start 3.5 -2.45) (mid 5.95 0) (end 3.5 2.45)
    (stroke (width 0.05) (type default)) (layer "F.Fab") (tstamp e1e618c7-7156-45b3-987a-4554ffb5a9b1))
  (fp_arc (start 3.5 -1.9) (mid 5.4 0) (end 3.5 1.9)
    (stroke (width 0.05) (type default)) (layer "F.Fab") (tstamp 59b6c25e-fbb5-4631-b835-f38ef73928d1))
  (pad "1" connect rect (at -3.5 -1.125) (size 3 2.25) (layers "F.Cu" "F.Mask") (tstamp 0cc5f00c-1760-4d21-a0f6-d6aa657ff2d2))
  (pad "1" thru_hole circle (at -3.5 0) (size 3 3) (drill 1.7) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp 0260cc44-a652-4c5c-9689-ebb02ae27d63))
  (pad "1" connect roundrect (at -3.5 0.2) (size 3 4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2222222222) (tstamp 8ff98a26-6739-43f9-9186-5964d84409b5))
  (pad "2" connect rect (at 0 -1.125) (size 3 2.25) (layers "F.Cu" "F.Mask") (tstamp 0a811570-5e29-4b72-8750-ea5c0872ea7e))
  (pad "2" thru_hole circle (at 0 0) (size 3 3) (drill 1.7) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp 0f928d64-f90f-4f0a-8106-236c96ae7909))
  (pad "2" connect roundrect (at 0 0.25) (size 3 4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2222222222) (tstamp 9711c732-0344-4dc9-9f9a-658730f5b02b))
  (pad "3" connect rect (at 3.5 -1.125) (size 3 2.25) (layers "F.Cu" "F.Mask") (tstamp 4072afc8-53a3-4461-b21c-a7d9b5fba031))
  (pad "3" thru_hole circle (at 3.5 0) (size 3 3) (drill 1.7) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp 8a3d5d93-ec90-434f-a2af-5fad2ec22a57))
  (pad "3" connect roundrect (at 3.5 0.25) (size 3 4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2222222222) (tstamp fdb62d3b-b671-4533-9c9f-22f9d789041f))
  (model "${KICAD7_3DMODEL_DIR}/Connector_AMASS.3dshapes/Amass_MR30PB-FB.wrl"
    (offset (xyz 0 2.5 0.7))
    (scale (xyz 1 1 1))
    (rotate (xyz 90 0 0))
  )
  (model "${KICAD7_3DMODEL_DIR}/Connector_AMASS.3dshapes/Amass_MR30PB-FB.wrl" hide
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
