(footprint "Murata_DLM0NSxxxxHY2x" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "LCSC" "C913480")
  (property "MFG" "Murata")
  (property "MPN" "DLM0NSN500HY2")
  (property "Sheetfile" "QuadCameraCarrier.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "EMI 3-inductor common mode filter")
  (property "ki_keywords" "EMI common mode filter c-phy")
  (attr smd)
  (fp_text reference "FL21" (at 0 -0.75 unlocked) (layer "F.SilkS") hide
      (effects (font (size 0.2 0.2) (thickness 0.05)))
    (tstamp f48f3773-ec69-4ed3-9fbf-b9b4b65279f4)
  )
  (fp_text value "Filter_EMI_Duo_CommonMode" (at 0.05 0.8 unlocked) (layer "F.Fab") hide
      (effects (font (size 0.2 0.2) (thickness 0.05)))
    (tstamp 54291893-e53b-4863-a89c-0b87f14816e2)
  )
  (fp_text user "${REFERENCE}" (at 0 -0.75 unlocked) (layer "F.Fab") hide
      (effects (font (size 0.2 0.2) (thickness 0.05)))
    (tstamp 4843fc8c-2028-4054-918a-500e2e354101)
  )
  (fp_poly
    (pts
      (xy -0.5 -0.35)
      (xy -0.5 0.35)
      (xy -0.65 0.35)
      (xy -0.65 -0.35)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 64954ec4-9b2e-4af2-a95e-8c2a8fd3b340))
  (fp_poly
    (pts
      (xy 0.65 -0.35)
      (xy 0.65 0.35)
      (xy 0.5 0.35)
      (xy 0.5 -0.35)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 3b4336aa-a49e-4ac6-b6c5-ca9d06dc6bf7))
  (fp_line (start -0.675 0.325) (end -0.675 -0.325)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0dd3f94d-6b55-4750-9d58-a65eff12bcf7))
  (fp_line (start -0.401535 -0.578453) (end -0.425 -0.575)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c850d44f-0580-4662-bb91-b6b57cdb6d8c))
  (fp_line (start -0.401535 0.578453) (end -0.425 0.575)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e442101a-a833-4612-a6a2-89cb62cd98dc))
  (fp_line (start -0.3 0.6) (end 0.3 0.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a65910c9-6142-40b1-9731-d9f2ead68fc8))
  (fp_line (start 0.3 -0.6) (end -0.3 -0.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 80e12f92-67f1-40f3-b386-160ca13c21f0))
  (fp_line (start 0.401535 -0.578453) (end 0.425 -0.575)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d542c0b6-145f-46b7-902e-29dcd1ed8160))
  (fp_line (start 0.401535 0.578453) (end 0.425 0.575)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 834b2865-b816-487e-afd4-fa55be895ba1))
  (fp_line (start 0.675 0.325) (end 0.675 -0.325)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp edddfb09-b562-49c5-bd7a-215e57e5cc69))
  (fp_arc (start -0.675 -0.325) (mid -0.601777 -0.501777) (end -0.425 -0.575)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7a916999-9a39-4755-b22e-1b1dfec56072))
  (fp_arc (start -0.425 0.575) (mid -0.601777 0.501777) (end -0.675 0.325)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2b626cda-38a5-4517-8fa0-a57428106c9f))
  (fp_arc (start -0.401535 -0.578453) (mid -0.351898 -0.594554) (end -0.3 -0.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e0bb022b-15a6-4bd8-b17b-a1f2a0e18921))
  (fp_arc (start -0.3 0.6) (mid -0.351898 0.594554) (end -0.401535 0.578453)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2a235cdb-e939-41af-b578-195ca0bf499e))
  (fp_arc (start 0.3 -0.6) (mid 0.351898 -0.594554) (end 0.401535 -0.578453)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp dc11e2a4-34f5-425c-85e3-30be03ad94d8))
  (fp_arc (start 0.401535 0.578453) (mid 0.351898 0.594554) (end 0.3 0.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 782daf4b-f29d-449b-9eb6-e123e30d0b5d))
  (fp_arc (start 0.425 -0.575) (mid 0.601777 -0.501777) (end 0.675 -0.325)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp df979608-957a-4b05-b302-9053fa04e7c9))
  (fp_arc (start 0.675 0.325) (mid 0.601777 0.501777) (end 0.425 0.575)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b2268135-d22a-4358-ad6a-e92cf474e563))
  (fp_rect (start -0.425 -0.325) (end 0.425 0.325)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.Fab") (tstamp 5ccd798e-34ce-4682-b701-4c9f7d872aa6))
  (pad "" smd oval (at -0.25 -0.3) (size 0.2 0.25) (layers "F.Paste") (tstamp 4587c216-3d26-4314-9144-c620d00f9310))
  (pad "" smd oval (at -0.25 0.3) (size 0.2 0.25) (layers "F.Paste") (tstamp a9468a58-c073-493b-bf9f-63c5afa9c8d2))
  (pad "" smd oval (at 0.25 -0.3) (size 0.2 0.25) (layers "F.Paste") (tstamp 307e4f1e-ff46-4d8e-bcb4-562d2d72de20))
  (pad "" smd oval (at 0.25 0.3) (size 0.2 0.25) (layers "F.Paste") (tstamp 7d4de181-8f35-4d31-b096-71b4da2ca3cd))
  (pad "1" smd roundrect (at -0.25 -0.3) (size 0.3 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.1) (chamfer bottom_left bottom_right) (tstamp 03043987-29ee-4ef4-9b36-dcf53ca2e666))
  (pad "2" smd roundrect (at -0.25 0.3 180) (size 0.3 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.1) (chamfer bottom_left bottom_right) (tstamp a24d6880-3238-425a-808c-3730b6b13aa6))
  (pad "3" smd roundrect (at 0.25 -0.3) (size 0.3 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.1) (chamfer bottom_left bottom_right) (tstamp 4828e401-ebb9-45c8-ba00-99c61b7ec33f))
  (pad "4" smd roundrect (at 0.25 0.3 180) (size 0.3 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.1) (chamfer bottom_left bottom_right) (tstamp c3d65e7b-ab1f-4c37-b27d-15c3d507257c))
  (model ":KICAD7_3DMODEL_DIR:Filter.3dshapes/Murata DLM0NS.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
