(footprint "1608_A" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (tags "0603 1608")
  (property "Sheet file" "ESC12S30.kicad_sch")
  (property "Sheet name" "")
  (property "USD_per_1" "0,08")
  (property "USD_per_1000" "0,024")
  (solder_mask_margin 0.05)
  (solder_paste_margin -0.1)
  (attr smd)
  (fp_text reference "R31" (at 1.3 0 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)) (justify left))
    (tstamp 286496ee-a624-452d-97d6-5c06edf19a68)
  )
  (fp_text value "10k" (at 1.3 0.6 unlocked) (layer "F.Fab")
      (effects (font (size 0.2 0.2) (thickness 0.05)) (justify left))
    (tstamp 6a84b6aa-60b7-4fc3-a43c-735a4be4e6f0)
  )
  (fp_poly
    (pts
      (xy 0.325 -0.425)
      (xy -0.325 -0.425)
      (xy -0.325 -0.575)
      (xy 0.325 -0.575)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 52c1a281-9b00-455c-a52b-113c12592e6c))
  (fp_poly
    (pts
      (xy 0.325 0.575)
      (xy -0.325 0.575)
      (xy -0.325 0.425)
      (xy 0.325 0.425)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 6396cc12-a8a5-4fd3-9e06-992034167459))
  (fp_line (start -1.75 0.4) (end -1.75 -0.4)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0a07e8e9-c9f4-4fbf-b903-42ce4df3d8da))
  (fp_line (start -1.2 -0.95) (end 1.2 -0.95)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ae5a7f99-9fa2-45d4-9e72-791d7e64acbd))
  (fp_line (start 1.2 0.95) (end -1.2 0.95)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5e0b9728-a9c5-4e93-adac-b3817f049e91))
  (fp_line (start 1.75 -0.4) (end 1.75 0.4)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1fdbbb76-0226-435b-b00d-ca6c5b7acce3))
  (fp_arc (start -1.75 -0.4) (mid -1.588909 -0.788909) (end -1.2 -0.95)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 987be7cf-fcd4-41ae-89ea-4788c2e13904))
  (fp_arc (start -1.2 0.95) (mid -1.588909 0.788909) (end -1.75 0.4)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 155747c5-5657-4eb3-bbeb-0093f20566a9))
  (fp_arc (start 1.2 -0.95) (mid 1.588909 -0.788909) (end 1.75 -0.4)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 41d416bf-d644-44d1-9b28-609ac8cbf1c5))
  (fp_arc (start 1.75 0.4) (mid 1.588909 0.788909) (end 1.2 0.95)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a822bc84-ad52-4d04-983c-aa47650fa1fe))
  (fp_rect (start -0.8 -0.4) (end 0.8 0.4)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.Fab") (tstamp 329d6a21-1376-455d-b4ba-cbd5d15abce7))
  (pad "1" smd roundrect (at -0.825 0) (size 0.85 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.059) (tstamp 6b54222d-8709-4193-988b-a932c58516dc))
  (pad "2" smd roundrect (at 0.825 0) (size 0.85 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.059) (tstamp bc4b66fa-2dfc-4a75-8861-ee11207dd50d))
  (model "${KICAD7_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
