(footprint "MOUNT_HOLE_M1.6"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(locked yes)
	(layer "F.Cu")
	(tags "MOUNT HOLE FASTENER SCREW")
	(property "Reference" "H1"
		(at 0 -1 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "7d5ae79b-170c-4376-b30b-55fbac62881b")
		(effects
			(font
				(size 0.0254 0.0254)
			)
		)
	)
	(property "Value" "M1.6"
		(at 0 1 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "306617d3-42f4-444b-bc3a-a6bd865f2dfa")
		(effects
			(font
				(size 0.0254 0.0254)
			)
		)
	)
	(property "Footprint" "MOUNT_HOLE_M1.6"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "cbea89e1-a1e5-4998-929a-019ea0cee6e0")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "cb941b90-efc4-450c-bf4b-beb66e657f52")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9848959d-93b6-48e9-b79a-80114b6a88de")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a23b2a79-c070-4815-a84c-b6cd34f2a088")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(solder_mask_margin 0.0001)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_circle
		(center 0 0)
		(end 1.525 0)
		(stroke
			(width 0.15)
			(type solid)
		)
		(fill none)
		(layer "B.SilkS")
		(uuid "6ad4024f-31fc-45a8-aa11-572b9690c9db")
	)
	(fp_circle
		(center 0 0)
		(end 1.75 0)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "B.CrtYd")
		(uuid "6f912aa5-812c-408f-a7a2-8c6cc45f4bc0")
	)
	(fp_circle
		(center 0 0)
		(end 1.75 0)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "154831a2-0ed9-477f-8056-518d40500363")
	)
	(fp_text user "M1.6"
		(at 2.4 -1.2 0)
		(layer "F.Fab")
		(uuid "da46a971-2b22-4e11-8f26-823135322af6")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.127)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.3 2.3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "c0f4785f-d505-4322-9ae4-1dd57625c807")
	)
	(pad "1" connect circle
		(at 0 0)
		(size 3.2 3.2)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1d1ec6cb-22db-4ce7-93fb-4aedc118f4ca")
	)
)
