(footprint "UFBGA-201_10x10mm_Layout15x15_P0.65mm_0.125_opt_pads_C" (version 20210108) (generator pcbnew) (layer "F.Cu")
  (tedit 6000724D)
  (descr "UFBGA-201, 15x15 raster, 10x10mm package, pitch 0.65mm. This version allows routing with 125/125um tracks and 450/250um vias")
  (tags "BGA 201 0.65")
  (property "Sheet file" "UniversalRoboticsController.kicad_sch")
  (property "Sheet name" "")
  (attr smd)
  (fp_text reference "U11" (at 0 -5.875 180) (layer "F.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 738b7a5d-7da8-469a-a6fb-591039843483)
  )
  (fp_text value "STM32H750IBKx" (at 0 5.5 180) (layer "F.Fab")
    (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp def0cc78-8b37-4e2e-a3f6-fac57cbf25a1)
  )
  (fp_text user "${REFERENCE}" (at 0 -4 180) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c0e5188c-973a-4c2d-930b-59691a4ea7ef)
  )
  (fp_arc (start 5.15 5.15) (end 5.225 5.15) (angle 90) (layer "F.SilkS") (width 0.15) (tstamp 57dd72c9-07ea-4be4-b989-292e538d614f))
  (fp_arc (start 5.15 -5.15) (end 5.15 -5.225) (angle 90) (layer "F.SilkS") (width 0.15) (tstamp 6a71ac30-f53b-43cb-9e36-efcc9415f1ad))
  (fp_arc (start -5.15 5.15) (end -5.15 5.225) (angle 90) (layer "F.SilkS") (width 0.15) (tstamp a6d446d9-58ba-47dd-8a4f-6f4c129ac532))
  (fp_poly (pts (xy 5.3 -5.15)
    (xy 5.3 5.15)
    (xy 5.15 5.3)
    (xy -5.15 5.3)
    (xy -5.3 5.15)
    (xy -5.3 -4.5)
    (xy -5.15 -4.5)
    (xy -5.15 5.15)
    (xy 5.15 5.15)
    (xy 5.15 -5.15)
    (xy -4.5 -5.15)
    (xy -4.5 -5.3)
    (xy 5.15 -5.3)) (layer "F.SilkS") (width 0) (fill solid) (tstamp d2bb8955-421f-4627-ae9d-f4818070cbd2))
  (fp_line (start 5.5 5) (end 5.5 -5) (layer "F.CrtYd") (width 0.05) (tstamp 136b4733-ef54-4586-bb63-1b4723d2edae))
  (fp_line (start -5.5 -5) (end -5.5 5) (layer "F.CrtYd") (width 0.05) (tstamp 2b5a4732-8c76-4d85-906a-d171d9c0222d))
  (fp_line (start 5 -5.5) (end -5 -5.5) (layer "F.CrtYd") (width 0.05) (tstamp 432ebb35-bd40-428c-afa0-a2c22322120c))
  (fp_line (start -5 5.5) (end 5 5.5) (layer "F.CrtYd") (width 0.05) (tstamp 4b2ba687-ccfa-4b17-8d32-915edaf6a265))
  (fp_arc (start -5 -5) (end -5 -5.5) (angle -90) (layer "F.CrtYd") (width 0.05) (tstamp 2b7feb93-ff17-4669-99b7-2a53e9d35e6f))
  (fp_arc (start 5 5) (end 5 5.5) (angle -90) (layer "F.CrtYd") (width 0.05) (tstamp 4e14beb7-6260-4b9b-8af9-ff6d6273bdd5))
  (fp_arc (start 5 -5) (end 5.5 -5) (angle -90) (layer "F.CrtYd") (width 0.05) (tstamp 4f37754c-c6b7-4d36-a5ad-c89519ed3af8))
  (fp_arc (start -5 5) (end -5.5 5) (angle -90) (layer "F.CrtYd") (width 0.05) (tstamp 88ae44b3-fc69-4f67-8be0-841afbc63bed))
  (fp_line (start -5 5) (end -5 -5) (layer "F.Fab") (width 0.05) (tstamp 2008377c-528d-4123-90a5-dc8ae6d63d5c))
  (fp_line (start -5 -4) (end -4 -5) (layer "F.Fab") (width 0.05) (tstamp 226ebe1a-16b1-40c3-b717-c7c1eb40c129))
  (fp_line (start 5 -5) (end 5 5) (layer "F.Fab") (width 0.05) (tstamp 330f8276-160f-4d0b-ac42-f74abf2b41b8))
  (fp_line (start 5 5) (end -5 5) (layer "F.Fab") (width 0.05) (tstamp 9599b6e2-0d3e-4089-aecc-ba50fda2ae45))
  (fp_line (start -5 -5) (end 5 -5) (layer "F.Fab") (width 0.05) (tstamp 9a10cfab-414d-48ec-bffa-b25d5a617fbf))
  (pad "A1" smd roundrect (at -4.55 -4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp d4a11aaa-e428-40fd-8907-a39396b055bc))
  (pad "A2" smd roundrect (at -3.9 -4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 42f8977e-df60-47e0-8a7d-cc1a76678557))
  (pad "A3" smd roundrect (at -3.25 -4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 71832796-b402-4f2d-95d7-d283f4c51664))
  (pad "A4" smd roundrect (at -2.6 -4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 00b1b2a0-c361-4c83-9d0b-f22945510723))
  (pad "A5" smd roundrect (at -1.95 -4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 44231479-3167-4b5b-95b6-aac3f9c27b33))
  (pad "A6" smd roundrect (at -1.3 -4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp ca471c33-b93d-467f-950e-c23ead9474c0))
  (pad "A7" smd roundrect (at -0.65 -4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp f807828c-82d0-4150-8de4-d52949352e45))
  (pad "A8" smd roundrect (at 0 -4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6f6758c0-9562-4a9c-ab49-691bb47600e0))
  (pad "A9" smd roundrect (at 0.65 -4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 328087b1-ba3e-4afc-84e6-350a193fbc89))
  (pad "A10" smd roundrect (at 1.3 -4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp e1d64a17-5a23-4a8f-b79e-c152c593dfb7))
  (pad "A11" smd roundrect (at 1.95 -4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp b0812c4d-098c-47d0-a7e5-b17b36687252))
  (pad "A12" smd roundrect (at 2.6 -4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp b129dbc4-f788-4581-a902-1bf134f21bd5))
  (pad "A13" smd roundrect (at 3.25 -4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp b231a8b5-26f9-4f63-bf13-ef6a6008e09e))
  (pad "A14" smd roundrect (at 3.9 -4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 89d8d1ae-3f5c-4501-81bb-b41d08ec6221))
  (pad "A15" smd roundrect (at 4.55 -4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 59217f62-f96e-4043-bfde-acc3ba51bf67))
  (pad "B1" smd roundrect (at -4.55 -3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3a9aa55b-b548-4a00-b16c-a486b8d58366))
  (pad "B2" smd roundrect (at -3.9 -3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 104fc769-7fb1-4102-aa68-8e4540b97aac))
  (pad "B3" smd roundrect (at -3.25 -3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp fc908542-291b-4caa-acbe-31f7cde2136c))
  (pad "B4" smd roundrect (at -2.6 -3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3d5ecedd-cbac-4346-be84-d6795ddcdab1))
  (pad "B5" smd roundrect (at -1.95 -3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 88965b52-0bf1-4f09-bfbf-c13c33cbbfe1))
  (pad "B6" smd roundrect (at -1.3 -3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp d4636e7e-f16c-4c8e-8848-311b9cc2ec40))
  (pad "B7" smd roundrect (at -0.65 -3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 83877133-27c7-48dc-96b3-83aa53143cb0))
  (pad "B8" smd roundrect (at 0 -3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp dd1cee7c-a28f-4288-bb82-e0b3781cec20))
  (pad "B9" smd roundrect (at 0.65 -3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3d8ae09e-6675-4878-a27f-f9724ae24f14))
  (pad "B10" smd roundrect (at 1.3 -3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 14625c54-5377-4aa8-9c06-2053c7419839))
  (pad "B11" smd roundrect (at 1.95 -3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp eea6f944-1b63-4b4b-ae0f-0dacd1ee8de6))
  (pad "B12" smd roundrect (at 2.6 -3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 24555128-b814-4bfe-8a33-8822c9f20b74))
  (pad "B13" smd roundrect (at 3.25 -3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp b8ec9ee5-2918-43b0-a418-756c3d2840d3))
  (pad "B14" smd roundrect (at 3.9 -3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp c307478c-8234-4618-8a75-f7e4c692b353))
  (pad "B15" smd roundrect (at 4.55 -3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp d56ac110-8192-4df3-8dc5-1bf8b809229a))
  (pad "C1" smd roundrect (at -4.55 -3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4fa47540-fbc9-4f5f-89e6-a32625d893db))
  (pad "C2" smd roundrect (at -3.9 -3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp c0d842ce-6ddf-457e-a1b6-a5b836e4841f))
  (pad "C3" smd roundrect (at -3.25 -3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7ee88c8b-2fb4-469c-ad35-820671feeb5f))
  (pad "C4" smd roundrect (at -2.6 -3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp b4550135-967e-4909-918b-ac155408b555))
  (pad "C5" smd roundrect (at -1.95 -3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 72a0aa24-b737-4796-9826-7745e8b9a0a4))
  (pad "C6" smd roundrect (at -1.3 -3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3b2f68be-e69b-498b-a585-ddecade5a906))
  (pad "C7" smd roundrect (at -0.65 -3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp c80150ae-9396-4b53-a024-6c04792f58b9))
  (pad "C8" smd roundrect (at 0 -3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 25563148-56c0-4a1a-a646-1df81317160a))
  (pad "C9" smd roundrect (at 0.65 -3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2f6cd025-d417-45ea-b261-6210ce5e8a46))
  (pad "C10" smd roundrect (at 1.3 -3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4a5ce4bc-9014-4e55-897d-4dd78ba83722))
  (pad "C11" smd roundrect (at 1.95 -3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 31ec44a9-520f-4d27-9b7f-7a1295e7e955))
  (pad "C12" smd roundrect (at 2.6 -3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp cb322523-002e-40ed-b71c-c458aec0f070))
  (pad "C13" smd roundrect (at 3.25 -3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp cba94cf0-811e-46d6-9189-707abaf16748))
  (pad "C14" smd roundrect (at 3.9 -3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 87a128f7-0c9a-44ab-81ab-367e694fe3f7))
  (pad "C15" smd roundrect (at 4.55 -3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2a865169-dc24-41da-8208-8183eb2ad234))
  (pad "D1" smd roundrect (at -4.55 -2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 37020c92-f3ff-4e19-9455-e58a77881a36))
  (pad "D2" smd roundrect (at -3.9 -2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp ef0bb2d0-bfa4-49c5-9c99-1593085752bf))
  (pad "D3" smd roundrect (at -3.25 -2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0f22219c-089b-46fe-910e-5fc2e2231af6))
  (pad "D4" smd roundrect (at -2.6 -2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 18d1ee36-c850-446b-8237-6719b57879b8))
  (pad "D5" smd roundrect (at -1.95 -2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 50c26fd3-f2d4-43ac-8fe7-ed560e9adaee))
  (pad "D6" smd roundrect (at -1.3 -2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp be671cd8-30db-46bc-8d7c-9698f13d1d0c))
  (pad "D7" smd roundrect (at -0.65 -2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 421eb145-71b7-4625-8a15-d88e3d37183e))
  (pad "D8" smd roundrect (at 0 -2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 740d88de-bc8b-489b-b141-5f25e5756825))
  (pad "D9" smd roundrect (at 0.65 -2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 46011083-4b65-4c9b-b521-cba343a03805))
  (pad "D10" smd roundrect (at 1.3 -2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 792adfca-9296-459f-998d-c3d5fde35c00))
  (pad "D11" smd roundrect (at 1.95 -2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp db279f04-49d7-4e40-990c-c3bac16a2b77))
  (pad "D12" smd roundrect (at 2.6 -2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 967a1cdf-1537-41b3-9bb0-8bef1875a8e9))
  (pad "D13" smd roundrect (at 3.25 -2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6ce8c2ba-2c44-4467-976f-e2b7ba93aeff))
  (pad "D14" smd roundrect (at 3.9 -2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 93958e06-d2f1-4c03-a300-72208f0aa42d))
  (pad "D15" smd roundrect (at 4.55 -2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp e6af7ff2-3438-4ac8-8619-a11a7e0cfb25))
  (pad "E1" smd roundrect (at -4.55 -1.95) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp fdc06a73-c14e-4f3c-9113-918f172d42eb))
  (pad "E2" smd roundrect (at -3.9 -1.95) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3a027f47-3463-4dc0-879b-744b8a5f381d))
  (pad "E3" smd roundrect (at -3.25 -1.95) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 71dfe985-04cf-4884-b752-35932a9d47f1))
  (pad "E4" smd roundrect (at -2.6 -1.95) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5b6eafea-e4e2-47c3-8d59-4295c4c232d8))
  (pad "E12" smd roundrect (at 2.6 -1.95) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 269d6c18-9653-49ae-a2d4-e19a6bb64adb))
  (pad "E13" smd roundrect (at 3.25 -1.95) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 81f5643e-745d-4356-96be-9f09e619db91))
  (pad "E14" smd roundrect (at 3.9 -1.95) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 26b3fb10-1a8a-4dfa-af4f-b63d7be9d5c6))
  (pad "E15" smd roundrect (at 4.55 -1.95) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 20de0ee8-4ac7-44ba-8593-0c399981a189))
  (pad "F1" smd roundrect (at -4.55 -1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp afa2e069-37f9-4476-bf61-3b9b98dccca2))
  (pad "F2" smd roundrect (at -3.9 -1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp fa8d89ed-ca9b-4981-8dd1-84fef35ddf88))
  (pad "F3" smd roundrect (at -3.25 -1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 816948a9-646b-483b-90da-64fdc2ad73ac))
  (pad "F4" smd roundrect (at -2.6 -1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp f37abe84-b478-4592-95ee-3b5ed590efbb))
  (pad "F6" smd roundrect (at -1.3 -1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6bba952a-b5fc-428f-a1d7-7ffe3bdf4bfa))
  (pad "F7" smd roundrect (at -0.65 -1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 358513b8-6b0b-4c08-bedb-0545bca80f7d))
  (pad "F8" smd roundrect (at 0 -1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9390481a-8f10-451e-b819-8101b04c19be))
  (pad "F9" smd roundrect (at 0.65 -1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 47e5e045-f1a6-4049-8bfe-2e59ef3abe2d))
  (pad "F10" smd roundrect (at 1.3 -1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4d07675e-a111-415a-909f-86f67dae7599))
  (pad "F12" smd roundrect (at 2.6 -1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp dace64a4-9cb8-4cf5-8c4f-57132043b681))
  (pad "F13" smd roundrect (at 3.25 -1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp bda7df60-ce96-4b6e-a34a-ae130deb0ee4))
  (pad "F14" smd roundrect (at 3.9 -1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp caaec61e-6d04-4bbe-8dfc-e16dd9f9a2e0))
  (pad "F15" smd roundrect (at 4.55 -1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp e51f9d78-8a49-4e83-90c6-1b3836afd638))
  (pad "G1" smd roundrect (at -4.55 -0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1d6e9ce7-1737-4052-8bbf-9bf0176bc4aa))
  (pad "G2" smd roundrect (at -3.9 -0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp a3b311bd-cebd-4237-a3cd-55f10f8d819f))
  (pad "G3" smd roundrect (at -3.25 -0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 98f6bffd-bc1f-4835-a1a6-a99ff5ad9fd5))
  (pad "G4" smd roundrect (at -2.6 -0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7a63aefb-9912-49d3-a161-fcf31f3cf57f))
  (pad "G6" smd roundrect (at -1.3 -0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp f4570e0f-cb82-4302-ad96-8f1692eea71b))
  (pad "G7" smd roundrect (at -0.65 -0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9ce9e69d-f24d-48e0-8724-86fcb1d1ec9a))
  (pad "G8" smd roundrect (at 0 -0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp fb47a579-a8b6-47a8-a1c7-59687740f404))
  (pad "G9" smd roundrect (at 0.65 -0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 00cf1435-4993-43ba-bc2a-eb77a11147f4))
  (pad "G10" smd roundrect (at 1.3 -0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0f5d01b3-d7c3-4510-84c8-2744337c8f07))
  (pad "G12" smd roundrect (at 2.6 -0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp a329932c-e9fc-44a2-a13b-e0dd1bbc1b22))
  (pad "G13" smd roundrect (at 3.25 -0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp eac7332e-074a-4fab-9c9c-1500430a93d5))
  (pad "G14" smd roundrect (at 3.9 -0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7087845d-0824-49d3-89e6-e04afa3443fd))
  (pad "G15" smd roundrect (at 4.55 -0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp d3668452-e5d7-4c99-8acb-286b00593fa7))
  (pad "H1" smd roundrect (at -4.55 0) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6848fabb-5703-4f88-9544-9c6d163c646d))
  (pad "H2" smd roundrect (at -3.9 0) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8bd361d5-7dc8-4612-8fc3-ce6d07363564))
  (pad "H3" smd roundrect (at -3.25 0) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0c796941-a362-445e-b5d8-4d36b9ff7b1a))
  (pad "H4" smd roundrect (at -2.6 0) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp d68edd55-58e4-42b5-b9d9-51ed9e45109a))
  (pad "H6" smd roundrect (at -1.3 0) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 97acfa70-f157-4f79-b85d-6bae115d55e6))
  (pad "H7" smd roundrect (at -0.65 0) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 03e7ec5b-286e-40a1-8ad7-8007881ccf46))
  (pad "H8" smd roundrect (at 0 0) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp fc1c46ab-4582-4e50-8749-1c066bc783b7))
  (pad "H9" smd roundrect (at 0.65 0) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5814cf4e-d7cd-4777-b542-77e8ed5b54f4))
  (pad "H10" smd roundrect (at 1.3 0) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 17205062-60f8-4c97-b42b-89ceb6d8972e))
  (pad "H12" smd roundrect (at 2.6 0) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 205fff40-bbae-476c-bae9-381a33d3c072))
  (pad "H13" smd roundrect (at 3.25 0) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5089e697-4a21-4f61-8141-071d0a103fc6))
  (pad "H14" smd roundrect (at 3.9 0) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp cfb11f57-3138-4e94-ab9c-d643368d00b7))
  (pad "H15" smd roundrect (at 4.55 0) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 788d7830-a04d-4943-8b47-c92a17eda4e7))
  (pad "J1" smd roundrect (at -4.55 0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp cd20921d-50d0-4244-96ae-e029e1dfd4f2))
  (pad "J2" smd roundrect (at -3.9 0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp eb72c82b-535a-4500-b10d-d80473b1d0bc))
  (pad "J3" smd roundrect (at -3.25 0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp f291697b-3a02-4cd3-9dc0-a67001efe20a))
  (pad "J4" smd roundrect (at -2.6 0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp d57ed539-3bd8-4284-b777-2c4b7c86cc45))
  (pad "J6" smd roundrect (at -1.3 0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp f5527a44-e5b6-4e93-bd17-5a91c3fda852))
  (pad "J7" smd roundrect (at -0.65 0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9e46f7e6-90cb-42bf-b7bc-d28505f2a50c))
  (pad "J8" smd roundrect (at 0 0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 288682b1-1a17-4365-9add-50ee906dee15))
  (pad "J9" smd roundrect (at 0.65 0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3968f01e-47c7-4d07-87e5-6c56f84056b4))
  (pad "J10" smd roundrect (at 1.3 0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 55cfe3a1-73e6-462c-aebc-8c16f3ac49b7))
  (pad "J12" smd roundrect (at 2.6 0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 65d73c37-4950-46ce-8837-7c22432e9b4c))
  (pad "J13" smd roundrect (at 3.25 0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp d1224bf1-43bb-4555-a8aa-680173ee15c1))
  (pad "J14" smd roundrect (at 3.9 0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 554f4b58-a55d-45e9-8a10-ca61362423a3))
  (pad "J15" smd roundrect (at 4.55 0.65) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp b2aa2ded-ab0a-426e-927a-9608f79a521e))
  (pad "K1" smd roundrect (at -4.55 1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4b136b1d-032d-4edf-9a47-2975d8db72c2))
  (pad "K2" smd roundrect (at -3.9 1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 30b4c19f-977e-4102-9fc3-033d23dc0081))
  (pad "K3" smd roundrect (at -3.25 1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp e7e29171-589b-4434-a381-7bffaf481457))
  (pad "K4" smd roundrect (at -2.6 1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp a04f681a-5e30-4f3c-aa14-2ddde853ea31))
  (pad "K6" smd roundrect (at -1.3 1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp d5d50930-c3d4-41a5-822f-a2784792b2a9))
  (pad "K7" smd roundrect (at -0.65 1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 436dd3f2-9f19-4960-896e-f92271805720))
  (pad "K8" smd roundrect (at 0 1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 15923242-1fa7-4854-ad48-a0f8a17600e2))
  (pad "K9" smd roundrect (at 0.65 1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp e96d0ba0-19f3-40d6-8bd2-8a848c24e9f5))
  (pad "K10" smd roundrect (at 1.3 1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3e9a605a-9ae4-4841-b8f9-f79cdfd81ad2))
  (pad "K12" smd roundrect (at 2.6 1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 01aad36f-aae0-4ec2-84c2-97532e6b6524))
  (pad "K13" smd roundrect (at 3.25 1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp dec8d39b-8239-4c10-9ba4-fe5ed9e4900e))
  (pad "K14" smd roundrect (at 3.9 1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8cf936e7-a3f0-4f3b-ab2d-1d41d55661c7))
  (pad "K15" smd roundrect (at 4.55 1.3) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp f4a62fdd-fad2-4ac8-923e-e7299b3f2aa8))
  (pad "L1" smd roundrect (at -4.55 1.95) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6d79c477-7034-4bc4-bf10-8be3a24265eb))
  (pad "L2" smd roundrect (at -3.9 1.95) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 06476fa9-ad21-4c3d-acd0-6854c2b7e152))
  (pad "L3" smd roundrect (at -3.25 1.95) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 45084710-8897-41e2-93df-858ff964dace))
  (pad "L4" smd roundrect (at -2.6 1.95) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 355cfcac-9e0b-4858-ba51-c48f4d0e097d))
  (pad "L12" smd roundrect (at 2.6 1.95) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp ea6c162b-fb8d-4364-9c76-ea792f593484))
  (pad "L13" smd roundrect (at 3.25 1.95) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1607877a-7669-41fd-90f3-a34e7a5b979b))
  (pad "L14" smd roundrect (at 3.9 1.95) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp b0ba1139-5f4a-4045-a966-743aa58e5227))
  (pad "L15" smd roundrect (at 4.55 1.95) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 59a5fad2-9087-4dae-90c5-a1e75b23b044))
  (pad "M1" smd roundrect (at -4.55 2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp e7f6f82d-ecd4-45db-9282-544570ba71bb))
  (pad "M2" smd roundrect (at -3.9 2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2b1b1375-5aa6-4abc-8152-6f0acf09807c))
  (pad "M3" smd roundrect (at -3.25 2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp f6ea3eed-80f5-4a28-a401-58aedb2c3b52))
  (pad "M4" smd roundrect (at -2.6 2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp f11bce10-cc87-410d-9c8c-9522296a3c69))
  (pad "M5" smd roundrect (at -1.95 2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp e8cd48d4-b24f-4662-9050-9a147849a912))
  (pad "M6" smd roundrect (at -1.3 2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp ffb61734-739f-4ccf-ad01-d8f53c467576))
  (pad "M7" smd roundrect (at -0.65 2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4bddf3ba-54c9-4c64-8fbc-1462b4fecc6b))
  (pad "M8" smd roundrect (at 0 2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1eeff795-66f8-4b30-92b2-d948c2840708))
  (pad "M9" smd roundrect (at 0.65 2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 52aa9b24-3a92-46d3-94d9-17e89d5495a8))
  (pad "M10" smd roundrect (at 1.3 2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp bb615508-c6c1-4bc3-a0d8-1053f2f03f77))
  (pad "M11" smd roundrect (at 1.95 2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6ff37b8b-603c-450a-9dc7-507ff3886fbc))
  (pad "M12" smd roundrect (at 2.6 2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp da3b1a2c-0911-47fc-8b8a-a06f61d6ac7b))
  (pad "M13" smd roundrect (at 3.25 2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4e0c2bd6-175b-405b-adbf-b8190511cbf1))
  (pad "M14" smd roundrect (at 3.9 2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 38f310c5-1bf7-4d7b-80cd-caca5871720e))
  (pad "M15" smd roundrect (at 4.55 2.6) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp f2cc9a98-87a3-44f4-b1a8-b952a8e8afaf))
  (pad "N1" smd roundrect (at -4.55 3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3e304a05-93a8-4b59-9e32-ec6765ed494a))
  (pad "N2" smd roundrect (at -3.9 3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp d8721165-ff77-4640-a7c0-d21fdc549c73))
  (pad "N3" smd roundrect (at -3.25 3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp d3f9ca2d-454e-42fa-b6ff-bc08d5a365d7))
  (pad "N4" smd roundrect (at -2.6 3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp bb94ee10-3b92-4b46-854b-ef9f9e58695b))
  (pad "N5" smd roundrect (at -1.95 3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp fe8dd065-d026-4a2a-abe4-e81f632bd906))
  (pad "N6" smd roundrect (at -1.3 3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 053594cc-4d76-46d4-9c87-d8ff8c10956b))
  (pad "N7" smd roundrect (at -0.65 3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp a87caa54-177b-4010-9f8c-5069a8d70248))
  (pad "N8" smd roundrect (at 0 3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 91e44072-f7c1-41a7-8bef-1cab9fda9bba))
  (pad "N9" smd roundrect (at 0.65 3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp ab339a46-c10a-41ef-855d-2299d6309299))
  (pad "N10" smd roundrect (at 1.3 3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 63206a66-c456-4260-851f-67fc34d96684))
  (pad "N11" smd roundrect (at 1.95 3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp a1af04ae-761d-44e4-9b96-a7e23dac7fec))
  (pad "N12" smd roundrect (at 2.6 3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8d5e3a6d-ef09-4d10-8952-5657ffeb3f2d))
  (pad "N13" smd roundrect (at 3.25 3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8ecbdac2-5365-4c3b-b44d-519b388bafc5))
  (pad "N14" smd roundrect (at 3.9 3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp ca0339fd-5666-40e5-b277-50a2ec8d4143))
  (pad "N15" smd roundrect (at 4.55 3.25) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 58a0e5e5-d3d9-4993-8ff9-ca78bb15827c))
  (pad "P1" smd roundrect (at -4.55 3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4b06d1d2-d168-46eb-92ce-4fba8784a16d))
  (pad "P2" smd roundrect (at -3.9 3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7a59a30a-9226-4f13-89b4-6cc656ce1cce))
  (pad "P3" smd roundrect (at -3.25 3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp d805cdd5-4c09-4ef9-b925-2360944e2a4c))
  (pad "P4" smd roundrect (at -2.6 3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7e86523a-2f43-49c5-bc20-c45a0090e195))
  (pad "P5" smd roundrect (at -1.95 3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp d8a34734-5afe-491a-bf70-50388cf404df))
  (pad "P6" smd roundrect (at -1.3 3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp d28fdb7b-d0e0-4ab7-916b-775b430d24a1))
  (pad "P7" smd roundrect (at -0.65 3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7c134987-a008-4d0c-9f69-f408067dea7e))
  (pad "P8" smd roundrect (at 0 3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp f32548ac-5a03-45f2-bf54-b57e522a1a01))
  (pad "P9" smd roundrect (at 0.65 3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp d647ae88-7ef1-4d89-aef7-1ca3866831b7))
  (pad "P10" smd roundrect (at 1.3 3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 10ab4e36-78e5-4383-ab77-e994f877c329))
  (pad "P11" smd roundrect (at 1.95 3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp b24ba7d3-0fa6-4bc7-b4ce-667f2cb8405b))
  (pad "P12" smd roundrect (at 2.6 3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7ff94dd8-45b1-4ba8-943a-792ad0225e0e))
  (pad "P13" smd roundrect (at 3.25 3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 47afef47-aa0a-4b99-b629-8a5d14e0940f))
  (pad "P14" smd roundrect (at 3.9 3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp f1eb9292-e83d-4cf8-8e47-e1095bf85349))
  (pad "P15" smd roundrect (at 4.55 3.9) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp ae0ebc4c-244a-4247-9ca9-caacf8b7625d))
  (pad "R1" smd roundrect (at -4.55 4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp eb8c850c-3f3c-4159-8265-c371f2896972))
  (pad "R2" smd roundrect (at -3.9 4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 02446149-e1d4-466f-a1a8-42c9a33441f9))
  (pad "R3" smd roundrect (at -3.25 4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp b5046c6b-0226-4df1-a9ab-eea96e644418))
  (pad "R4" smd roundrect (at -2.6 4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7e40cb7a-d764-4273-870c-0bd08baa2784))
  (pad "R5" smd roundrect (at -1.95 4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1b83b912-7c46-4b2b-abab-800d0528ea32))
  (pad "R6" smd roundrect (at -1.3 4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp c5f7b221-a82c-47fb-aa17-f3007f9348e6))
  (pad "R7" smd roundrect (at -0.65 4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3500730b-0b2f-42b3-b5f6-6dad576a81f5))
  (pad "R8" smd roundrect (at 0 4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4ccf7356-67be-4527-b0ef-f808ab28bbd3))
  (pad "R9" smd roundrect (at 0.65 4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 96a979c4-9d95-42b0-bed4-163d9dbff282))
  (pad "R10" smd roundrect (at 1.3 4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp cbac0c71-1b51-44f2-ae3a-ac94a657cdbf))
  (pad "R11" smd roundrect (at 1.95 4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1edbc73e-38c6-4376-ac51-43c35dab52d0))
  (pad "R12" smd roundrect (at 2.6 4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9f7ae9ba-9312-4f50-b9ea-90c9a0257278))
  (pad "R13" smd roundrect (at 3.25 4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp db01c8ac-8c15-4269-a513-fe243acd7e4e))
  (pad "R14" smd roundrect (at 3.9 4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 790bfc6c-b903-4383-ae82-83ea796fdea7))
  (pad "R15" smd roundrect (at 4.55 4.55) (locked) (size 0.274 0.274) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.308) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2b48755b-012f-4d84-8758-8f8baa0c5383))
  (model "${KICAD7_3DMODEL_DIR}/Package_BGA.3dshapes/UFBGA-201_10x10mm_Layout15x15_P0.65mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
