(footprint "3216_B"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(tags "1206 3216")
	(property "Reference" "C2"
		(at 2 0 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "9938f9ab-c6e9-4b61-b41b-9acab13ec249")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
			(justify left)
		)
	)
	(property "Value" "10uF"
		(at 2.05 0.675 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "9e4ab4ac-adf7-44d4-8b37-63ef87171dea")
		(effects
			(font
				(size 0.2 0.2)
				(thickness 0.05)
			)
			(justify left)
		)
	)
	(property "Footprint" "3216_B"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "a1306088-1c8d-4489-8657-de6be24ec49c")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "676328d3-077e-4dc2-8447-5c5a08826ff0")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "de269c1c-077f-46ce-b328-2bd39b69fa8d")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(solder_mask_margin 0.05)
	(solder_paste_margin -0.05)
	(attr smd)
	(fp_line
		(start -0.85 -0.9)
		(end 0.85 -0.9)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "641907f1-6ccf-41b1-8a63-427c98634a6f")
	)
	(fp_line
		(start -0.85 0.9)
		(end 0.85 0.9)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "85838b44-c9da-4ab5-9b9a-1f7dad69d970")
	)
	(fp_line
		(start -2.2 -1.075)
		(end -2.2 1.075)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b6a58964-797f-433f-af11-b2d762c1ede8")
	)
	(fp_line
		(start -2.2 -1.075)
		(end 2.2 -1.075)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "96ae015b-49bb-48d5-9893-222f556f953b")
	)
	(fp_line
		(start 2.2 -1.075)
		(end 2.2 1.075)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "79a21ad8-3167-4bd0-b0f4-2f286d9b4d63")
	)
	(fp_line
		(start 2.2 1.075)
		(end -2.2 1.075)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "3b12b7e7-842e-40e5-a655-eaa012d045ac")
	)
	(fp_rect
		(start -1.6 -0.8)
		(end 1.6 0.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "b1f2bac9-6cdf-48a7-92a4-cb46c9e95e76")
	)
	(pad "1" smd roundrect
		(at -1.525 0)
		(size 0.85 1.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.059)
		(uuid "c8d00ae7-55ab-4592-9c2b-fa8a297f8372")
	)
	(pad "2" smd roundrect
		(at 1.525 0)
		(size 0.85 1.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.059)
		(uuid "e8301d3d-fdb7-4240-b93e-c232a3d2e94f")
	)
	(model "${KICAD7_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
