(module Battery_Retainer_SR44_Keystone_2997 (layer F.Cu) (tedit 54764DCF)
  (solder_mask_margin 0.05)
  (solder_paste_margin -0.1)
  (fp_text reference BT1 (at 5.08 5.08 270) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text value SR44 (at -5.08 5.08 270) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text user "OPEN SIDE" (at 0 -6.35) (layer Cmts.User)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_line (start -7.15 -5.9) (end -7.15 4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.1 7.4) (end -7.15 4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.1 7.4) (end 7.15 4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 7.15 -5.9) (end 7.15 4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -7.15 -5.9) (end 7.15 -5.9) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.1 7.4) (end 4.1 7.4) (layer F.CrtYd) (width 0.05))
  (pad 1 thru_hole oval (at -6.605 0) (size 2.2 3.1) (drill 1.85) (layers *.Cu *.Mask))
  (pad 1 thru_hole oval (at 6.605 0) (size 2.2 3.2) (drill 1.85) (layers *.Cu *.Mask))
  (pad 2 connect circle (at 0 0) (size 10.5 10.5) (layers F.Cu F.Mask))
)
