(module 1P_TH_0.5_8x1.1 (layer F.Cu) (tedit 5861932D)
  (solder_mask_margin 0.01)
  (fp_text reference TP1 (at 0 -1.2) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value TEST_POINT (at 0 1.4) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  (pad 2 connect roundrect (at 0 0.15) (size 0.8 1.1) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
)
