(footprint "11P_4x1.5_P2" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd exclude_from_pos_files exclude_from_bom)
  (fp_text reference "REF**" (at -11.5 0 90 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a8541be1-c6a5-4699-bc8e-5b130fd4c843)
  )
  (fp_text value "11P_4x1.5_P2" (at 0 -2.25 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp d86f51dd-c4c7-4840-88e1-5600b6b68310)
  )
  (fp_text user "${REFERENCE}" (at 0.05 -11.45 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a852d905-035c-4472-b349-d3980b5d0a06)
  )
  (pad "1" connect roundrect (at -10 0) (size 1.5 4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1666666667)
    (thermal_bridge_angle 45) (tstamp 3f76e8fa-7fc4-4aef-aa98-10aced053d2c))
  (pad "2" connect oval (at -8 0) (size 1.5 4) (layers "F.Cu" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 072bdc68-6c94-4e45-853c-3dd4cf42d57d))
  (pad "3" connect oval (at -6 0) (size 1.5 4) (layers "F.Cu" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 6f30194f-0abb-4b24-bc75-3cf76ee4a178))
  (pad "4" connect oval (at -4 0) (size 1.5 4) (layers "F.Cu" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 7555017b-7ab7-449c-8f41-fa3d33f0b625))
  (pad "5" connect oval (at -2 0) (size 1.5 4) (layers "F.Cu" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 27996fa8-828d-4f0b-88a9-2db6ec2df233))
  (pad "6" connect oval (at 0 0) (size 1.5 4) (layers "F.Cu" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 45f897b0-7cef-4744-a790-a4c673935694))
  (pad "7" connect oval (at 2 0) (size 1.5 4) (layers "F.Cu" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 602f4466-da68-4a78-b45e-4db0eba8635f))
  (pad "8" connect oval (at 4 0) (size 1.5 4) (layers "F.Cu" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 73950ad2-564e-4ab0-82ee-9acd7c289d69))
  (pad "9" connect oval (at 6 0) (size 1.5 4) (layers "F.Cu" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 2c219da7-1dc0-4cb1-9ea1-27330f007e5a))
  (pad "10" connect oval (at 8 0) (size 1.5 4) (layers "F.Cu" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 07bf6f27-a157-467d-b148-93cc1a2fbdd2))
  (pad "11" connect oval (at 10 0) (size 1.5 4) (layers "F.Cu" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 90fdb267-4a1c-456d-8a1d-25b2dfa51088))
)
