(module Murata_PVA2xxxxx (layer F.Cu) (tedit 5509F0B6)
  (attr smd)
  (fp_text reference Murata_PVA2xxxxx (at 0 -2.3) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text value VAL** (at 0 2.4) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_line (start 0 0.1) (end 0.1 -0.1) (layer F.SilkS) (width 0.127))
  (fp_line (start 0 -0.5) (end 0 0.1) (layer F.SilkS) (width 0.127))
  (fp_line (start 0 0.1) (end -0.1 -0.1) (layer F.SilkS) (width 0.127))
  (fp_line (start -0.7 0.5) (end -0.5 0.5) (layer F.SilkS) (width 0.127))
  (fp_line (start -0.5 0.5) (end -0.4 0.3) (layer F.SilkS) (width 0.127))
  (fp_line (start -0.4 0.3) (end -0.2 0.7) (layer F.SilkS) (width 0.127))
  (fp_line (start -0.2 0.7) (end 0 0.3) (layer F.SilkS) (width 0.127))
  (fp_line (start 0 0.3) (end 0.2 0.7) (layer F.SilkS) (width 0.127))
  (fp_line (start 0.2 0.7) (end 0.4 0.3) (layer F.SilkS) (width 0.127))
  (fp_line (start 0.4 0.3) (end 0.5 0.5) (layer F.SilkS) (width 0.127))
  (fp_line (start 0.5 0.5) (end 0.7 0.5) (layer F.SilkS) (width 0.127))
  (fp_line (start -1.6 -1.8) (end 1.6 -1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.6 -1.8) (end 1.6 1.95) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.6 1.95) (end -1.6 1.95) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.6 1.95) (end -1.6 -1.8) (layer F.CrtYd) (width 0.05))
  (pad 2 smd rect (at 0 -1.2) (size 1.1 0.7) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -0.9 1.3) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0.9 1.3) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask))
  (model 3D/walter/smd_resistors/trim_murata_pva2a.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
