(footprint "XKB_X05C2016TZ_16S_P0.5_Vertical"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "J34"
		(at 0 -2.075 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "520e9ac4-1e4d-4605-ba8c-c9168034f6e4")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "RGMII"
		(at 0 1.825 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "59649aa5-08d4-409a-9c55-0c8f8961a0c1")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.0625)
			)
		)
	)
	(property "Footprint" "Connector_FFC-FPC:XKB_X05C2022TZ_22S_P0.5_Vertical"
		(at 0.025 -4.225 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "c016e038-f830-4b1d-ad8d-5148f3a6da82")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 1.5 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "49db4f47-d0c0-46ea-8201-2c3f93cda445")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Generic connectable mounting pin connector, single row, 01x20, script generated (kicad-library-utils/schlib/autogen/connector/)"
		(at -0.05 -4.45 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "96216103-005d-448d-8ef7-04518a185657")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_arc
		(start -6.775 -1.35)
		(mid -6.753033 -1.403033)
		(end -6.7 -1.425)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ec739e11-8fde-48be-90e0-f749bca28353")
	)
	(fp_arc
		(start -6.7 1.425)
		(mid -6.753033 1.403033)
		(end -6.775 1.35)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0ebe127e-7f1f-4a14-b047-00a6019ae2e4")
	)
	(fp_arc
		(start 6.7 -1.425)
		(mid 6.753033 -1.403033)
		(end 6.775 -1.35)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "32b2d66d-fcd8-47c7-baee-ba672a74619d")
	)
	(fp_arc
		(start 6.775 1.35)
		(mid 6.753033 1.403033)
		(end 6.7 1.425)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "46e9cb66-decb-40e9-8cdc-83efd19a7f19")
	)
	(fp_poly
		(pts
			(xy -3.575 2) (xy -3.925 2) (xy -3.75 1.65)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "3e3fa2a2-d495-4247-a21c-f17e184f4f90")
	)
	(fp_poly
		(pts
			(xy -5.7 -1.35) (xy -6.7 -1.35) (xy -6.7 1.35) (xy -5.7 1.35) (xy -5.7 1.5) (xy -6.7 1.5) (xy -6.85 1.35)
			(xy -6.85 -1.35) (xy -6.7 -1.5) (xy -5.7 -1.5)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "bb46a466-fa92-440b-80c2-3b8320f78c8e")
	)
	(fp_poly
		(pts
			(xy 5.7 1.35) (xy 6.7 1.35) (xy 6.7 -1.35) (xy 5.7 -1.35) (xy 5.7 -1.5) (xy 6.7 -1.5) (xy 6.85 -1.35)
			(xy 6.85 1.35) (xy 6.7 1.5) (xy 5.7 1.5)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "b3851921-f7a7-43a5-afe0-78a3bc2f9168")
	)
	(fp_line
		(start -7.15 1.1)
		(end -7.15 -1.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "15959061-c3ed-4eee-ab89-e1b31129d71e")
	)
	(fp_line
		(start -6.45 -1.8)
		(end 6.45 -1.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9560e49e-23fa-45b9-a1f8-828e893b93bc")
	)
	(fp_line
		(start 6.45 1.8)
		(end -6.45 1.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "bcba9b27-1950-4895-866c-94d513205b8e")
	)
	(fp_line
		(start 7.15 -1.1)
		(end 7.15 1.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "56bde811-423b-4961-be26-4155a9930c3c")
	)
	(fp_arc
		(start -7.15 -1.1)
		(mid -6.944975 -1.594975)
		(end -6.45 -1.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ad45b82f-40a0-40a2-b03f-364b7ee857f4")
	)
	(fp_arc
		(start -6.45 1.8)
		(mid -6.944975 1.594975)
		(end -7.15 1.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e7a3e0e3-7d69-4c47-98eb-edd85c794cc7")
	)
	(fp_arc
		(start 6.45 -1.8)
		(mid 6.944975 -1.594975)
		(end 7.15 -1.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e032eada-5afe-4660-b285-1eaba7830e7a")
	)
	(fp_arc
		(start 7.15 1.1)
		(mid 6.944975 1.594975)
		(end 6.45 1.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "5f7fd1e4-cc93-4b3f-9f58-2fe729fb53bf")
	)
	(fp_line
		(start -6.8 -1)
		(end -6 -1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "a9128df3-ce48-466a-8369-ddb9e8639c7a")
	)
	(fp_line
		(start -6.8 1)
		(end -6.8 -1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "c5d80450-65ff-41da-9568-6d5cd2cb267b")
	)
	(fp_line
		(start -6 1)
		(end -6.8 1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "504ea073-e208-473f-8f17-22e5c8233c95")
	)
	(fp_line
		(start 6 -1)
		(end 6.8 -1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "7c06f56f-d362-48a4-aa66-5da907fe184f")
	)
	(fp_line
		(start 6.8 -1)
		(end 6.8 1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "73a7fd40-713b-4866-8abe-b90351d1375b")
	)
	(fp_line
		(start 6.8 1)
		(end 6 1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "4228e33e-0fc9-40ea-8b53-050c3431b3a2")
	)
	(fp_rect
		(start -5.75 -1)
		(end 5.75 1)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "4fd57854-4fc1-4136-af59-4f804a14476d")
	)
	(fp_text user "${REFERENCE}"
		(at 0.05 -3.15 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "351948f0-3dea-4cd6-a743-2aa72a96ccb2")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.0625)
			)
		)
	)
	(pad "1" smd roundrect
		(at -3.75 0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "b0849725-6b3f-4a30-87f5-481b78014733")
	)
	(pad "2" smd roundrect
		(at -3.25 -0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "75015af4-d263-420b-b715-5c811a0edb26")
	)
	(pad "3" smd roundrect
		(at -2.75 0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "08808bb1-de93-4d20-9e4b-6a8214aaed95")
	)
	(pad "4" smd roundrect
		(at -2.25 -0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "bff227a5-f232-49df-99df-190f128904a9")
	)
	(pad "5" smd roundrect
		(at -1.75 0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "443207e2-5b90-4434-b736-8dbf1e3e6182")
	)
	(pad "6" smd roundrect
		(at -1.25 -0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "ee2971a1-afd9-47a2-a8a5-5e778aed1cab")
	)
	(pad "7" smd roundrect
		(at -0.75 0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "583ea84f-ac2e-4532-8cc1-bcd3b4b22085")
	)
	(pad "8" smd roundrect
		(at -0.25 -0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "032df448-a44d-41dd-8a5a-02bde75bec1d")
	)
	(pad "9" smd roundrect
		(at 0.25 0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "688af42b-ca4f-4b54-840d-f7e09ab1e37d")
	)
	(pad "10" smd roundrect
		(at 0.75 -0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "85f8cf42-e740-400b-b2e9-f6004438dde5")
	)
	(pad "11" smd roundrect
		(at 1.25 0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "ca6822ed-084c-4599-b50d-69f85d5dd357")
	)
	(pad "12" smd roundrect
		(at 1.75 -0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "a3dc07e6-bb0c-4339-8cf0-60be76522f57")
	)
	(pad "13" smd roundrect
		(at 2.25 0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "23ed40e0-d930-4e21-805d-203aa1eff930")
	)
	(pad "14" smd roundrect
		(at 2.75 -0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "b474ce6f-7207-4318-994a-df0c76364303")
	)
	(pad "15" smd roundrect
		(at 3.25 0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "6eb68ac1-a258-4e33-a529-db10f0c0e0ff")
	)
	(pad "16" smd roundrect
		(at 3.75 -0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "91d83112-5d63-4d89-9d6f-d0948bbf78ea")
	)
	(pad "MP" smd roundrect
		(at -5.55 0)
		(size 2 2.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "b9a218ee-5453-4f55-b8ba-a786b8877312")
	)
	(pad "MP" smd roundrect
		(at 5.55 0)
		(size 2 2.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "744a62d8-b9bb-4565-8ce2-ab381ae10ad8")
	)
	(model "${KICAD7_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/X05C2016XZ.stp"
		(hide yes)
		(offset
			(xyz 0 0 4.4)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${KICAD7_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/FPC-SMD_16P-P0.50_X05C2016TZ.step"
		(offset
			(xyz 0 2.95 2.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
