(footprint "Arc_Ri0.9_0.15-0.15_x12_90deg" (version 20221019) (generator pcbnew)
  (layer "F.Cu")
  (zone_connect 0)
  (attr board_only exclude_from_pos_files exclude_from_bom)
  (fp_text reference "REF**" (at 0 -8.075 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2c79dc91-7d87-4312-a8b9-19715fd00ffa)
  )
  (fp_text value "Arc_Ri0.9_0.15-0.15_x12_90deg" (at 0 -6.575 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 5beec144-4cc1-474b-a704-c5bb50798690)
  )
  (fp_text user "${REFERENCE}" (at 0 -5.075 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 329fd6c7-7418-4566-b934-69bde1aafa29)
  )
  (pad "1" smd custom (at -0.975 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 0.285570888344 -0.689429111656) (end 0.975 -0.975) (width 0.15))
    ))
  (pad "1" smd custom (at 0 -0.975) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -0.975 0.975) (mid -0.689429111656 0.285570888344) (end 0 0) (width 0.15))
    ))
  (pad "2" smd custom (at -1.275 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 0.373438853988 -0.901561146012) (end 1.275 -1.275) (width 0.15))
    ))
  (pad "2" smd custom (at 0 -1.275) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -1.275 1.275) (mid -0.901561146012 0.373438853988) (end 0 0) (width 0.15))
    ))
  (pad "3" smd custom (at -1.575 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 0.461306819632 -1.11369318037) (end 1.575 -1.575) (width 0.15))
    ))
  (pad "3" smd custom (at 0 -1.575) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -1.575 1.575) (mid -1.11369318037 0.461306819632) (end 0 0) (width 0.15))
    ))
  (pad "4" smd custom (at -1.875 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 0.549174785276 -1.32582521472) (end 1.875 -1.875) (width 0.15))
    ))
  (pad "4" smd custom (at 0 -1.875) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -1.875 1.875) (mid -1.32582521472 0.549174785276) (end 0 0) (width 0.15))
    ))
  (pad "5" smd custom (at -2.175 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 0.63704275092 -1.53795724908) (end 2.175 -2.175) (width 0.15))
    ))
  (pad "5" smd custom (at 0 -2.175) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -2.175 2.175) (mid -1.53795724908 0.63704275092) (end 0 0) (width 0.15))
    ))
  (pad "6" smd custom (at -2.475 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 0.724910716565 -1.75008928344) (end 2.475 -2.475) (width 0.15))
    ))
  (pad "6" smd custom (at 0 -2.475) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -2.475 2.475) (mid -1.75008928344 0.724910716565) (end 0 0) (width 0.15))
    ))
  (pad "7" smd custom (at -2.775 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 0.812778682209 -1.96222131779) (end 2.775 -2.775) (width 0.15))
    ))
  (pad "7" smd custom (at 0 -2.775) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -2.775 2.775) (mid -1.96222131779 0.812778682209) (end 0 0) (width 0.15))
    ))
  (pad "8" smd custom (at -3.075 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 0.900646647853 -2.17435335215) (end 3.075 -3.075) (width 0.15))
    ))
  (pad "8" smd custom (at 0 -3.075) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -3.075 3.075) (mid -2.17435335215 0.900646647853) (end 0 0) (width 0.15))
    ))
  (pad "9" smd custom (at -3.375 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 0.988514613497 -2.3864853865) (end 3.375 -3.375) (width 0.15))
    ))
  (pad "9" smd custom (at 0 -3.375) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -3.375 3.375) (mid -2.3864853865 0.988514613497) (end 0 0) (width 0.15))
    ))
  (pad "10" smd custom (at -3.675 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 1.07638257914 -2.59861742086) (end 3.675 -3.675) (width 0.15))
    ))
  (pad "10" smd custom (at 0 -3.675) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -3.675 3.675) (mid -2.59861742086 1.07638257914) (end 0 0) (width 0.15))
    ))
  (pad "11" smd custom (at -3.975 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 1.16425054479 -2.81074945521) (end 3.975 -3.975) (width 0.15))
    ))
  (pad "11" smd custom (at 0 -3.975) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -3.975 3.975) (mid -2.81074945521 1.16425054479) (end 0 0) (width 0.15))
    ))
  (pad "12" smd custom (at -4.275 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 1.25211851043 -3.02288148957) (end 4.275 -4.275) (width 0.15))
    ))
  (pad "12" smd custom (at 0 -4.275) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -4.275 4.275) (mid -3.02288148957 1.25211851043) (end 0 0) (width 0.15))
    ))
)

