(footprint "3P_6x3.75_P8" (version 20220815) (generator pcbnew)
  (layer "F.Cu")
  (property "Dielectric" "")
  (property "Footprint_Density" "")
  (property "Footprint_Library" "")
  (property "JLCPCB Part" "")
  (property "LCSC" "")
  (property "MFG" "")
  (property "MPN" "DO NOT POPULATE")
  (property "MPN_ALT1" "")
  (property "Mouser" "")
  (property "Note" "")
  (property "Package" "")
  (property "Sheetfile" "File: AK80 Controller v1.kicad_sch")
  (property "Sheetname" "")
  (property "Spice_Model" "")
  (property "Spice_Netlist_Enabled" "")
  (property "Spice_Primitive" "")
  (property "Tolerance" "")
  (property "USD_per_1" "")
  (property "USD_per_1000" "")
  (property "Voltage" "")
  (property "exclude_from_bom" "")
  (property "ki_description" "Generic screw terminal, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
  (property "ki_keywords" "screw terminal")
  (attr exclude_from_pos_files exclude_from_bom)
  (fp_text reference "J4" (at 0 -7.5) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 9af85132-a065-4bc1-989f-e61cba64a625)
  )
  (fp_text value "M1" (at 2.5 0 -90) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05)))
    (tstamp 34a7740a-1ebd-44e4-ae94-1cd13e67ee19)
  )
  (pad "1" connect roundrect (at 0 -8) (size 6 3.75) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.167) (tstamp 9499aed9-9cc2-4f52-8388-ce3dcb8fe883))
  (pad "2" connect roundrect (at 0 0) (size 6 3.75) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.167) (tstamp b9fc73d2-d6c3-4a87-9e6d-30e2fa57347b))
  (pad "3" connect roundrect (at 0 8) (size 6 3.75) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.167) (tstamp 07a8f978-56d8-4b5a-88b2-c9ced5ca6689))
)
