(module Program_Connector_6P_board_edge_tilt (layer F.Cu) (tedit 5478B595)
  (solder_mask_margin -0.01)
  (attr virtual)
  (fp_text reference Test-pads-6P_board_edge (at 0.75 0 90) (layer Cmts.User)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text value VAL** (at -3.9 0 90) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_arc (start -2 0) (end -2 1.3) (angle 180) (layer Dwgs.User) (width 0.05))
  (fp_line (start 0 1.3) (end -2 1.3) (layer Dwgs.User) (width 0.05))
  (fp_line (start 0 -1.3) (end -2 -1.3) (layer Dwgs.User) (width 0.05))
  (fp_text user "CUT OUT" (at -1.5 0) (layer Cmts.User)
    (effects (font (size 0.45 0.45) (thickness 0.1125)))
  )
  (fp_line (start 0 -4.8) (end 0 4.8) (layer F.CrtYd) (width 0.05))
  (fp_text user RST (at -2.6 4.4) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text user SCK (at -2.6 3.3) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text user SIO (at -2.6 2.2) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text user VCC (at -2.6 -2.2) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text user GND (at -2.6 -3.3) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text user GND (at -2.6 -4.4) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (pad 1 connect oval (at -1 -4.4) (size 1 0.8) (layers F.Cu F.Mask))
  (pad 2 connect oval (at -1 -3.3) (size 1 0.8) (layers F.Cu F.Mask))
  (pad 3 connect oval (at -1 -2.2) (size 1 0.8) (layers F.Cu F.Mask))
  (pad 4 connect oval (at -1 2.2) (size 1 0.8) (layers F.Cu F.Mask))
  (pad 5 connect oval (at -1 3.3) (size 1 0.8) (layers F.Cu F.Mask))
  (pad 6 connect oval (at -1 4.4) (size 1 0.8) (layers F.Cu F.Mask))
)
