(footprint "1P_6.5x2.1" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr exclude_from_pos_files exclude_from_bom)
  (fp_text reference "REF**" (at 3.6 0 90 unlocked) (layer "F.SilkS") hide
      (effects (font (size 0.25 0.25) (thickness 0.05) bold))
    (tstamp 51b0b778-dcee-4a39-8265-5c0115d61865)
  )
  (fp_text value "1P_6.5x2.1" (at -3.85 0 90 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 69e043fe-e40d-411e-a56a-dcb6d396e455)
  )
  (fp_text user "${REFERENCE}" (at 3.6 0 90 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05) bold))
    (tstamp b3d98023-09e4-41af-81fe-9e9aff16b0a6)
  )
  (fp_line (start -3.4 -0.35) (end -3.4 0.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fec97153-b0b5-442b-8b56-fe44971e3742))
  (fp_line (start 3.4 -1.2) (end -2.55 -1.2)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e88c5bdc-c1c9-4695-bc22-f4416f4e3f33))
  (fp_line (start 3.4 -1.2) (end 3.4 1.2)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 34eb84c3-eb81-4b83-9fb1-9aa9228994a6))
  (fp_line (start 3.4 1.2) (end -2.55 1.2)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9147af03-66ad-4521-bd43-0e0550d0a336))
  (fp_arc (start -3.4 -0.35) (mid -3.151041 -0.951041) (end -2.55 -1.2)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a255d091-aec3-4c57-ab59-2fcae5147886))
  (fp_arc (start -2.55 1.2) (mid -3.151041 0.951041) (end -3.4 0.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5ef17a17-adc2-4e06-9fd6-e9aee713a588))
  (pad "1" smd roundrect (at 0 0) (size 6.5 2.1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp 297b4bc9-e93f-4426-8678-c3d5a23c5388))
)
