(footprint "LQFP-64_10x10mm_P0.5mm" (version 20210108) (generator pcbnew) (layer "F.Cu")
  (tedit 6005E797)
  (descr "LQFP, 64 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ad7606_7606-6_7606-4.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
  (tags "LQFP QFP")
  (property "Sheet file" "BrushedMotorController18V15A.kicad_sch")
  (property "Sheet name" "")
  (attr smd)
  (fp_text reference "U1" (at 0 -7.4) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e1fc39ab-8c48-449a-b2b1-e000a606be9c)
  )
  (fp_text value "STM32F405RGTx" (at 0 7.4) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c0fedb35-3fc9-4ed1-a53e-5e7f7b452136)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ab1e8071-6034-4570-9992-d82ad7167919)
  )
  (fp_line (start 4.16 -5.11) (end 5.11 -5.11) (layer "F.SilkS") (width 0.12) (tstamp 36cf28eb-5473-4679-90d2-09607dda3b89))
  (fp_line (start 4.16 5.11) (end 5.11 5.11) (layer "F.SilkS") (width 0.12) (tstamp 4fa78d4f-68cc-4442-a0e5-57975ae3b238))
  (fp_line (start -4.16 -5.11) (end -5.11 -5.11) (layer "F.SilkS") (width 0.12) (tstamp 8fab45ff-cde3-4df4-922d-d05b99642ed9))
  (fp_line (start -5.11 -4.16) (end -6.45 -4.16) (layer "F.SilkS") (width 0.12) (tstamp ac4fa75d-beeb-4657-b86a-37168bce83ed))
  (fp_line (start 5.11 5.11) (end 5.11 4.16) (layer "F.SilkS") (width 0.12) (tstamp ad8b35ab-4992-433d-a5ab-03082a9f847d))
  (fp_line (start -5.11 5.11) (end -5.11 4.16) (layer "F.SilkS") (width 0.12) (tstamp dd15dffb-f885-4c89-ba02-ff7cd07ab65b))
  (fp_line (start -5.11 -5.11) (end -5.11 -4.16) (layer "F.SilkS") (width 0.12) (tstamp defd574b-4329-46ce-b124-fb309f5864cd))
  (fp_line (start 5.11 -5.11) (end 5.11 -4.16) (layer "F.SilkS") (width 0.12) (tstamp e2ee836e-a76d-4476-86f3-9e096380e066))
  (fp_line (start -4.16 5.11) (end -5.11 5.11) (layer "F.SilkS") (width 0.12) (tstamp f5204fed-ab40-4fbd-800a-3cd3efc8e05a))
  (fp_line (start 4.15 5.25) (end 5.25 5.25) (layer "F.CrtYd") (width 0.05) (tstamp 0a7b6dc1-9091-46fd-83f4-8dd04b37e255))
  (fp_line (start -4.15 -5.25) (end -5.25 -5.25) (layer "F.CrtYd") (width 0.05) (tstamp 0b014002-6243-4a68-a04d-4660b3c63805))
  (fp_line (start -5.25 4.15) (end -6.7 4.15) (layer "F.CrtYd") (width 0.05) (tstamp 16e6af73-28b0-4eae-a97f-44d590445f81))
  (fp_line (start -6.7 4.15) (end -6.7 0) (layer "F.CrtYd") (width 0.05) (tstamp 462a77f3-c4c0-4db4-a07f-f8c274ab818d))
  (fp_line (start 5.25 -4.15) (end 6.7 -4.15) (layer "F.CrtYd") (width 0.05) (tstamp 5775d908-f745-445a-907d-3c2737d9e684))
  (fp_line (start 0 6.7) (end -4.15 6.7) (layer "F.CrtYd") (width 0.05) (tstamp 604a3fd6-7d56-4df3-8a63-75e5484d1de4))
  (fp_line (start 4.15 6.7) (end 4.15 5.25) (layer "F.CrtYd") (width 0.05) (tstamp 6087540a-e5a7-468d-8bb3-2975bd5cffaa))
  (fp_line (start 4.15 -6.7) (end 4.15 -5.25) (layer "F.CrtYd") (width 0.05) (tstamp 6a7164bb-d0f1-4959-b5fc-00ff43771f36))
  (fp_line (start -5.25 -5.25) (end -5.25 -4.15) (layer "F.CrtYd") (width 0.05) (tstamp 7153640e-b839-4cc6-b0d5-e4f7e8b61510))
  (fp_line (start -6.7 -4.15) (end -6.7 0) (layer "F.CrtYd") (width 0.05) (tstamp 7a2329a6-4104-4a47-a32b-8d9aacad51e7))
  (fp_line (start 5.25 5.25) (end 5.25 4.15) (layer "F.CrtYd") (width 0.05) (tstamp 824a7141-8586-475c-873c-c917d2d77b5e))
  (fp_line (start -4.15 5.25) (end -5.25 5.25) (layer "F.CrtYd") (width 0.05) (tstamp 84019f07-5d27-4dcd-a8a1-be96d392530d))
  (fp_line (start 6.7 4.15) (end 6.7 0) (layer "F.CrtYd") (width 0.05) (tstamp 875922e6-73fb-463b-a7f9-fa833d991ad3))
  (fp_line (start -4.15 -6.7) (end -4.15 -5.25) (layer "F.CrtYd") (width 0.05) (tstamp 9b3ecfc7-d80d-4bd1-8441-2b21f90a1b59))
  (fp_line (start -5.25 -4.15) (end -6.7 -4.15) (layer "F.CrtYd") (width 0.05) (tstamp a3d92519-3af8-41b9-800f-3b83f04a952b))
  (fp_line (start 5.25 -5.25) (end 5.25 -4.15) (layer "F.CrtYd") (width 0.05) (tstamp adf3442b-4883-42b4-91a3-2faba6640ad8))
  (fp_line (start 5.25 4.15) (end 6.7 4.15) (layer "F.CrtYd") (width 0.05) (tstamp b33b8ec8-4b4d-4ed9-a5e2-bc5261e497ca))
  (fp_line (start 4.15 -5.25) (end 5.25 -5.25) (layer "F.CrtYd") (width 0.05) (tstamp b3eb69da-d7c4-4e4b-a4d4-4c259de7ae53))
  (fp_line (start -4.15 6.7) (end -4.15 5.25) (layer "F.CrtYd") (width 0.05) (tstamp bb4b8fef-b713-44d8-bcbd-0a32d038c08f))
  (fp_line (start 0 -6.7) (end 4.15 -6.7) (layer "F.CrtYd") (width 0.05) (tstamp d90fc061-12e1-4d29-838e-a44c894921de))
  (fp_line (start 6.7 -4.15) (end 6.7 0) (layer "F.CrtYd") (width 0.05) (tstamp dffb5f8d-487e-4e73-8dcb-605c4369dbba))
  (fp_line (start 0 -6.7) (end -4.15 -6.7) (layer "F.CrtYd") (width 0.05) (tstamp e86d11e6-daf3-41aa-9ec3-345f4a0a6080))
  (fp_line (start -5.25 5.25) (end -5.25 4.15) (layer "F.CrtYd") (width 0.05) (tstamp e95dbbe6-552e-473e-9034-98daefd44545))
  (fp_line (start 0 6.7) (end 4.15 6.7) (layer "F.CrtYd") (width 0.05) (tstamp ef25db6b-c6a6-4665-b519-0f24380b68b7))
  (fp_line (start -5 5) (end -5 -4) (layer "F.Fab") (width 0.1) (tstamp 38847c28-eb71-4b00-a99c-40a5880852fc))
  (fp_line (start 5 5) (end -5 5) (layer "F.Fab") (width 0.1) (tstamp 457a51c1-ef8c-430f-a2d5-4b0ac05dd5de))
  (fp_line (start -4 -5) (end 5 -5) (layer "F.Fab") (width 0.1) (tstamp 47bf0b37-68e9-425f-b493-06a5dee041a4))
  (fp_line (start -5 -4) (end -4 -5) (layer "F.Fab") (width 0.1) (tstamp 487038f2-78ed-4b01-b2b8-579d223208a0))
  (fp_line (start 5 -5) (end 5 5) (layer "F.Fab") (width 0.1) (tstamp c021a2af-d102-4336-9f38-9f6b2d239302))
  (pad "1" smd roundrect (at -5.675 -3.75) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a449a526-8b4a-42b1-b2fb-4e5a224530d2))
  (pad "2" smd roundrect (at -5.675 -3.25) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 548b73fc-500c-4888-b1b9-b46194e2caff))
  (pad "3" smd roundrect (at -5.675 -2.75) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 41a7cf46-280b-49ec-b0e0-d785de450c01))
  (pad "4" smd roundrect (at -5.675 -2.25) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 59213433-472d-4d19-9a86-24f01028b14c))
  (pad "5" smd roundrect (at -5.675 -1.75) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 99de8aba-2541-48a7-9265-a48bc37f357e))
  (pad "6" smd roundrect (at -5.675 -1.25) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 078f43a6-5c3b-4698-86ea-826d7d009edf))
  (pad "7" smd roundrect (at -5.675 -0.75) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 65c6471b-bb2b-4eda-b9a4-5dcb767bfa66))
  (pad "8" smd roundrect (at -5.675 -0.25) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 42a565f3-cbc1-45cd-92b0-dcb248254192))
  (pad "9" smd roundrect (at -5.675 0.25) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 088d120b-75a1-4059-b14c-e64dd1851689))
  (pad "10" smd roundrect (at -5.675 0.75) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2701b80d-64f2-4570-809b-d697bcc09c0b))
  (pad "11" smd roundrect (at -5.675 1.25) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 3fdff2c7-1e98-4a63-a8a8-4f8bb12c7c61))
  (pad "12" smd roundrect (at -5.675 1.75) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 60dd3ef5-9748-4535-89f5-c1f2cfce8a62))
  (pad "13" smd roundrect (at -5.675 2.25) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 6dd7e670-9c2b-4919-a74e-52440c4b7c06))
  (pad "14" smd roundrect (at -5.675 2.75) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4c359b92-2089-4713-bcbe-646348f6a9ba))
  (pad "15" smd roundrect (at -5.675 3.25) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 84e2d0f3-6584-41eb-9874-d609c33d59a6))
  (pad "16" smd roundrect (at -5.675 3.75) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d7b7e9c7-3467-4b3d-93a1-4ce85d421a08))
  (pad "17" smd roundrect (at -3.75 5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 29119672-6a2d-4b38-98d2-01c7e2717f1c))
  (pad "18" smd roundrect (at -3.25 5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 121e3e9b-b8a2-4963-85dd-0a65dcdee283))
  (pad "19" smd roundrect (at -2.75 5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 0edb58ff-421f-4255-8b09-c82d1debb1a8))
  (pad "20" smd roundrect (at -2.25 5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 35fae5ab-2530-49b2-b968-13d35eeb380b))
  (pad "21" smd roundrect (at -1.75 5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 3d7ebd37-6996-4975-97f6-cebe64e7b6f0))
  (pad "22" smd roundrect (at -1.25 5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 248e2e15-dd18-4c51-b1d6-d39efd400651))
  (pad "23" smd roundrect (at -0.75 5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp fcf9d8b9-8769-444f-9454-a0c7d42aa266))
  (pad "24" smd roundrect (at -0.25 5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 92042f87-7ace-4c19-8448-1cff07d42787))
  (pad "25" smd roundrect (at 0.25 5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 09cae79f-3958-4546-8b39-fcc976861984))
  (pad "26" smd roundrect (at 0.75 5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9486b44d-d347-4414-b979-f19346b2190e))
  (pad "27" smd roundrect (at 1.25 5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1b4e5047-69ea-49b3-aa5e-773f61a76861))
  (pad "28" smd roundrect (at 1.75 5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 61ff2117-eb3d-410b-a664-daeef46df4e8))
  (pad "29" smd roundrect (at 2.25 5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5566c6b2-69de-4e41-bfff-184be829b75e))
  (pad "30" smd roundrect (at 2.75 5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f897ad5a-d9c8-4702-985b-e622a4da4420))
  (pad "31" smd roundrect (at 3.25 5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ecac30f3-bde6-4be5-ae3a-24f263edb395))
  (pad "32" smd roundrect (at 3.75 5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e2b3b648-9e57-4b07-83c2-4d8f26f0dfb8))
  (pad "33" smd roundrect (at 5.675 3.75) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 79fb748f-ee0f-4b92-9687-46b38d59d1c6))
  (pad "34" smd roundrect (at 5.675 3.25) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5602f440-42d9-46f1-bd2b-722f5cb0b064))
  (pad "35" smd roundrect (at 5.675 2.75) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 110709f4-423a-4b19-bfa6-368f42150206))
  (pad "36" smd roundrect (at 5.675 2.25) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp cccdd618-f2fb-4e27-b0c6-e596960b022b))
  (pad "37" smd roundrect (at 5.675 1.75) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 3e57aa59-d8df-4801-8482-4d1b32a24bb9))
  (pad "38" smd roundrect (at 5.675 1.25) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 761002ed-baa5-4157-b326-b096d75d00dd))
  (pad "39" smd roundrect (at 5.675 0.75) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f4308256-45a2-4c59-ac3e-b8f7950c0af8))
  (pad "40" smd roundrect (at 5.675 0.25) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8c5d4027-9164-4334-ae73-f446104f9650))
  (pad "41" smd roundrect (at 5.675 -0.25) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 7c87632b-e324-476c-a2bf-b37f6454c811))
  (pad "42" smd roundrect (at 5.675 -0.75) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 93acfa68-47b3-4bfe-a316-5e27335965b4))
  (pad "43" smd roundrect (at 5.675 -1.25) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 41f8f2f5-5e1f-43a4-a3f9-eb5b8f30957e))
  (pad "44" smd roundrect (at 5.675 -1.75) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 063ab033-b056-458c-8107-cf7f26d072aa))
  (pad "45" smd roundrect (at 5.675 -2.25) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ab589c0f-e439-42f7-b9c5-b34903a668b9))
  (pad "46" smd roundrect (at 5.675 -2.75) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a84754a6-97e1-4333-ae41-2c8b0f3059f9))
  (pad "47" smd roundrect (at 5.675 -3.25) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 683ef652-dd68-4a21-8504-43934f366f4f))
  (pad "48" smd roundrect (at 5.675 -3.75) (locked) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 7c9deeba-4a99-44c6-8cec-97209510d1d1))
  (pad "49" smd roundrect (at 3.75 -5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f3a0d76f-1917-4e8b-ba59-0106373f92ca))
  (pad "50" smd roundrect (at 3.25 -5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c29bc552-fdc3-44ec-952f-eb0279dab723))
  (pad "51" smd roundrect (at 2.75 -5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a25e7559-61d3-454c-86ba-e8ba6609958c))
  (pad "52" smd roundrect (at 2.25 -5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8ceed8f4-50c3-45d8-9850-daba32daa266))
  (pad "53" smd roundrect (at 1.75 -5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5eefa5a1-71ea-44ba-8cb0-ec72c42fa138))
  (pad "54" smd roundrect (at 1.25 -5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 7d25959d-7809-48fa-915b-79d84b882fea))
  (pad "55" smd roundrect (at 0.75 -5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9945b258-1a1c-41ed-a0c4-ddaa38554b51))
  (pad "56" smd roundrect (at 0.25 -5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 6f353d20-f376-4aa8-adc5-bd80b0fb91ac))
  (pad "57" smd roundrect (at -0.25 -5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 63a0be28-19ac-425c-aefe-0781e61604a6))
  (pad "58" smd roundrect (at -0.75 -5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 61f30d86-d474-4a1b-ac9d-a19d8bee74d8))
  (pad "59" smd roundrect (at -1.25 -5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9c233b36-3018-40ea-90b7-f43fff803fc3))
  (pad "60" smd roundrect (at -1.75 -5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ddc1ee84-611c-433d-93d4-231d4e86f592))
  (pad "61" smd roundrect (at -2.25 -5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 3ff4d9f1-fef5-4135-ba47-bb12a04439b5))
  (pad "62" smd roundrect (at -2.75 -5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c014fb11-3971-4e5c-910d-2bf1cb4e4769))
  (pad "63" smd roundrect (at -3.25 -5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 72d3bdab-71e4-4ba5-884f-5e87372ade4c))
  (pad "64" smd roundrect (at -3.75 -5.675) (locked) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 92409bcd-0ea8-4d2a-8a71-a12b9e408902))
  (model "${KICAD7_3DMODEL_DIR}/Package_QFP.3dshapes/LQFP-64_10x10mm_P0.5mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
