(module Knowles_Receiver_2403_260_00106 (layer F.Cu) (tedit 5422F038)
  (fp_text reference Knowles_Receiver_2403_260_00106 (at 0 1.1) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text value VAL** (at 0 -1.6) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.127)))
  )
  (fp_text user + (at 3.9 -2.3) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.15)))
  )
  (fp_text user - (at -3.9 -2.3) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.15)))
  )
  (fp_line (start -6.1 -3.2) (end -6.1 3.2) (layer F.SilkS) (width 0.127))
  (fp_line (start -6.1 3.2) (end 6.1 3.2) (layer F.SilkS) (width 0.127))
  (fp_line (start 6.1 3.2) (end 6.1 -3.2) (layer F.SilkS) (width 0.127))
  (fp_line (start -6.1 -3.2) (end 6.1 -3.2) (layer F.SilkS) (width 0.127))
  (pad 1 connect rect (at -5.6 -1.95) (size 1.4 2) (layers F.Cu F.Mask)
    (zone_connect 2))
  (pad 2 connect rect (at 5.6 -1.95) (size 1.4 2) (layers F.Cu F.Mask)
    (zone_connect 2))
)
