(footprint "DFN-6_0.5mm_1.5x1mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "LCSC" "C507245")
  (property "MFG" "TI")
  (property "MPN" "SN74LVC1G66DRYR")
  (property "Sheetfile" "../../library/blocks/TI INA241 Shunt Amplifier.kicad_sch")
  (property "Sheetname" "In-line Shunt Amplifier")
  (property "ki_description" "Single Bilateral Analog Switch, SON")
  (property "ki_keywords" "Single Bilateral Analog Switch")
  (attr smd)
  (fp_text reference "U9" (at -1.4 0 90) (layer "F.SilkS") hide
      (effects (font (size 0.6 0.6) (thickness 0.125)))
    (tstamp 85ef388c-77c2-4dca-8912-4f79f78678fd)
  )
  (fp_text value "74LVC1G66" (at 0 -0.95 180) (layer "F.Fab")
      (effects (font (size 0.2 0.2) (thickness 0.05)))
    (tstamp e622a9c9-394a-4b1d-b752-67bc197e995b)
  )
  (fp_arc (start -0.925 -0.6) (mid -0.903033 -0.653033) (end -0.85 -0.675)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 64178941-7717-4d2c-aa66-31a66b45926f))
  (fp_arc (start -0.85 0.675) (mid -0.903033 0.653033) (end -0.925 0.6)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 3cc6e582-f2d2-480a-9095-7b14ce23fa5b))
  (fp_arc (start 0.85 -0.675) (mid 0.903033 -0.653033) (end 0.925 -0.6)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 2cad5d1a-6c62-487e-a704-46c31635e4ef))
  (fp_arc (start 0.925 0.6) (mid 0.903033 0.653033) (end 0.85 0.675)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 6f54c0ac-13c1-495c-82a9-8099aad4e34d))
  (fp_poly
    (pts
      (xy -0.5 0.725)
      (xy -0.625 0.9)
      (xy -0.375 0.9)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp f28b191d-ac6f-427b-a3b2-dd6cc381a7a0))
  (fp_poly
    (pts
      (xy -0.85 0.6)
      (xy -0.85 -0.6)
      (xy -0.75 -0.6)
      (xy -0.75 -0.75)
      (xy -0.85 -0.75)
      (xy -1 -0.6)
      (xy -1 0.6)
      (xy -0.85 0.75)
      (xy -0.75 0.75)
      (xy -0.75 0.6)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 7b8c62db-593c-4d7a-abc9-04642f6d6777))
  (fp_poly
    (pts
      (xy 0.85 -0.6)
      (xy 0.85 0.6)
      (xy 0.75 0.6)
      (xy 0.75 0.75)
      (xy 0.85 0.75)
      (xy 1 0.6)
      (xy 1 -0.6)
      (xy 0.85 -0.75)
      (xy 0.75 -0.75)
      (xy 0.75 -0.6)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 5fec8e96-10da-4fc6-b9e3-f15c01e66dbf))
  (fp_line (start -1 0.5) (end -1 -0.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0c17dec6-e4fb-4215-b629-499a13c5808f))
  (fp_line (start -0.75 -0.75) (end -0.7 -0.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 12a7c1d2-22a1-49d7-b85b-6c7c97319ae3))
  (fp_line (start -0.75 0.75) (end -0.7 0.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6ec031eb-8a7d-4af7-af7f-06fbad377a43))
  (fp_line (start -0.55 0.8) (end 0.55 0.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1e21515f-beb9-4578-9f2a-7c65ffa583a3))
  (fp_line (start 0.55 -0.8) (end -0.55 -0.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 467bc2e1-1546-4704-89e4-3803163b385a))
  (fp_line (start 0.75 -0.75) (end 0.7 -0.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp aba67a64-65a0-40e8-960c-fc8ba931a83d))
  (fp_line (start 0.75 0.75) (end 0.7 0.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5605b3d2-db5d-41c9-ac48-b16ce6a40e90))
  (fp_line (start 1 -0.5) (end 1 0.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b2cf2e62-3d2c-4e2b-b2df-c11402d5471e))
  (fp_arc (start -1 -0.5) (mid -0.926777 -0.676777) (end -0.75 -0.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4cc2f4b5-ca86-4280-9b19-13f62dcb19cf))
  (fp_arc (start -0.75 0.75) (mid -0.926777 0.676777) (end -1 0.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 40de71f8-759e-4779-a9a8-a2c646112075))
  (fp_arc (start -0.7 -0.75) (mid -0.629057 -0.787171) (end -0.55 -0.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp eafd927f-c2f6-47f4-88e7-74231e5f4292))
  (fp_arc (start -0.55 0.8) (mid -0.629057 0.787171) (end -0.7 0.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4d88ef1d-4497-4dc5-aef8-77d10fb6874b))
  (fp_arc (start 0.55 -0.8) (mid 0.629057 -0.787171) (end 0.7 -0.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5f00bd56-aad1-4bcc-acf9-c0371bb64330))
  (fp_arc (start 0.7 0.75) (mid 0.629057 0.787171) (end 0.55 0.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9d392ecb-7ee8-42af-9ad7-9c4be3dc09b7))
  (fp_arc (start 0.75 -0.75) (mid 0.926777 -0.676777) (end 1 -0.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b548f657-ad8f-4042-8ab3-a98e6796829e))
  (fp_arc (start 1 0.5) (mid 0.926777 0.676777) (end 0.75 0.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fe9dccf9-0c06-45e4-8d32-e78d265d05f4))
  (fp_line (start -0.75 -0.5) (end 0.75 -0.5)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 7ea69655-3306-44e8-b5a5-e009a2c6d343))
  (fp_line (start -0.75 0.5) (end -0.75 -0.5)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 14b8627f-8f60-46a5-8a9b-463b8750da12))
  (fp_line (start 0.75 -0.5) (end 0.75 0.5)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp dddbbc63-13c3-49d5-9453-43fc825713dd))
  (fp_line (start 0.75 0.5) (end -0.75 0.5)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp b00c0f07-7cd9-4c66-8858-80121ba4e99c))
  (pad "" smd oval (at -0.5 0.385) (size 0.25 0.45) (layers "F.Paste") (tstamp c4933459-4144-4cc5-b210-a85c60326082))
  (pad "1" smd roundrect (at -0.5 0.385) (size 0.3 0.52) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.1) (chamfer top_left top_right)
    (solder_mask_margin 0.05) (solder_paste_margin -0.025) (tstamp 92c6fce5-7cfd-400e-bbeb-e3b1d9aeaa09))
  (pad "2" smd oval (at 0 0.385) (size 0.25 0.45) (layers "F.Paste") (tstamp b45efbde-d1bf-4e80-97df-19436be3683f))
  (pad "2" smd roundrect (at 0 0.385) (size 0.3 0.52) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.1) (chamfer top_left top_right)
    (solder_mask_margin 0.05) (solder_paste_margin -0.025) (tstamp fb617024-9c5e-497f-925d-60d03570df27))
  (pad "3" smd oval (at 0.5 0.385) (size 0.25 0.45) (layers "F.Paste") (tstamp f9c50ffc-e00f-444a-92f0-8bc64bf8a9dd))
  (pad "3" smd roundrect (at 0.5 0.385) (size 0.3 0.52) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.1) (chamfer top_left top_right)
    (solder_mask_margin 0.05) (solder_paste_margin -0.025) (tstamp d3af1e0c-3f3b-4f1b-b0db-63e6d850b1eb))
  (pad "4" smd oval (at 0.5 -0.385) (size 0.25 0.45) (layers "F.Paste") (tstamp 1bcc3463-7c47-43b4-89f8-fd296ec45410))
  (pad "4" smd roundrect (at 0.5 -0.385 180) (size 0.3 0.52) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.1) (chamfer top_left top_right)
    (solder_mask_margin 0.05) (solder_paste_margin -0.025) (tstamp 08e9554d-beea-4177-9191-9e512339883d))
  (pad "5" smd oval (at 0 -0.385) (size 0.25 0.45) (layers "F.Paste") (tstamp a803947b-52a5-48fe-a305-ed00bbcf89e0))
  (pad "5" smd roundrect (at 0 -0.385 180) (size 0.3 0.52) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.1) (chamfer top_left top_right)
    (solder_mask_margin 0.05) (solder_paste_margin -0.025) (tstamp 120ec107-48fd-49ff-a6d3-a67f3efc45c6))
  (pad "6" smd oval (at -0.5 -0.385) (size 0.25 0.45) (layers "F.Paste") (tstamp 07af8df9-8367-4a6d-aa4b-bac332b2a3d2))
  (pad "6" smd roundrect (at -0.5 -0.385 180) (size 0.3 0.52) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.1) (chamfer top_left top_right)
    (solder_mask_margin 0.05) (solder_paste_margin -0.025) (tstamp 53f8bcff-de08-4484-8831-4116cdd8362b))
  (model "3D/SH/DFN-6_0.5mm_1.5x1mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 0.3937007874 0.3937007874 0.3937007874))
    (rotate (xyz 0 0 0))
  )
)
