(module MEAS_810M1 (layer F.Cu) (tedit 57543DA7)
  (fp_text reference U7 (at 0 -7.366) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value Meas_810M1 (at 0 5.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user "Epoxy feed" (at 0 -1.5) (layer B.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)) (justify mirror))
  )
  (fp_text user "DO NOT REFLOW SOLDER!" (at 0 -5.5) (layer F.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.125)))
  )
  (fp_circle (center -8.128 7.366) (end -8.128 7.493) (layer F.SilkS) (width 0.125))
  (fp_line (start 8.89 -7.62) (end 8.89 7.62) (layer F.CrtYd) (width 0.05))
  (fp_line (start 8.89 7.62) (end -8.89 7.62) (layer F.CrtYd) (width 0.05))
  (fp_line (start -8.89 7.62) (end -8.89 -7.62) (layer F.CrtYd) (width 0.05))
  (fp_line (start -8.89 -7.62) (end 8.89 -7.62) (layer F.CrtYd) (width 0.05))
  (fp_line (start -6.35 6.985) (end -8.255 6.985) (layer F.SilkS) (width 0.125))
  (fp_line (start -8.255 6.985) (end -8.255 5.08) (layer F.SilkS) (width 0.125))
  (fp_line (start 8.255 5.08) (end 8.255 6.985) (layer F.SilkS) (width 0.125))
  (fp_line (start 8.255 6.985) (end 6.35 6.985) (layer F.SilkS) (width 0.125))
  (fp_line (start 6.35 -6.985) (end 8.255 -6.985) (layer F.SilkS) (width 0.125))
  (fp_line (start 8.255 -6.985) (end 8.255 -5.08) (layer F.SilkS) (width 0.125))
  (fp_line (start -8.255 -6.985) (end -6.35 -6.985) (layer F.SilkS) (width 0.125))
  (fp_line (start -8.255 -6.985) (end -8.255 -5.08) (layer F.SilkS) (width 0.125))
  (fp_line (start -7.62 -6.35) (end 7.62 -6.35) (layer F.Fab) (width 0.05))
  (fp_line (start 7.62 -6.35) (end 7.62 6.35) (layer F.Fab) (width 0.05))
  (fp_line (start 7.62 6.35) (end -7.62 6.35) (layer F.Fab) (width 0.05))
  (fp_line (start -7.62 6.35) (end -7.62 -6.35) (layer F.Fab) (width 0.05))
  (pad 3 connect oval (at -6.35 3.81) (size 3.81 1.27) (layers F.Cu F.Mask))
  (pad 4 connect oval (at 6.731 3.81) (size 3.05 1.27) (layers F.Cu F.Mask)
    (zone_connect 1) (thermal_width 0.2) (thermal_gap 0.2))
  (pad 5 connect oval (at 6.731 -3.81) (size 3.05 1.27) (layers F.Cu F.Mask)
    (zone_connect 1) (thermal_width 0.2) (thermal_gap 0.2))
  (pad 1 connect oval (at -6.731 -3.81) (size 3.05 1.27) (layers F.Cu F.Mask))
  (pad 2 connect oval (at -6.731 -0.127) (size 3.05 1.524) (layers F.Cu F.Mask)
    (zone_connect 1) (thermal_width 0.2) (thermal_gap 0.2))
  (pad "" np_thru_hole circle (at 0 0) (size 1 1) (drill 1) (layers *.Cu *.Mask))
)
