(footprint "D_SOD-323HE_KA" (version 20220815) (generator pcbnew)
  (layer "F.Cu")
  (descr "SOD-323F http://www.nxp.com/documents/outline_drawing/SOD323F.pdf")
  (tags "SOD-323HE")
  (property "Dielectric" "")
  (property "Footprint_Density" "")
  (property "Footprint_Library" "")
  (property "JLCPCB Part" "")
  (property "LCSC" "")
  (property "MFG" "")
  (property "MPN" "")
  (property "MPN_ALT1" "")
  (property "Mouser" "")
  (property "Note" "")
  (property "Package" "")
  (property "Sheetfile" "File: AK80 Controller v1.kicad_sch")
  (property "Sheetname" "")
  (property "Spice_Model" "")
  (property "Spice_Netlist_Enabled" "")
  (property "Spice_Primitive" "")
  (property "Tolerance" "")
  (property "USD_per_1" "")
  (property "USD_per_1000" "")
  (property "Voltage" "")
  (attr smd)
  (fp_text reference "D1" (at 0 -1.35) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 3d2080e1-8159-4140-98f2-373f3cd81f35)
  )
  (fp_text value "80V" (at 0 1.1) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp 66d26795-c0f6-4250-a5b4-f167fa7516bc)
  )
  (fp_text user "${REFERENCE}" (at 0 -1.85) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ef1eca2b-b1df-4ef6-b0fd-7a28c56a84d8)
  )
  (fp_rect (start -1.95 -0.35) (end -1.8 0.35)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp ffd74b47-85e9-4146-919f-af8792ff3cf6))
  (fp_rect (start -1.45 -0.85) (end 0.9 -0.7)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp d5a14ce0-fcb0-4349-9f0d-bc3163f2f3b5))
  (fp_rect (start -1.45 0.7) (end 0.9 0.85)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp cf9b752e-c682-4fa2-9a02-90bf8fd59147))
  (fp_arc (start -1.875 -0.35) (mid -1.75052 -0.65052) (end -1.45 -0.775)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp f4690d73-b415-4ab5-85ce-9582e5667092))
  (fp_arc (start -1.45 0.775) (mid -1.75052 0.65052) (end -1.875 0.35)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 54cb6ece-4e43-4675-893a-f101d28ef1d0))
  (fp_line (start -1.8 -0.35) (end -1.8 0.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 985d0f71-5ad7-4f31-ba21-d429fb2d57a4))
  (fp_line (start -1.45 -0.7) (end -1.15 -0.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 58c9a97a-0f50-44fa-b700-2b185638966c))
  (fp_line (start -1.45 0.7) (end -1.15 0.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e776c3c6-ee7e-405b-acfe-452b3f8b1c3c))
  (fp_line (start -0.9 0.95) (end 0.9 0.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9f7ddff7-94fc-4ab3-a46e-bda0daa91bac))
  (fp_line (start 0.9 -0.95) (end -0.9 -0.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 87610d8d-5dc0-4c69-8f57-e86ec79b089c))
  (fp_line (start 1.45 -0.7) (end 1.15 -0.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9fef9efa-a03a-468e-b6c8-d3f00174297d))
  (fp_line (start 1.45 0.7) (end 1.15 0.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c7229d18-45c8-4746-bb07-11ae462a8016))
  (fp_line (start 1.8 0.35) (end 1.8 -0.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 38bac979-addf-4a26-b4a9-8ea928121f35))
  (fp_arc (start -1.8 -0.35) (mid -1.697487 -0.597487) (end -1.45 -0.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4f2c6388-715a-4eed-bca0-b26400342d29))
  (fp_arc (start -1.45 0.7) (mid -1.697487 0.597487) (end -1.8 0.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 585625de-1989-4f0a-944d-171e13386b73))
  (fp_arc (start -1.15 -0.7) (mid -1.076777 -0.876777) (end -0.9 -0.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e11b8ab7-6761-428d-b18a-00b00b9e78a9))
  (fp_arc (start -0.9 0.95) (mid -1.076777 0.876777) (end -1.15 0.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d6c22c3a-8dac-41a9-be91-abaa761d6b19))
  (fp_arc (start 0.9 -0.95) (mid 1.076777 -0.876777) (end 1.15 -0.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b7242a36-b69e-4b4b-ad45-cd4abd24ea86))
  (fp_arc (start 1.15 0.7) (mid 1.076777 0.876777) (end 0.9 0.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4d633f8b-a237-4e3b-ad1f-75b1ee84bc43))
  (fp_arc (start 1.45 -0.7) (mid 1.697487 -0.597487) (end 1.8 -0.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3973a2ae-74f8-4bd5-9123-93e07c5b50ac))
  (fp_arc (start 1.8 0.35) (mid 1.697487 0.597487) (end 1.45 0.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d0e81b85-5023-4124-9f80-723064167701))
  (fp_line (start -0.9 -0.7) (end 0.9 -0.7)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cada950e-f109-4b19-88c2-e3c75d4da9c9))
  (fp_line (start -0.9 0.7) (end -0.9 -0.7)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 889042d6-691c-4c8c-ba02-89f1aa85ac49))
  (fp_line (start -0.3 -0.35) (end -0.3 0.35)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 483b3797-716f-4a5d-9874-f5bb54ab1bb7))
  (fp_line (start -0.3 0) (end -0.5 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 18356008-f605-49c7-83a6-6312fc95d255))
  (fp_line (start -0.3 0) (end 0.2 -0.35)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 43f025aa-fc86-43f1-bc3b-e31e97f22ee1))
  (fp_line (start 0.2 -0.35) (end 0.2 0.35)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d27f85a7-2519-4fa8-b127-bf6955d5530a))
  (fp_line (start 0.2 0) (end 0.45 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ae6c0c45-7fd5-4925-8340-762e62a479b6))
  (fp_line (start 0.2 0.35) (end -0.3 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 58ff8de3-5681-4aa9-ba0b-ba065ca4aee1))
  (fp_line (start 0.9 -0.7) (end 0.9 0.7)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5e0f7081-4a59-40f3-bbd2-a9f511c7c9e0))
  (fp_line (start 0.9 0.7) (end -0.9 0.7)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5ee89735-0fa1-46e9-8bd0-82c51ca8925e))
  (pad "A" smd roundrect (at 1.25 0) (size 0.8 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 3d6512db-199e-4e15-86cb-ec934bd2fcc3))
  (pad "K" smd roundrect (at -0.65 0) (size 2 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1818181818) (tstamp dfe47bb3-628f-4c24-80c4-79559c33cc98))
  (model "${KICAD7_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323F.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
