(footprint "SMD Nut M2 x 1.5 SMTSO2015" (version 20221018) (generator pcbnew)
  locked (layer "F.Cu")
  (property "LCSC" "C2916320")
  (property "MFG" "Sinhoo")
  (property "MPN" "SMTSO2015CTJ")
  (property "Sheetfile" "QuadCameraCarrier.kicad_sch")
  (property "Sheetname" "")
  (property "exclude_from_bom" "")
  (attr smd exclude_from_bom)
  (fp_text reference "H2" (at 0 -7.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp afd3a7d4-886b-449f-a07b-e785844ac7f6)
  )
  (fp_text value "MOUNT_HOLE" (at 0 -6 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b41e0e7a-fc35-4f12-812e-87519c880037)
  )
  (fp_text user "${REFERENCE}" (at 0 -4.5 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b297350a-1e26-449c-b906-67c325783f03)
  )
  (fp_arc (start -2.533845 0.788749) (mid -2.65374 -0.012456) (end -2.526329 -0.8125)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp 7b6c4a43-dcae-43a2-b147-e31274065e4f))
  (fp_arc (start -1.95 -1.8) (mid -1.316084 -2.304435) (end -0.559519 -2.594115)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp c54ce6cb-56d6-4e8a-a706-57e21fddb111))
  (fp_arc (start -0.583845 2.588749) (mid -1.337657 2.291979) (end -1.96681 1.781615)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp 2cef1f36-5fa7-412b-a68b-751f422d5e19))
  (fp_arc (start 0.583845 -2.588749) (mid 1.337657 -2.291979) (end 1.96681 -1.781615)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp 62931b21-f626-4b0d-a7d2-e23974762e28))
  (fp_arc (start 1.95 1.8) (mid 1.316084 2.304435) (end 0.559519 2.594115)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp c322ac42-14a3-420b-b91e-9e8851605185))
  (fp_arc (start 2.533845 -0.788749) (mid 2.65374 0.012456) (end 2.526329 0.8125)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp 16f5630c-7378-4757-be9c-56c43d0a3c35))
  (fp_circle (center 0 0) (end 2.15 0)
    (stroke (width 0.05) (type default)) (fill none) (layer "B.CrtYd") (tstamp 97530ef3-fdc5-415e-9336-bd8bff70866e))
  (fp_circle (center 0 0) (end 3.25 0)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 51ce6094-c25e-4dde-92b8-f836aa137642))
  (pad "1" thru_hole circle locked (at 0 0) (size 4.03 4.03) (drill 3.73) (layers "*.Cu" "B.Mask")
    (zone_connect 2) (tstamp 3b29eab4-ece3-4502-b1dc-f5aa23afec1c))
  (pad "1" smd circle locked (at 0 0) (size 6.2 6.2) (layers "F.Cu" "F.Mask")
    (zone_connect 2) (tstamp d0d5afb7-1e51-4ca4-8dc5-0ee8fd4da2fe))
  (model ":KICAD7_3DMODEL_DIR:Hardware.3dshapes/Nut [SMTSO] [M2 x 1.5].step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
