(footprint "2P_1.5x1_P1.25" (version 20201116) (generator pcbnew) (layer "F.Cu")
  (tedit 5FE715D4)
  (fp_text reference "REF**" (at 0 -1.675 unlocked) (layer "F.SilkS")
    (effects (font (size 0.6 0.6) (thickness 0.15)))
    (tstamp 860f7b7c-6cca-492a-bde3-535abe0d65c8)
  )
  (fp_text value "2P_1.5x1_P1.25" (at 0 0.2 unlocked) (layer "F.Fab")
    (effects (font (size 0.1 0.1) (thickness 0.025)))
    (tstamp cfdfeed9-b6c3-46e0-8eef-aff480b7b591)
  )
  (fp_text user "${REF}" (at 0 -0.225 unlocked) (layer "F.Fab")
    (effects (font (size 0.1 0.1) (thickness 0.025)))
    (tstamp 91170ebc-e622-4895-940d-7a1cc58ff1bc)
  )
  (pad "1" connect roundrect (at 0 -0.625) (size 1.5 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1) (tstamp 56271e0b-8ae5-4800-a250-c049cefc12a1))
  (pad "2" connect roundrect (at 0 0.625) (size 1.5 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1) (tstamp 37f5a987-65a2-480b-8031-bf1685d11195))
)
