(module CONN_Hirose_DF50-40DP-1H (layer F.Cu) (tedit 53D41943)
  (attr smd)
  (fp_text reference P3 (at -5 0) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SCROBBY_HARNESS (at 0 4.75) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_line (start -12.5 3) (end -12.5 -6) (layer F.SilkS) (width 0.15))
  (fp_line (start -12.5 -6) (end 12.5 -6) (layer F.SilkS) (width 0.15))
  (fp_line (start 12.5 -6) (end 12.5 3) (layer F.SilkS) (width 0.15))
  (fp_line (start 12.5 3) (end -12.5 3) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -9.5 2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -9.5 -2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -8.5 2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -8.5 -2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -7.5 2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -7.5 -2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -6.5 2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -6.5 -2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -5.5 2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -5.5 -2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -4.5 2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at -4.5 -2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at -3.5 2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at -3.5 -2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at -2.5 2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at -2.5 -2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at -1.5 2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at -1.5 -2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at -0.5 2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at -0.5 -2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at 0.5 2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd rect (at 0.5 -2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd rect (at 1.5 2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd rect (at 1.5 -2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 25 smd rect (at 2.5 2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 26 smd rect (at 2.5 -2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 27 smd rect (at 3.5 2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 28 smd rect (at 3.5 -2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 29 smd rect (at 4.5 2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 30 smd rect (at 4.5 -2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 31 smd rect (at 5.5 2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 32 smd rect (at 5.5 -2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 33 smd rect (at 6.5 2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 34 smd rect (at 6.5 -2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 35 smd rect (at 7.5 2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 36 smd rect (at 7.5 -2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 37 smd rect (at 8.5 2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 38 smd rect (at 8.5 -2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 39 smd rect (at 9.5 2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 40 smd rect (at 9.5 -2.85) (size 0.6 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 41 smd rect (at -11.625 -1.75) (size 1.75 1.8) (layers F.Cu F.Paste F.Mask)
    (zone_connect 2))
  (pad 41 smd rect (at 11.625 -1.75) (size 1.75 1.8) (layers F.Cu F.Paste F.Mask)
    (zone_connect 2))
)
