(footprint "6432_KC_C" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "LCSC" "C481523")
  (property "MFG" "Milliohm")
  (property "MPN" "LRS2512-3WR0003F")
  (property "Sheetfile" "../../library/blocks/TI INA241 Shunt Amplifier.kicad_sch")
  (property "Sheetname" "In-line Shunt Amplifier")
  (property "ki_description" "Shunt resistor, US symbol")
  (property "ki_keywords" "R res shunt resistor")
  (attr smd)
  (fp_text reference "R32" (at -2.7 -2.3) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp f1de42be-46ac-4d08-a963-323c8a0f7b18)
  )
  (fp_text value "R_Shunt" (at 0 -1.1) (layer "F.Fab")
      (effects (font (size 0.6 0.6) (thickness 0.15)))
    (tstamp 615103c4-cf6b-4a42-bedc-4addea6eb705)
  )
  (fp_rect (start -1.25 -1.85) (end 1.25 -1.7)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 8eaaaac3-b2da-4f15-bca0-a92867d60859))
  (fp_rect (start -1.25 1.7) (end 1.25 1.85)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 4ad7eb35-9eb9-4038-ba15-580e73904277))
  (fp_line (start -3.45 -1.6) (end -3.45 1.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c641470c-406b-4aaf-ac6d-cb64c9058f6f))
  (fp_line (start -3.2 -1.85) (end 3.2 -1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 17353777-350d-4253-ad82-b4856a254039))
  (fp_line (start -3.2 1.85) (end 3.2 1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 63a8ad0f-3ee3-4bac-89e0-9d71b5abd983))
  (fp_line (start 3.45 1.6) (end 3.45 -1.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp adb4c623-479d-4e45-a38e-efaf2382f0d6))
  (fp_arc (start -3.45 -1.6) (mid -3.376777 -1.776777) (end -3.2 -1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 04b5c24d-21ba-46b1-8ffc-6a1adff1fca6))
  (fp_arc (start -3.2 1.85) (mid -3.376777 1.776777) (end -3.45 1.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 63af0035-f163-458a-bbe2-5ce9dae7c4be))
  (fp_arc (start 3.2 -1.85) (mid 3.376777 -1.776777) (end 3.45 -1.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6ed06136-a1a4-48af-b789-dd6102fecbde))
  (fp_arc (start 3.45 1.6) (mid 3.376777 1.776777) (end 3.2 1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 67afac33-dbe5-4fff-b35d-34bd9633b511))
  (fp_line (start -3.2 -1.6) (end 3.2 -1.6)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp baca97e7-5dc9-49de-8dea-8abe3f69d155))
  (fp_line (start -3.2 1.6) (end -3.2 -1.6)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp cb4f41ba-8179-4c6d-a424-5af529ca83cd))
  (fp_line (start 3.2 -1.6) (end 3.2 1.6)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp b3175f69-c41d-44c4-85a3-c27de40d0da8))
  (fp_line (start 3.2 1.6) (end -3.2 1.6)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 491dd092-5f24-4234-a744-d23eb8157d69))
  (pad "" smd roundrect (at -2.875 -1.2) (size 0.85 1) (layers "F.Paste") (roundrect_rratio 0.1176470588) (tstamp 1382a966-e0ea-413c-a1d3-67c239897c88))
  (pad "" smd roundrect (at -2.875 0) (size 0.85 1) (layers "F.Paste") (roundrect_rratio 0.1176470588) (tstamp 43ec3235-27e5-45ee-b82c-4800c2844f3d))
  (pad "" smd roundrect (at -2.875 1.2) (size 0.85 1) (layers "F.Paste") (roundrect_rratio 0.1176470588) (tstamp a1bb61c9-4abe-4bda-b763-cee269cd9487))
  (pad "" smd roundrect (at -1.825 -1.2) (size 0.85 1) (layers "F.Paste") (roundrect_rratio 0.1176470588) (tstamp d3548140-d0cf-4208-9bef-528a82a0bdc7))
  (pad "" smd roundrect (at -1.825 0) (size 0.85 1) (layers "F.Paste") (roundrect_rratio 0.1176470588) (tstamp c7fc74d7-28e9-4ec6-b28f-da9458367c56))
  (pad "" smd roundrect (at -1.825 1.2) (size 0.85 1) (layers "F.Paste") (roundrect_rratio 0.1176470588) (tstamp bf9a382a-fb63-43e0-ab37-3fbba49e4ced))
  (pad "" smd roundrect (at 1.825 -1.2) (size 0.85 1) (layers "F.Paste") (roundrect_rratio 0.1176470588) (tstamp 829d6018-9676-4c90-85e9-85ee34f66f51))
  (pad "" smd roundrect (at 1.825 0) (size 0.85 1) (layers "F.Paste") (roundrect_rratio 0.1176470588) (tstamp a7b8221f-46cf-4fcf-982f-3842a5abe725))
  (pad "" smd roundrect (at 1.825 1.2) (size 0.85 1) (layers "F.Paste") (roundrect_rratio 0.1176470588) (tstamp d785deea-bd67-447a-b46d-0337a781c054))
  (pad "" smd roundrect (at 2.875 -1.2) (size 0.85 1) (layers "F.Paste") (roundrect_rratio 0.1176470588) (tstamp be067e9b-db93-4ec9-a510-faf6dac50c55))
  (pad "" smd roundrect (at 2.875 0) (size 0.85 1) (layers "F.Paste") (roundrect_rratio 0.1176470588) (tstamp 91cef2e3-94e5-4ebf-8c40-19226ae84f4a))
  (pad "" smd roundrect (at 2.875 1.2) (size 0.85 1) (layers "F.Paste") (roundrect_rratio 0.1176470588) (tstamp ea886dc1-a785-4528-83b5-4f5dd220c039))
  (pad "1" smd roundrect (at -2.35 0) (size 1.9 3.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.05263157895) (tstamp 7825fff3-10fc-4a87-9479-ed527eeeeeb7))
  (pad "2" smd oval (at -0.35 0) (size 2.2 0.2) (drill (offset -1 0)) (layers "F.Cu") (tstamp 34735957-c9b4-4fc3-9753-d5876f44c880))
  (pad "3" smd oval (at 0.35 0 180) (size 2.2 0.2) (drill (offset -1 0)) (layers "F.Cu") (tstamp 41234707-92e3-44e7-bad2-112b7db506d6))
  (pad "4" smd roundrect (at 2.35 0) (size 1.9 3.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.05263157895) (tstamp 58dba25a-1ba1-43a2-902a-a39aeca13a56))
  (model "Resistor_SMD.3dshapes/Resistor_SMD_6432.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
